; Windows USB CDC Driver Setup File for GCR readers family
; Copyright (c) 2009 Gemalto

[Version]
Signature="$Windows NT$"
Class=Ports
ClassGuid={4D36E978-E325-11CE-BFC1-08002BE10318}
Provider=%MFGNAME%
LayoutFile=layout.inf
DriverVer=11/23/2009,1.2.0.0
CatalogFile=gcr.cat

[Manufacturer]
%MFGNAME%=VirComDevice,NT,NTamd64

[DestinationDirs]
DefaultDestDir = 12

[SourceDisksFiles]
;Not Used, only for chkinf test.

[SourceDisksNames]
1=%INSTDISK%,,

[VirComDevice]
%USB\VID_08E6&PID_4010% = DriverInstall, USB\VID_08E6&PID_4010
%USB\VID_08E6&PID_4011% = DriverInstall, USB\VID_08E6&PID_4011
%USB\VID_08E6&PID_4012% = DriverInstall, USB\VID_08E6&PID_4012
%USB\VID_08E6&PID_4013% = DriverInstall, USB\VID_08E6&PID_4013
%USB\VID_08E6&PID_4014% = DriverInstall, USB\VID_08E6&PID_4014
%USB\VID_08E6&PID_4015% = DriverInstall, USB\VID_08E6&PID_4015
%USB\VID_08E6&PID_4016% = DriverInstall, USB\VID_08E6&PID_4016
%USB\VID_08E6&PID_4017% = DriverInstall, USB\VID_08E6&PID_4017
%USB\VID_08E6&PID_4018% = DriverInstall, USB\VID_08E6&PID_4018
%USB\VID_08E6&PID_4019% = DriverInstall, USB\VID_08E6&PID_4019
%USB\VID_08E6&PID_401A% = DriverInstall, USB\VID_08E6&PID_401A
%USB\VID_08E6&PID_401B% = DriverInstall, USB\VID_08E6&PID_401B
%USB\VID_08E6&PID_401C% = DriverInstall, USB\VID_08E6&PID_401C
%USB\VID_08E6&PID_401D% = DriverInstall, USB\VID_08E6&PID_401D
%USB\VID_08E6&PID_401E% = DriverInstall, USB\VID_08E6&PID_401E
%USB\VID_08E6&PID_401F% = DriverInstall, USB\VID_08E6&PID_401F

[VirComDevice.NT]
%USB\VID_08E6&PID_4010% = DriverInstall, USB\VID_08E6&PID_4010
%USB\VID_08E6&PID_4011% = DriverInstall, USB\VID_08E6&PID_4011
%USB\VID_08E6&PID_4012% = DriverInstall, USB\VID_08E6&PID_4012
%USB\VID_08E6&PID_4013% = DriverInstall, USB\VID_08E6&PID_4013
%USB\VID_08E6&PID_4014% = DriverInstall, USB\VID_08E6&PID_4014
%USB\VID_08E6&PID_4015% = DriverInstall, USB\VID_08E6&PID_4015
%USB\VID_08E6&PID_4016% = DriverInstall, USB\VID_08E6&PID_4016
%USB\VID_08E6&PID_4017% = DriverInstall, USB\VID_08E6&PID_4017
%USB\VID_08E6&PID_4018% = DriverInstall, USB\VID_08E6&PID_4018
%USB\VID_08E6&PID_4019% = DriverInstall, USB\VID_08E6&PID_4019
%USB\VID_08E6&PID_401A% = DriverInstall, USB\VID_08E6&PID_401A
%USB\VID_08E6&PID_401B% = DriverInstall, USB\VID_08E6&PID_401B
%USB\VID_08E6&PID_401C% = DriverInstall, USB\VID_08E6&PID_401C
%USB\VID_08E6&PID_401D% = DriverInstall, USB\VID_08E6&PID_401D
%USB\VID_08E6&PID_401E% = DriverInstall, USB\VID_08E6&PID_401E
%USB\VID_08E6&PID_401F% = DriverInstall, USB\VID_08E6&PID_401F

[VirComDevice.NTamd64]
%USB\VID_08E6&PID_4010% = DriverInstall, USB\VID_08E6&PID_4010
%USB\VID_08E6&PID_4011% = DriverInstall, USB\VID_08E6&PID_4011
%USB\VID_08E6&PID_4012% = DriverInstall, USB\VID_08E6&PID_4012
%USB\VID_08E6&PID_4013% = DriverInstall, USB\VID_08E6&PID_4013
%USB\VID_08E6&PID_4014% = DriverInstall, USB\VID_08E6&PID_4014
%USB\VID_08E6&PID_4015% = DriverInstall, USB\VID_08E6&PID_4015
%USB\VID_08E6&PID_4016% = DriverInstall, USB\VID_08E6&PID_4016
%USB\VID_08E6&PID_4017% = DriverInstall, USB\VID_08E6&PID_4017
%USB\VID_08E6&PID_4018% = DriverInstall, USB\VID_08E6&PID_4018
%USB\VID_08E6&PID_4019% = DriverInstall, USB\VID_08E6&PID_4019
%USB\VID_08E6&PID_401A% = DriverInstall, USB\VID_08E6&PID_401A
%USB\VID_08E6&PID_401B% = DriverInstall, USB\VID_08E6&PID_401B
%USB\VID_08E6&PID_401C% = DriverInstall, USB\VID_08E6&PID_401C
%USB\VID_08E6&PID_401D% = DriverInstall, USB\VID_08E6&PID_401D
%USB\VID_08E6&PID_401E% = DriverInstall, USB\VID_08E6&PID_401E
%USB\VID_08E6&PID_401F% = DriverInstall, USB\VID_08E6&PID_401F

[DriverInstall.NT]
Include=mdmcpq.inf
CopyFiles=FakeModemCopyFileSection
AddReg=DriverInstall.AddReg

[DriverInstall.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,usbser.sys
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"

[DriverInstall.NT.Services]
AddService=usbser, 0x00000002, DriverServiceInst

[DriverServiceInst]
DisplayName=%SERVICE%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\usbser.sys

[Strings]
MFGNAME              = "Gemalto"
USB\VID_08E6&PID_4010="Sealys Vitale"
USB\VID_08E6&PID_4011="Sealys Santé v1"
USB\VID_08E6&PID_4012="Sealys Santé v2"
USB\VID_08E6&PID_4013="Sealys Santé v3"
USB\VID_08E6&PID_4014="Sealys Santé v4"
USB\VID_08E6&PID_4015="Sealys Santé v5"
USB\VID_08E6&PID_4016="Sealys Santé v6"
USB\VID_08E6&PID_4017="Sealys Santé v7"
USB\VID_08E6&PID_4018="Sealys Santé v8"
USB\VID_08E6&PID_4019="Sealys Santé v9"
USB\VID_08E6&PID_401A="Sealys Santé v10"
USB\VID_08E6&PID_401B="Sealys Santé v11"
USB\VID_08E6&PID_401C="Sealys Santé v12"
USB\VID_08E6&PID_401D="Sealys Santé v13"
USB\VID_08E6&PID_401E="Sealys Santé v14"
USB\VID_08E6&PID_401F="Sealys Santé v15"
SERVICE              = "USB RS-232 Emulation Driver"
INSTDISK             ="Installation Disc for Sealys reader"
