;******************************************************************************
;**                                                                          **
;**  Copyright 2009-2025 Intel Corporation. All Rights Reserved.             **
;**                                                                          **
;**  The material contained or described herein and all documents related    **
;**  to such material ("Material") is owned by Intel Corporation or its      **
;**  suppliers or licensors, and title to such Material remains with Intel   **
;**  Corporation or its suppliers or licensors. The Material contains        **
;**  proprietary information of Intel or its suppliers and licensors. The    **
;**  Material is protected by worldwide copyright laws and treaty            **
;**  provisions. No part of the Material may be used, copied, reproduced,    **
;**  modified, published, uploaded, posted, transmitted, distributed or      **
;**  disclosed in any way without Intel's prior express written permission.  **
;**  No license under any patent, copyright or other intellectual property   **
;**  rights in the Material is granted to or conferred upon you, either      **
;**  expressly, by implication, inducement, estoppel or otherwise. Any       **
;**  license under such intellectual property rights must be express and     **
;**  approved by Intel in writing.                                           **
;**                                                                          **
;**  Unless otherwise agreed by Intel in writing, you may not remove or      **
;**  alter this notice or any other notice embedded in Materials by Intel    **
;**  or Intel's suppliers or licensors in any way.                           **
;******************************************************************************
;
;******************************************************************************

; e1d.INF (Windows 10/11 / Server 2019/2022 64 bit)

;
; Intel(R) Gigabit Network connections
;******************************************************************************
;

[Version]
Signature   = "$Windows NT$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %Intel%
CatalogFile = e1d.cat
PnpLockdown = 1
DriverVer = 11/16/2025,12.19.2.66

[Manufacturer]
%Intel%     = Intel, NTamd64.10.0...17763, NTamd64.10.0.1..17763,  NTamd64.10.0...18362, NTamd64.10.0.1..18362

[ControlFlags]
ExcludeFromSelect = \ 
    PCI\VEN_8086&DEV_153A,\ 
    PCI\VEN_8086&DEV_153B

[Intel.NTamd64.10.0.1..17763]
; DisplayName                   Section                          DeviceID
; -----------                   -------                          --------
%E153ANC.DeviceDesc%            = I217.10.0.1,          PCI\VEN_8086&DEV_153A
%E153ANC.DeviceDesc%            = I217.10.0.1,          PCI\VEN_8086&DEV_153A&SUBSYS_00008086
%E153BNC.DeviceDesc%            = I217.10.0.1,          PCI\VEN_8086&DEV_153B
%E153BNC.DeviceDesc%            = I217.10.0.1,          PCI\VEN_8086&DEV_153B&SUBSYS_00008086
%E155ANC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_155A
%E155ANC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_155A&SUBSYS_00008086
%E1559NC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_1559
%E1559NC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_1559&SUBSYS_00008086
%E15A0NC.DeviceDesc%            = I217.10.0.1,          PCI\VEN_8086&DEV_15A0
%E15A0NC.DeviceDesc%            = I217.10.0.1,          PCI\VEN_8086&DEV_15A0&SUBSYS_00008086
%E15A1NC.DeviceDesc%            = I217.10.0.1,          PCI\VEN_8086&DEV_15A1
%E15A1NC.DeviceDesc%            = I217.10.0.1,          PCI\VEN_8086&DEV_15A1&SUBSYS_00008086
%E15A2NC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_15A2
%E15A2NC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_15A2&SUBSYS_00008086
%E15A3NC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_15A3
%E15A3NC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_15A3&SUBSYS_00008086
%E156FNC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_156F
%E156FNC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_156F&SUBSYS_00008086
%E1570NC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_1570
%E1570NC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_1570&SUBSYS_00008086
%E15B7NC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_15B7
%E15B7NC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_15B7&SUBSYS_00008086
%E15B8NC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_15B8
%E15B8NC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_15B8&SUBSYS_00008086
%E15B9NC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_15B9
%E15B9NC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_15B9&SUBSYS_00008086
%E15D7NC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_15D7
%E15D7NC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_15D7&SUBSYS_00008086
%E15D8NC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_15D8
%E15D8NC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_15D8&SUBSYS_00008086
%E15E3NC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_15E3
%E15E3NC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_15E3&SUBSYS_00008086
%E15D6NC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_15D6
%E15D6NC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_15D6&SUBSYS_00008086
%E15BBNC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_15BB
%E15BBNC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_15BB&SUBSYS_00008086
%E15BCNC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_15BC
%E15BCNC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_15BC&SUBSYS_00008086
%E15BDNC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_15BD
%E15BDNC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_15BD&SUBSYS_00008086
%E15BENC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_15BE
%E15BENC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_15BE&SUBSYS_00008086
%E15DFNC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_15DF
%E15DFNC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_15DF&SUBSYS_00008086
%E15E0NC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_15E0
%E15E0NC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_15E0&SUBSYS_00008086
%E15E1NC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_15E1
%E15E1NC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_15E1&SUBSYS_00008086
%E15E2NC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_15E2
%E15E2NC.DeviceDesc%            = I219.10.0.1,          PCI\VEN_8086&DEV_15E2&SUBSYS_00008086
%E0D4ENC.DeviceDesc%            = I219_MS.10.0.1,       PCI\VEN_8086&DEV_0D4E
%E0D4ENC.DeviceDesc%            = I219_MS.10.0.1,       PCI\VEN_8086&DEV_0D4E&SUBSYS_00008086
%E0D4FNC.DeviceDesc%            = I219_MS.10.0.1,       PCI\VEN_8086&DEV_0D4F
%E0D4FNC.DeviceDesc%            = I219_MS.10.0.1,       PCI\VEN_8086&DEV_0D4F&SUBSYS_00008086
%E0D4CNC.DeviceDesc%            = I219_MS.10.0.1,       PCI\VEN_8086&DEV_0D4C
%E0D4CNC.DeviceDesc%            = I219_MS.10.0.1,       PCI\VEN_8086&DEV_0D4C&SUBSYS_00008086
%E0D4DNC.DeviceDesc%            = I219_MS.10.0.1,       PCI\VEN_8086&DEV_0D4D
%E0D4DNC.DeviceDesc%            = I219_MS.10.0.1,       PCI\VEN_8086&DEV_0D4D&SUBSYS_00008086
%E0D53NC.DeviceDesc%            = I219_MS.10.0.1,       PCI\VEN_8086&DEV_0D53
%E0D53NC.DeviceDesc%            = I219_MS.10.0.1,       PCI\VEN_8086&DEV_0D53&SUBSYS_00008086
%E0D55NC.DeviceDesc%            = I219_MS.10.0.1,       PCI\VEN_8086&DEV_0D55
%E0D55NC.DeviceDesc%            = I219_MS.10.0.1,       PCI\VEN_8086&DEV_0D55&SUBSYS_00008086
%E15F9NC.DeviceDesc%            = I219_SS.10.0.1,       PCI\VEN_8086&DEV_15F9
%E15F9NC.DeviceDesc%            = I219_SS.10.0.1,       PCI\VEN_8086&DEV_15F9&SUBSYS_00008086
%E15FANC.DeviceDesc%            = I219_SS.10.0.1,       PCI\VEN_8086&DEV_15FA
%E15FANC.DeviceDesc%            = I219_SS.10.0.1,       PCI\VEN_8086&DEV_15FA&SUBSYS_00008086
%E15FBNC.DeviceDesc%            = I219_SS.10.0.1,       PCI\VEN_8086&DEV_15FB
%E15FBNC.DeviceDesc%            = I219_SS.10.0.1,       PCI\VEN_8086&DEV_15FB&SUBSYS_00008086
%E15FCNC.DeviceDesc%            = I219_SS.10.0.1,       PCI\VEN_8086&DEV_15FC
%E15FCNC.DeviceDesc%            = I219_SS.10.0.1,       PCI\VEN_8086&DEV_15FC&SUBSYS_00008086
%E15F4NC.DeviceDesc%            = I219_SS.10.0.1,       PCI\VEN_8086&DEV_15F4
%E15F4NC.DeviceDesc%            = I219_SS.10.0.1,       PCI\VEN_8086&DEV_15F4&SUBSYS_00008086
%E1A1ENC.DeviceDesc%            = I219_SS.10.0.1,       PCI\VEN_8086&DEV_1A1E
%E1A1ENC.DeviceDesc%            = I219_SS.10.0.1,       PCI\VEN_8086&DEV_1A1E&SUBSYS_00008086
%E1A1FNC.DeviceDesc%            = I219_SS.10.0.1,       PCI\VEN_8086&DEV_1A1F
%E1A1FNC.DeviceDesc%            = I219_SS.10.0.1,       PCI\VEN_8086&DEV_1A1F&SUBSYS_00008086
%E1A1CNC.DeviceDesc%            = I219_SS.10.0.1,       PCI\VEN_8086&DEV_1A1C
%E1A1CNC.DeviceDesc%            = I219_SS.10.0.1,       PCI\VEN_8086&DEV_1A1C&SUBSYS_00008086
%E1A1DNC.DeviceDesc%            = I219_SS.10.0.1,       PCI\VEN_8086&DEV_1A1D
%E1A1DNC.DeviceDesc%            = I219_SS.10.0.1,       PCI\VEN_8086&DEV_1A1D&SUBSYS_00008086
%E550ANC.DeviceDesc%            = I219_SS_NOK1.10.0.1,  PCI\VEN_8086&DEV_550A
%E550ANC.DeviceDesc%            = I219_SS_NOK1.10.0.1,  PCI\VEN_8086&DEV_550A&SUBSYS_00008086
%E550BNC.DeviceDesc%            = I219_SS_NOK1.10.0.1,  PCI\VEN_8086&DEV_550B
%E550BNC.DeviceDesc%            = I219_SS_NOK1.10.0.1,  PCI\VEN_8086&DEV_550B&SUBSYS_00008086
%E550CNC.DeviceDesc%            = I219_SS.10.0.1,       PCI\VEN_8086&DEV_550C
%E550CNC.DeviceDesc%            = I219_SS.10.0.1,       PCI\VEN_8086&DEV_550C&SUBSYS_00008086
%E550DNC.DeviceDesc%            = I219_SS.10.0.1,       PCI\VEN_8086&DEV_550D
%E550DNC.DeviceDesc%            = I219_SS.10.0.1,       PCI\VEN_8086&DEV_550D&SUBSYS_00008086
%E0DC5NC.DeviceDesc%            = I219_SS.10.0.1,       PCI\VEN_8086&DEV_0DC5
%E0DC5NC.DeviceDesc%            = I219_SS.10.0.1,       PCI\VEN_8086&DEV_0DC5&SUBSYS_00008086
%E0DC6NC.DeviceDesc%            = I219_SS.10.0.1,       PCI\VEN_8086&DEV_0DC6
%E0DC6NC.DeviceDesc%            = I219_SS.10.0.1,       PCI\VEN_8086&DEV_0DC6&SUBSYS_00008086
%E0DC7NC.DeviceDesc%            = I219_SS.10.0.1,       PCI\VEN_8086&DEV_0DC7
%E0DC7NC.DeviceDesc%            = I219_SS.10.0.1,       PCI\VEN_8086&DEV_0DC7&SUBSYS_00008086
%E0DC8NC.DeviceDesc%            = I219_SS.10.0.1,       PCI\VEN_8086&DEV_0DC8
%E0DC8NC.DeviceDesc%            = I219_SS.10.0.1,       PCI\VEN_8086&DEV_0DC8&SUBSYS_00008086
%E57A0NC.DeviceDesc%            = I219_SS_NOK1.10.0.1,  PCI\VEN_8086&DEV_57A0
%E57A0NC.DeviceDesc%            = I219_SS_NOK1.10.0.1,  PCI\VEN_8086&DEV_57A0&SUBSYS_00008086
%E57A1NC.DeviceDesc%            = I219_SS_NOK1.10.0.1,  PCI\VEN_8086&DEV_57A1
%E57A1NC.DeviceDesc%            = I219_SS_NOK1.10.0.1,  PCI\VEN_8086&DEV_57A1&SUBSYS_00008086
%E550ENC.DeviceDesc%            = I219_SS_NOK1.10.0.1,  PCI\VEN_8086&DEV_550E
%E550ENC.DeviceDesc%            = I219_SS_NOK1.10.0.1,  PCI\VEN_8086&DEV_550E&SUBSYS_00008086
%E550FNC.DeviceDesc%            = I219_SS_NOK1.10.0.1,  PCI\VEN_8086&DEV_550F
%E550FNC.DeviceDesc%            = I219_SS_NOK1.10.0.1,  PCI\VEN_8086&DEV_550F&SUBSYS_00008086
%E57B3NC.DeviceDesc%            = I219_SS_NOK1.10.0.1,  PCI\VEN_8086&DEV_57B3
%E57B3NC.DeviceDesc%            = I219_SS_NOK1.10.0.1,  PCI\VEN_8086&DEV_57B3&SUBSYS_00008086
%E57B4NC.DeviceDesc%            = I219_SS_NOK1.10.0.1,  PCI\VEN_8086&DEV_57B4
%E57B4NC.DeviceDesc%            = I219_SS_NOK1.10.0.1,  PCI\VEN_8086&DEV_57B4&SUBSYS_00008086
%E57B5NC.DeviceDesc%            = I219_SS.10.0.1,       PCI\VEN_8086&DEV_57B5
%E57B5NC.DeviceDesc%            = I219_SS.10.0.1,       PCI\VEN_8086&DEV_57B5&SUBSYS_00008086
%E57B6NC.DeviceDesc%            = I219_SS.10.0.1,       PCI\VEN_8086&DEV_57B6
%E57B6NC.DeviceDesc%            = I219_SS.10.0.1,       PCI\VEN_8086&DEV_57B6&SUBSYS_00008086
%E57B7NC.DeviceDesc%            = I219_SS_NOK1.10.0.1,  PCI\VEN_8086&DEV_57B7
%E57B7NC.DeviceDesc%            = I219_SS_NOK1.10.0.1,  PCI\VEN_8086&DEV_57B7&SUBSYS_00008086
%E57B8NC.DeviceDesc%            = I219_SS_NOK1.10.0.1,  PCI\VEN_8086&DEV_57B8
%E57B8NC.DeviceDesc%            = I219_SS_NOK1.10.0.1,  PCI\VEN_8086&DEV_57B8&SUBSYS_00008086

[Intel.NTamd64.10.0.1..18362]
; DisplayName                   Section                               DeviceID
; -----------                   -------                               --------
%E153ANC.DeviceDesc%            = I217.10.0.1.19H1,          PCI\VEN_8086&DEV_153A
%E153ANC.DeviceDesc%            = I217.10.0.1.19H1,          PCI\VEN_8086&DEV_153A&SUBSYS_00008086
%E153BNC.DeviceDesc%            = I217.10.0.1.19H1,          PCI\VEN_8086&DEV_153B
%E153BNC.DeviceDesc%            = I217.10.0.1.19H1,          PCI\VEN_8086&DEV_153B&SUBSYS_00008086
%E155ANC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_155A
%E155ANC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_155A&SUBSYS_00008086
%E1559NC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_1559
%E1559NC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_1559&SUBSYS_00008086
%E15A0NC.DeviceDesc%            = I217.10.0.1.19H1,          PCI\VEN_8086&DEV_15A0
%E15A0NC.DeviceDesc%            = I217.10.0.1.19H1,          PCI\VEN_8086&DEV_15A0&SUBSYS_00008086
%E15A1NC.DeviceDesc%            = I217.10.0.1.19H1,          PCI\VEN_8086&DEV_15A1
%E15A1NC.DeviceDesc%            = I217.10.0.1.19H1,          PCI\VEN_8086&DEV_15A1&SUBSYS_00008086
%E15A2NC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_15A2
%E15A2NC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_15A2&SUBSYS_00008086
%E15A3NC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_15A3
%E15A3NC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_15A3&SUBSYS_00008086
%E156FNC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_156F
%E156FNC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_156F&SUBSYS_00008086
%E1570NC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_1570
%E1570NC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_1570&SUBSYS_00008086
%E15B7NC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_15B7
%E15B7NC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_15B7&SUBSYS_00008086
%E15B8NC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_15B8
%E15B8NC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_15B8&SUBSYS_00008086
%E15B9NC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_15B9
%E15B9NC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_15B9&SUBSYS_00008086
%E15D7NC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_15D7
%E15D7NC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_15D7&SUBSYS_00008086
%E15D8NC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_15D8
%E15D8NC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_15D8&SUBSYS_00008086
%E15E3NC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_15E3
%E15E3NC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_15E3&SUBSYS_00008086
%E15D6NC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_15D6
%E15D6NC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_15D6&SUBSYS_00008086
%E15BBNC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_15BB
%E15BBNC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_15BB&SUBSYS_00008086
%E15BCNC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_15BC
%E15BCNC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_15BC&SUBSYS_00008086
%E15BDNC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_15BD
%E15BDNC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_15BD&SUBSYS_00008086
%E15BENC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_15BE
%E15BENC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_15BE&SUBSYS_00008086
%E15DFNC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_15DF
%E15DFNC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_15DF&SUBSYS_00008086
%E15E0NC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_15E0
%E15E0NC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_15E0&SUBSYS_00008086
%E15E1NC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_15E1
%E15E1NC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_15E1&SUBSYS_00008086
%E15E2NC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_15E2
%E15E2NC.DeviceDesc%            = I219.10.0.1.19H1,          PCI\VEN_8086&DEV_15E2&SUBSYS_00008086
%E0D4ENC.DeviceDesc%            = I219_MS.10.0.1.19H1,       PCI\VEN_8086&DEV_0D4E
%E0D4ENC.DeviceDesc%            = I219_MS.10.0.1.19H1,       PCI\VEN_8086&DEV_0D4E&SUBSYS_00008086
%E0D4FNC.DeviceDesc%            = I219_MS.10.0.1.19H1,       PCI\VEN_8086&DEV_0D4F
%E0D4FNC.DeviceDesc%            = I219_MS.10.0.1.19H1,       PCI\VEN_8086&DEV_0D4F&SUBSYS_00008086
%E0D4CNC.DeviceDesc%            = I219_MS.10.0.1.19H1,       PCI\VEN_8086&DEV_0D4C
%E0D4CNC.DeviceDesc%            = I219_MS.10.0.1.19H1,       PCI\VEN_8086&DEV_0D4C&SUBSYS_00008086
%E0D4DNC.DeviceDesc%            = I219_MS.10.0.1.19H1,       PCI\VEN_8086&DEV_0D4D
%E0D4DNC.DeviceDesc%            = I219_MS.10.0.1.19H1,       PCI\VEN_8086&DEV_0D4D&SUBSYS_00008086
%E0D53NC.DeviceDesc%            = I219_MS.10.0.1.19H1,       PCI\VEN_8086&DEV_0D53
%E0D53NC.DeviceDesc%            = I219_MS.10.0.1.19H1,       PCI\VEN_8086&DEV_0D53&SUBSYS_00008086
%E0D55NC.DeviceDesc%            = I219_MS.10.0.1.19H1,       PCI\VEN_8086&DEV_0D55
%E0D55NC.DeviceDesc%            = I219_MS.10.0.1.19H1,       PCI\VEN_8086&DEV_0D55&SUBSYS_00008086
%E15F9NC.DeviceDesc%            = I219_SS.10.0.1.19H1,       PCI\VEN_8086&DEV_15F9
%E15F9NC.DeviceDesc%            = I219_SS.10.0.1.19H1,       PCI\VEN_8086&DEV_15F9&SUBSYS_00008086
%E15FANC.DeviceDesc%            = I219_SS.10.0.1.19H1,       PCI\VEN_8086&DEV_15FA
%E15FANC.DeviceDesc%            = I219_SS.10.0.1.19H1,       PCI\VEN_8086&DEV_15FA&SUBSYS_00008086
%E15FBNC.DeviceDesc%            = I219_SS.10.0.1.19H1,       PCI\VEN_8086&DEV_15FB
%E15FBNC.DeviceDesc%            = I219_SS.10.0.1.19H1,       PCI\VEN_8086&DEV_15FB&SUBSYS_00008086
%E15FCNC.DeviceDesc%            = I219_SS.10.0.1.19H1,       PCI\VEN_8086&DEV_15FC
%E15FCNC.DeviceDesc%            = I219_SS.10.0.1.19H1,       PCI\VEN_8086&DEV_15FC&SUBSYS_00008086
%E15F4NC.DeviceDesc%            = I219_SS.10.0.1.19H1,       PCI\VEN_8086&DEV_15F4
%E15F4NC.DeviceDesc%            = I219_SS.10.0.1.19H1,       PCI\VEN_8086&DEV_15F4&SUBSYS_00008086
%E1A1ENC.DeviceDesc%            = I219_SS.10.0.1.19H1,       PCI\VEN_8086&DEV_1A1E
%E1A1ENC.DeviceDesc%            = I219_SS.10.0.1.19H1,       PCI\VEN_8086&DEV_1A1E&SUBSYS_00008086
%E1A1FNC.DeviceDesc%            = I219_SS.10.0.1.19H1,       PCI\VEN_8086&DEV_1A1F
%E1A1FNC.DeviceDesc%            = I219_SS.10.0.1.19H1,       PCI\VEN_8086&DEV_1A1F&SUBSYS_00008086
%E1A1CNC.DeviceDesc%            = I219_SS.10.0.1.19H1,       PCI\VEN_8086&DEV_1A1C
%E1A1CNC.DeviceDesc%            = I219_SS.10.0.1.19H1,       PCI\VEN_8086&DEV_1A1C&SUBSYS_00008086
%E1A1DNC.DeviceDesc%            = I219_SS.10.0.1.19H1,       PCI\VEN_8086&DEV_1A1D
%E1A1DNC.DeviceDesc%            = I219_SS.10.0.1.19H1,       PCI\VEN_8086&DEV_1A1D&SUBSYS_00008086
%E550ANC.DeviceDesc%            = I219_SS_NOK1.10.0.1.19H1,  PCI\VEN_8086&DEV_550A
%E550ANC.DeviceDesc%            = I219_SS_NOK1.10.0.1.19H1,  PCI\VEN_8086&DEV_550A&SUBSYS_00008086
%E550BNC.DeviceDesc%            = I219_SS_NOK1.10.0.1.19H1,  PCI\VEN_8086&DEV_550B
%E550BNC.DeviceDesc%            = I219_SS_NOK1.10.0.1.19H1,  PCI\VEN_8086&DEV_550B&SUBSYS_00008086
%E550CNC.DeviceDesc%            = I219_SS.10.0.1.19H1,       PCI\VEN_8086&DEV_550C
%E550CNC.DeviceDesc%            = I219_SS.10.0.1.19H1,       PCI\VEN_8086&DEV_550C&SUBSYS_00008086
%E550DNC.DeviceDesc%            = I219_SS.10.0.1.19H1,       PCI\VEN_8086&DEV_550D
%E550DNC.DeviceDesc%            = I219_SS.10.0.1.19H1,       PCI\VEN_8086&DEV_550D&SUBSYS_00008086
%E0DC5NC.DeviceDesc%            = I219_SS.10.0.1.19H1,       PCI\VEN_8086&DEV_0DC5
%E0DC5NC.DeviceDesc%            = I219_SS.10.0.1.19H1,       PCI\VEN_8086&DEV_0DC5&SUBSYS_00008086
%E0DC6NC.DeviceDesc%            = I219_SS.10.0.1.19H1,       PCI\VEN_8086&DEV_0DC6
%E0DC6NC.DeviceDesc%            = I219_SS.10.0.1.19H1,       PCI\VEN_8086&DEV_0DC6&SUBSYS_00008086
%E0DC7NC.DeviceDesc%            = I219_SS.10.0.1.19H1,       PCI\VEN_8086&DEV_0DC7
%E0DC7NC.DeviceDesc%            = I219_SS.10.0.1.19H1,       PCI\VEN_8086&DEV_0DC7&SUBSYS_00008086
%E0DC8NC.DeviceDesc%            = I219_SS.10.0.1.19H1,       PCI\VEN_8086&DEV_0DC8
%E0DC8NC.DeviceDesc%            = I219_SS.10.0.1.19H1,       PCI\VEN_8086&DEV_0DC8&SUBSYS_00008086
%E57A0NC.DeviceDesc%            = I219_SS_NOK1.10.0.1.19H1,  PCI\VEN_8086&DEV_57A0
%E57A0NC.DeviceDesc%            = I219_SS_NOK1.10.0.1.19H1,  PCI\VEN_8086&DEV_57A0&SUBSYS_00008086
%E57A1NC.DeviceDesc%            = I219_SS_NOK1.10.0.1.19H1,  PCI\VEN_8086&DEV_57A1
%E57A1NC.DeviceDesc%            = I219_SS_NOK1.10.0.1.19H1,  PCI\VEN_8086&DEV_57A1&SUBSYS_00008086
%E550ENC.DeviceDesc%            = I219_SS_NOK1.10.0.1.19H1,  PCI\VEN_8086&DEV_550E
%E550ENC.DeviceDesc%            = I219_SS_NOK1.10.0.1.19H1,  PCI\VEN_8086&DEV_550E&SUBSYS_00008086
%E550FNC.DeviceDesc%            = I219_SS_NOK1.10.0.1.19H1,  PCI\VEN_8086&DEV_550F
%E550FNC.DeviceDesc%            = I219_SS_NOK1.10.0.1.19H1,  PCI\VEN_8086&DEV_550F&SUBSYS_00008086
%E57B3NC.DeviceDesc%            = I219_SS_NOK1.10.0.1.19H1,  PCI\VEN_8086&DEV_57B3
%E57B3NC.DeviceDesc%            = I219_SS_NOK1.10.0.1.19H1,  PCI\VEN_8086&DEV_57B3&SUBSYS_00008086
%E57B4NC.DeviceDesc%            = I219_SS_NOK1.10.0.1.19H1,  PCI\VEN_8086&DEV_57B4
%E57B4NC.DeviceDesc%            = I219_SS_NOK1.10.0.1.19H1,  PCI\VEN_8086&DEV_57B4&SUBSYS_00008086
%E57B5NC.DeviceDesc%            = I219_SS.10.0.1.19H1,       PCI\VEN_8086&DEV_57B5
%E57B5NC.DeviceDesc%            = I219_SS.10.0.1.19H1,       PCI\VEN_8086&DEV_57B5&SUBSYS_00008086
%E57B6NC.DeviceDesc%            = I219_SS.10.0.1.19H1,       PCI\VEN_8086&DEV_57B6
%E57B6NC.DeviceDesc%            = I219_SS.10.0.1.19H1,       PCI\VEN_8086&DEV_57B6&SUBSYS_00008086
%E57B7NC.DeviceDesc%            = I219_SS_NOK1.10.0.1.19H1,  PCI\VEN_8086&DEV_57B7
%E57B7NC.DeviceDesc%            = I219_SS_NOK1.10.0.1.19H1,  PCI\VEN_8086&DEV_57B7&SUBSYS_00008086
%E57B8NC.DeviceDesc%            = I219_SS_NOK1.10.0.1.19H1,  PCI\VEN_8086&DEV_57B8
%E57B8NC.DeviceDesc%            = I219_SS_NOK1.10.0.1.19H1,  PCI\VEN_8086&DEV_57B8&SUBSYS_00008086

[Intel.NTamd64.10.0...17763]
; DisplayName                   Section       DeviceID
; -----------                   -------       --------
%E153ANC.DeviceDesc%            = I217,       PCI\VEN_8086&DEV_153A
%E153ANC.DeviceDesc%            = I217,       PCI\VEN_8086&DEV_153A&SUBSYS_00008086
%E155ANC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_155A
%E155ANC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_155A&SUBSYS_00008086
%E15A0NC.DeviceDesc%            = I217,       PCI\VEN_8086&DEV_15A0
%E15A0NC.DeviceDesc%            = I217,       PCI\VEN_8086&DEV_15A0&SUBSYS_00008086
%E15A2NC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_15A2
%E15A2NC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_15A2&SUBSYS_00008086
%E156FNC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_156F
%E156FNC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_156F&SUBSYS_00008086
%E15B7NC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_15B7
%E15B7NC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_15B7&SUBSYS_00008086
%E15B9NC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_15B9
%E15B9NC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_15B9&SUBSYS_00008086
%E15D7NC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_15D7
%E15D7NC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_15D7&SUBSYS_00008086
%E15E3NC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_15E3
%E15E3NC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_15E3&SUBSYS_00008086
%E15BBNC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_15BB
%E15BBNC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_15BB&SUBSYS_00008086
%E15BDNC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_15BD
%E15BDNC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_15BD&SUBSYS_00008086
%E15DFNC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_15DF
%E15DFNC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_15DF&SUBSYS_00008086
%E15E1NC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_15E1
%E15E1NC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_15E1&SUBSYS_00008086
%E0D4ENC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_0D4E
%E0D4ENC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_0D4E&SUBSYS_00008086
%E0D4CNC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_0D4C
%E0D4CNC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_0D4C&SUBSYS_00008086
%E0D53NC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_0D53
%E0D53NC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_0D53&SUBSYS_00008086
%E15F9NC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_15F9
%E15F9NC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_15F9&SUBSYS_00008086
%E15FBNC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_15FB
%E15FBNC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_15FB&SUBSYS_00008086
%E15F4NC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_15F4
%E15F4NC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_15F4&SUBSYS_00008086
%E1A1ENC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_1A1E
%E1A1ENC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_1A1E&SUBSYS_00008086
%E1A1CNC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_1A1C
%E1A1CNC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_1A1C&SUBSYS_00008086
%E550ANC.DeviceDesc%            = I219_NOK1,  PCI\VEN_8086&DEV_550A
%E550ANC.DeviceDesc%            = I219_NOK1,  PCI\VEN_8086&DEV_550A&SUBSYS_00008086
%E550CNC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_550C
%E550CNC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_550C&SUBSYS_00008086
%E0DC5NC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_0DC5
%E0DC5NC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_0DC5&SUBSYS_00008086
%E0DC7NC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_0DC7
%E0DC7NC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_0DC7&SUBSYS_00008086
%E57A0NC.DeviceDesc%            = I219_NOK1,  PCI\VEN_8086&DEV_57A0
%E57A0NC.DeviceDesc%            = I219_NOK1,  PCI\VEN_8086&DEV_57A0&SUBSYS_00008086
%E550ENC.DeviceDesc%            = I219_NOK1,  PCI\VEN_8086&DEV_550E
%E550ENC.DeviceDesc%            = I219_NOK1,  PCI\VEN_8086&DEV_550E&SUBSYS_00008086
%E57B3NC.DeviceDesc%            = I219_NOK1,  PCI\VEN_8086&DEV_57B3
%E57B3NC.DeviceDesc%            = I219_NOK1,  PCI\VEN_8086&DEV_57B3&SUBSYS_00008086
%E57B5NC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_57B5
%E57B5NC.DeviceDesc%            = I219,       PCI\VEN_8086&DEV_57B5&SUBSYS_00008086
%E57B7NC.DeviceDesc%            = I219_NOK1,  PCI\VEN_8086&DEV_57B7
%E57B7NC.DeviceDesc%            = I219_NOK1,  PCI\VEN_8086&DEV_57B7&SUBSYS_00008086

[Intel.NTamd64.10.0...18362]
; DisplayName                   Section            DeviceID
; -----------                   -------            --------
%E153ANC.DeviceDesc%            = I217.19H1,       PCI\VEN_8086&DEV_153A
%E153ANC.DeviceDesc%            = I217.19H1,       PCI\VEN_8086&DEV_153A&SUBSYS_00008086
%E155ANC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_155A
%E155ANC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_155A&SUBSYS_00008086
%E15A0NC.DeviceDesc%            = I217.19H1,       PCI\VEN_8086&DEV_15A0
%E15A0NC.DeviceDesc%            = I217.19H1,       PCI\VEN_8086&DEV_15A0&SUBSYS_00008086
%E15A2NC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_15A2
%E15A2NC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_15A2&SUBSYS_00008086
%E156FNC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_156F
%E156FNC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_156F&SUBSYS_00008086
%E15B7NC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_15B7
%E15B7NC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_15B7&SUBSYS_00008086
%E15B9NC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_15B9
%E15B9NC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_15B9&SUBSYS_00008086
%E15D7NC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_15D7
%E15D7NC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_15D7&SUBSYS_00008086
%E15E3NC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_15E3
%E15E3NC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_15E3&SUBSYS_00008086
%E15BBNC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_15BB
%E15BBNC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_15BB&SUBSYS_00008086
%E15BDNC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_15BD
%E15BDNC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_15BD&SUBSYS_00008086
%E15DFNC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_15DF
%E15DFNC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_15DF&SUBSYS_00008086
%E15E1NC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_15E1
%E15E1NC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_15E1&SUBSYS_00008086
%E0D4ENC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_0D4E
%E0D4ENC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_0D4E&SUBSYS_00008086
%E0D4CNC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_0D4C
%E0D4CNC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_0D4C&SUBSYS_00008086
%E0D53NC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_0D53
%E0D53NC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_0D53&SUBSYS_00008086
%E15F9NC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_15F9
%E15F9NC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_15F9&SUBSYS_00008086
%E15FBNC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_15FB
%E15FBNC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_15FB&SUBSYS_00008086
%E15F4NC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_15F4
%E15F4NC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_15F4&SUBSYS_00008086
%E1A1ENC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_1A1E
%E1A1ENC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_1A1E&SUBSYS_00008086
%E1A1CNC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_1A1C
%E1A1CNC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_1A1C&SUBSYS_00008086
%E550ANC.DeviceDesc%            = I219_NOK1.19H1,  PCI\VEN_8086&DEV_550A
%E550ANC.DeviceDesc%            = I219_NOK1.19H1,  PCI\VEN_8086&DEV_550A&SUBSYS_00008086
%E550CNC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_550C
%E550CNC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_550C&SUBSYS_00008086
%E0DC5NC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_0DC5
%E0DC5NC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_0DC5&SUBSYS_00008086
%E0DC7NC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_0DC7
%E0DC7NC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_0DC7&SUBSYS_00008086
%E57A0NC.DeviceDesc%            = I219_NOK1.19H1,  PCI\VEN_8086&DEV_57A0
%E57A0NC.DeviceDesc%            = I219_NOK1.19H1,  PCI\VEN_8086&DEV_57A0&SUBSYS_00008086
%E550ENC.DeviceDesc%            = I219_NOK1.19H1,  PCI\VEN_8086&DEV_550E
%E550ENC.DeviceDesc%            = I219_NOK1.19H1,  PCI\VEN_8086&DEV_550E&SUBSYS_00008086
%E57B3NC.DeviceDesc%            = I219_NOK1.19H1,  PCI\VEN_8086&DEV_57B3
%E57B3NC.DeviceDesc%            = I219_NOK1.19H1,  PCI\VEN_8086&DEV_57B3&SUBSYS_00008086
%E57B5NC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_57B5
%E57B5NC.DeviceDesc%            = I219.19H1,       PCI\VEN_8086&DEV_57B5&SUBSYS_00008086
%E57B7NC.DeviceDesc%            = I219_NOK1.19H1,  PCI\VEN_8086&DEV_57B7
%E57B7NC.DeviceDesc%            = I219_NOK1.19H1,  PCI\VEN_8086&DEV_57B7&SUBSYS_00008086
    
        
    
    
    
    
    
    
    

;===============================================================================

;                WINDOWS 10/11 for 64-bit EXTENDED PLATFORMS

;
;===============================================================================

;-------------------------------------------------------------------------------

; Intel(R) Ethernet Connection I217-LM

; Intel(R) Ethernet Connection I217-V

; Intel(R) Ethernet Connection (2) I218-LM

; Intel(R) Ethernet Connection (2) I218-V
;-------------------------------------------------------------------------------
[I217.10.0.1]
Characteristics    = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType            = 5    ; PCI
DelReg             = Advanced.DelReg
AddReg             = e1d.reg, TcpSeg.reg, JumboPacket.reg
AddReg             = Copper.reg, Copper1000.reg, Autoneg10100.reg
AddReg             = Powermgmt.reg, WakeOnSlot.reg
AddReg             = RTD3.reg
AddReg             = AcDcLink.reg
AddReg             = IntelANSVlanID.reg
AddReg             = NDISVlanId.reg
AddReg             = Sips.reg
AddReg             = Po.reg
AddReg             = EEE.reg
AddReg             = enableK1.reg
AddReg             = UninstallW2.reg
AddReg             = CoInKS.reg
CopyFiles          = winblue.CopyFiles, MessageDll.CopyFiles
*IfType            = 6    ; IF_TYPE_ETHERNET_CSMACD
*MediaType         = 0    ; NdisMedium802_3
*PhysicalMediaType = 14 ; NdisPhysicalMedium802_3

[I217.10.0.1.Services]
AddService = e1dexpress, 2, winblue.Service, winblue.EventLog

[I217.10.0.1.HW]
Include            = pci.inf
Needs              = PciIoSpaceNotRequired.HW
AddReg             = MSI.reg

;-------------------------------------------------------------------------------

; Intel(R) Ethernet Connection I218-LM

; Intel(R) Ethernet Connection I218-V

; Intel(R) Ethernet Connection (3) I218-LM

; Intel(R) Ethernet Connection (3) I218-V

; Intel(R) Ethernet Connection I219-LM

; Intel(R) Ethernet Connection I219-V

; Intel(R) Ethernet Connection (2) I219-LM

; Intel(R) Ethernet Connection (2) I219-V

; Intel(R) Ethernet Connection (3) I219-LM

; Intel(R) Ethernet Connection (4) I219-LM

; Intel(R) Ethernet Connection (4) I219-V

; Intel(R) Ethernet Connection (5) I219-LM

; Intel(R) Ethernet Connection (5) I219-V

; Intel(R) Ethernet Connection (6) I219-LM

; Intel(R) Ethernet Connection (6) I219-V

; Intel(R) Ethernet Connection (7) I219-LM

; Intel(R) Ethernet Connection (7) I219-V

; Intel(R) Ethernet Connection (8) I219-LM

; Intel(R) Ethernet Connection (8) I219-V

; Intel(R) Ethernet Connection (9) I219-LM

; Intel(R) Ethernet Connection (9) I219-V
;-------------------------------------------------------------------------------
[I219.10.0.1]
Characteristics    = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType            = 5    ; PCI
DelReg             = Advanced.DelReg
AddReg             = e1d.reg, TcpSeg.reg, JumboPacket.reg
AddReg             = Copper.reg, Copper1000.reg, Autoneg10100.reg
AddReg             = Powermgmt.reg, WakeOnSlot.reg
AddReg             = RTD3.reg
AddReg             = AcDcLink.reg
AddReg             = IntelANSVlanID.reg
AddReg             = NDISVlanId.reg
AddReg             = Sips.reg
AddReg             = Po.reg
AddReg             = EEE.reg
AddReg             = ulp.reg
AddReg             = enableK1.reg
AddReg             = UninstallW2.reg
AddReg             = CoInKS.reg
CopyFiles          = winblue.CopyFiles, MessageDll.CopyFiles
*IfType            = 6    ; IF_TYPE_ETHERNET_CSMACD
*MediaType         = 0    ; NdisMedium802_3
*PhysicalMediaType = 14 ; NdisPhysicalMedium802_3

[I219.10.0.1.Services]
AddService = e1dexpress, 2, winblue.Service, winblue.EventLog

[I219.10.0.1.HW]
Include            = pci.inf
Needs              = PciIoSpaceNotRequired.HW
AddReg             = MSI.reg

;-------------------------------------------------------------------------------

; Intel(R) Ethernet Connection (10) I219-LM

; Intel(R) Ethernet Connection (10) I219-V

; Intel(R) Ethernet Connection (11) I219-LM

; Intel(R) Ethernet Connection (11) I219-V

; Intel(R) Ethernet Connection (12) I219-LM

; Intel(R) Ethernet Connection (12) I219-V
;-------------------------------------------------------------------------------
[I219_MS.10.0.1]
Characteristics    = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType            = 5    ; PCI
DelReg             = Advanced.DelReg
AddReg             = e1d.reg, TcpSeg.reg, JumboPacket.reg
AddReg             = Copper.reg, Copper1000.reg, Autoneg10100.reg
AddReg             = Powermgmt.reg, WakeOnSlot.reg
AddReg             = ModernStandbyWoLMagicPacket.reg
AddReg             = RTD3.reg
AddReg             = AcDcLink.reg
AddReg             = IntelANSVlanID.reg
AddReg             = NDISVlanId.reg
AddReg             = Sips.reg
AddReg             = Po.reg
AddReg             = EEE.reg
AddReg             = ulp.reg
AddReg             = enableK1.reg
AddReg             = UninstallW2.reg
AddReg             = CoInKS.reg
CopyFiles          = winblue.CopyFiles, MessageDll.CopyFiles
*IfType            = 6    ; IF_TYPE_ETHERNET_CSMACD
*MediaType         = 0    ; NdisMedium802_3
*PhysicalMediaType = 14 ; NdisPhysicalMedium802_3

[I219_MS.10.0.1.Services]
AddService = e1dexpress, 2, winblue.Service, winblue.EventLog

[I219_MS.10.0.1.HW]
Include            = pci.inf
Needs              = PciIoSpaceNotRequired.HW
AddReg             = MSI.reg

;-------------------------------------------------------------------------------

; Intel(R) Ethernet Connection (14) I219-LM

; Intel(R) Ethernet Connection (14) I219-V

; Intel(R) Ethernet Connection (13) I219-LM

; Intel(R) Ethernet Connection (13) I219-V

; Intel(R) Ethernet Connection (15) I219-LM

; Intel(R) Ethernet Connection (16) I219-LM

; Intel(R) Ethernet Connection (16) I219-V

; Intel(R) Ethernet Connection (17) I219-LM

; Intel(R) Ethernet Connection (17) I219-V

; Intel(R) Ethernet Connection (23) I219-LM

; Intel(R) Ethernet Connection (23) I219-V

; Intel(R) Ethernet Connection (22) I219-LM

; Intel(R) Ethernet Connection (22) I219-V

; Intel(R) Ethernet Connection (19) I219-LM

; Intel(R) Ethernet Connection (19) I219-V

; Intel(R) Ethernet Connection (26) I219-LM

; Intel(R) Ethernet Connection (26) I219-V
;-------------------------------------------------------------------------------
[I219_SS.10.0.1]
Characteristics    = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType            = 5    ; PCI
DelReg             = Advanced.DelReg
AddReg             = e1d.reg, TcpSeg.reg, JumboPacket.reg
AddReg             = Copper.reg, Copper1000.reg, Autoneg10100.reg
AddReg             = Powermgmt.reg, WakeOnSlot.reg
AddReg             = ModernStandbyWoLMagicPacket.reg
AddReg             = RTD3.reg
AddReg             = AcDcLink.reg
AddReg             = IntelANSVlanID.reg
AddReg             = NDISVlanId.reg
AddReg             = Sips.reg
AddReg             = Po.reg
AddReg             = SelectiveSuspend.reg
AddReg             = EEE.reg
AddReg             = ulp.reg
AddReg             = enableK1.reg
AddReg             = UninstallW2.reg
AddReg             = CoInKS.reg
CopyFiles          = winblue.CopyFiles, MessageDll.CopyFiles
*IfType            = 6    ; IF_TYPE_ETHERNET_CSMACD
*MediaType         = 0    ; NdisMedium802_3
*PhysicalMediaType = 14 ; NdisPhysicalMedium802_3

[I219_SS.10.0.1.Services]
AddService = e1dexpress, 2, winblue.Service, winblue.EventLog

[I219_SS.10.0.1.HW]
Include            = pci.inf
Needs              = PciIoSpaceNotRequired.HW
AddReg             = MSI.reg

;-------------------------------------------------------------------------------

; Intel(R) Ethernet Connection (18) I219-LM

; Intel(R) Ethernet Connection (18) I219-V

; Intel(R) Ethernet Connection (20) I219-LM

; Intel(R) Ethernet Connection (20) I219-V

; Intel(R) Ethernet Connection (24) I219-LM

; Intel(R) Ethernet Connection (24) I219-V

; Intel(R) Ethernet Connection (25) I219-LM

; Intel(R) Ethernet Connection (25) I219-V

; Intel(R) Ethernet Connection (27) I219-LM

; Intel(R) Ethernet Connection (27) I219-V
;-------------------------------------------------------------------------------
[I219_SS_NOK1.10.0.1]
Characteristics    = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType            = 5    ; PCI
DelReg             = Advanced.DelReg
AddReg             = e1d.reg, TcpSeg.reg, JumboPacket.reg
AddReg             = Copper.reg, Copper1000.reg, Autoneg10100.reg
AddReg             = Powermgmt.reg, WakeOnSlot.reg
AddReg             = ModernStandbyWoLMagicPacket.reg
AddReg             = RTD3.reg
AddReg             = AcDcLink.reg
AddReg             = IntelANSVlanID.reg
AddReg             = NDISVlanId.reg
AddReg             = Sips.reg
AddReg             = Po.reg
AddReg             = SelectiveSuspend.reg
AddReg             = EEE.reg
AddReg             = ulp.reg
AddReg             = disableK1.reg
AddReg             = UninstallW2.reg
AddReg             = CoInKS.reg
CopyFiles          = winblue.CopyFiles, MessageDll.CopyFiles
*IfType            = 6    ; IF_TYPE_ETHERNET_CSMACD
*MediaType         = 0    ; NdisMedium802_3
*PhysicalMediaType = 14 ; NdisPhysicalMedium802_3

[I219_SS_NOK1.10.0.1.Services]
AddService = e1dexpress, 2, winblue.Service, winblue.EventLog

[I219_SS_NOK1.10.0.1.HW]
Include            = pci.inf
Needs              = PciIoSpaceNotRequired.HW
AddReg             = MSI.reg
    
        
    
    
    
    
    
    
    

;===============================================================================

;                WINDOWS 10 / 11 /  2022 for 64-bit EXTENDED PLATFORMS

;
;===============================================================================

;-------------------------------------------------------------------------------

; Intel(R) Ethernet Connection I217-LM

; Intel(R) Ethernet Connection I217-V

; Intel(R) Ethernet Connection (2) I218-LM

; Intel(R) Ethernet Connection (2) I218-V
;-------------------------------------------------------------------------------

[I217.10.0.1.19H1]
Characteristics    = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType            = 5    ; PCI
DelReg             = Advanced.DelReg
AddReg             = e1d.reg, TcpSeg.reg, JumboPacket.reg
AddReg             = Copper.reg, Copper1000.reg, Autoneg10100.reg
AddReg             = Powermgmt.reg, WakeOnSlot.reg
AddReg             = RTD3.reg
AddReg             = AcDcLink.reg
AddReg             = IntelANSVlanID.reg
AddReg             = NDISVlanId.reg
AddReg             = Sips.reg
AddReg             = Po.reg
AddReg             = EEE.reg
AddReg             = enableK1.reg
AddReg             = UninstallW2.reg
AddReg             = CoInKS.reg
AddReg             = PtpHardwareTimestamp.reg
AddReg             = SoftwareTimestamp.reg
CopyFiles          = winblue.CopyFiles, MessageDll.CopyFiles
*IfType            = 6    ; IF_TYPE_ETHERNET_CSMACD
*MediaType         = 0    ; NdisMedium802_3
*PhysicalMediaType = 14 ; NdisPhysicalMedium802_3

[I217.10.0.1.19H1.Services]
AddService = e1dexpress, 2, winblue.Service, winblue.EventLog

[I217.10.0.1.19H1.HW]
Include            = pci.inf
Needs              = PciIoSpaceNotRequired.HW
AddReg             = MSI.reg

;-------------------------------------------------------------------------------

; Intel(R) Ethernet Connection I218-LM

; Intel(R) Ethernet Connection I218-V

; Intel(R) Ethernet Connection (3) I218-LM

; Intel(R) Ethernet Connection (3) I218-V

; Intel(R) Ethernet Connection I219-LM

; Intel(R) Ethernet Connection I219-V

; Intel(R) Ethernet Connection (2) I219-LM

; Intel(R) Ethernet Connection (2) I219-V

; Intel(R) Ethernet Connection (3) I219-LM

; Intel(R) Ethernet Connection (4) I219-LM

; Intel(R) Ethernet Connection (4) I219-V

; Intel(R) Ethernet Connection (5) I219-LM

; Intel(R) Ethernet Connection (5) I219-V

; Intel(R) Ethernet Connection (6) I219-LM

; Intel(R) Ethernet Connection (6) I219-V

; Intel(R) Ethernet Connection (7) I219-LM

; Intel(R) Ethernet Connection (7) I219-V

; Intel(R) Ethernet Connection (8) I219-LM

; Intel(R) Ethernet Connection (8) I219-V

; Intel(R) Ethernet Connection (9) I219-LM

; Intel(R) Ethernet Connection (9) I219-V
;-------------------------------------------------------------------------------
[I219.10.0.1.19H1]
Characteristics    = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType            = 5    ; PCI
DelReg             = Advanced.DelReg
AddReg             = e1d.reg, TcpSeg.reg, JumboPacket.reg
AddReg             = Copper.reg, Copper1000.reg, Autoneg10100.reg
AddReg             = Powermgmt.reg, WakeOnSlot.reg
AddReg             = RTD3.reg
AddReg             = AcDcLink.reg
AddReg             = IntelANSVlanID.reg
AddReg             = NDISVlanId.reg
AddReg             = Sips.reg
AddReg             = Po.reg
AddReg             = EEE.reg
AddReg             = ulp.reg
AddReg             = enableK1.reg
AddReg             = UninstallW2.reg
AddReg             = CoInKS.reg
AddReg             = PtpHardwareTimestamp.reg
AddReg             = SoftwareTimestamp.reg
CopyFiles          = winblue.CopyFiles, MessageDll.CopyFiles
*IfType            = 6    ; IF_TYPE_ETHERNET_CSMACD
*MediaType         = 0    ; NdisMedium802_3
*PhysicalMediaType = 14 ; NdisPhysicalMedium802_3

[I219.10.0.1.19H1.Services]
AddService = e1dexpress, 2, winblue.Service, winblue.EventLog

[I219.10.0.1.19H1.HW]
Include            = pci.inf
Needs              = PciIoSpaceNotRequired.HW
AddReg             = MSI.reg

;-------------------------------------------------------------------------------

; Intel(R) Ethernet Connection (10) I219-LM

; Intel(R) Ethernet Connection (10) I219-V

; Intel(R) Ethernet Connection (11) I219-LM

; Intel(R) Ethernet Connection (11) I219-V

; Intel(R) Ethernet Connection (12) I219-LM

; Intel(R) Ethernet Connection (12) I219-V
;-------------------------------------------------------------------------------
[I219_MS.10.0.1.19H1]
Characteristics    = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType            = 5    ; PCI
DelReg             = Advanced.DelReg
AddReg             = e1d.reg, TcpSeg.reg, JumboPacket.reg
AddReg             = Copper.reg, Copper1000.reg, Autoneg10100.reg
AddReg             = Powermgmt.reg, WakeOnSlot.reg
AddReg             = ModernStandbyWoLMagicPacket.reg
AddReg             = RTD3.reg
AddReg             = AcDcLink.reg
AddReg             = IntelANSVlanID.reg
AddReg             = NDISVlanId.reg
AddReg             = Sips.reg
AddReg             = Po.reg
AddReg             = EEE.reg
AddReg             = ulp.reg
AddReg             = enableK1.reg
AddReg             = UninstallW2.reg
AddReg             = CoInKS.reg
AddReg             = PtpHardwareTimestamp.reg
AddReg             = SoftwareTimestamp.reg
CopyFiles          = winblue.CopyFiles, MessageDll.CopyFiles
*IfType            = 6    ; IF_TYPE_ETHERNET_CSMACD
*MediaType         = 0    ; NdisMedium802_3
*PhysicalMediaType = 14 ; NdisPhysicalMedium802_3

[I219_MS.10.0.1.19H1.Services]
AddService = e1dexpress, 2, winblue.Service, winblue.EventLog

[I219_MS.10.0.1.19H1.HW]
Include            = pci.inf
Needs              = PciIoSpaceNotRequired.HW
AddReg             = MSI.reg

;-------------------------------------------------------------------------------

; Intel(R) Ethernet Connection (14) I219-LM

; Intel(R) Ethernet Connection (14) I219-V

; Intel(R) Ethernet Connection (13) I219-LM

; Intel(R) Ethernet Connection (13) I219-V

; Intel(R) Ethernet Connection (15) I219-LM

; Intel(R) Ethernet Connection (16) I219-LM

; Intel(R) Ethernet Connection (16) I219-V

; Intel(R) Ethernet Connection (17) I219-LM

; Intel(R) Ethernet Connection (17) I219-V

; Intel(R) Ethernet Connection (23) I219-LM

; Intel(R) Ethernet Connection (23) I219-V

; Intel(R) Ethernet Connection (22) I219-LM

; Intel(R) Ethernet Connection (22) I219-V

; Intel(R) Ethernet Connection (19) I219-LM

; Intel(R) Ethernet Connection (19) I219-V

; Intel(R) Ethernet Connection (26) I219-LM

; Intel(R) Ethernet Connection (26) I219-V
;-------------------------------------------------------------------------------
[I219_SS.10.0.1.19H1]
Characteristics    = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType            = 5    ; PCI
DelReg             = Advanced.DelReg
AddReg             = e1d.reg, TcpSeg.reg, JumboPacket.reg
AddReg             = Copper.reg, Copper1000.reg, Autoneg10100.reg
AddReg             = Powermgmt.reg, WakeOnSlot.reg
AddReg             = ModernStandbyWoLMagicPacket.reg
AddReg             = RTD3.reg
AddReg             = AcDcLink.reg
AddReg             = IntelANSVlanID.reg
AddReg             = NDISVlanId.reg
AddReg             = Sips.reg
AddReg             = Po.reg
AddReg             = SelectiveSuspend.reg
AddReg             = EEE.reg
AddReg             = ulp.reg
AddReg             = enableK1.reg
AddReg             = UninstallW2.reg
AddReg             = CoInKS.reg
AddReg             = PtpHardwareTimestamp.reg
AddReg             = SoftwareTimestamp.reg
CopyFiles          = winblue.CopyFiles, MessageDll.CopyFiles
*IfType            = 6    ; IF_TYPE_ETHERNET_CSMACD
*MediaType         = 0    ; NdisMedium802_3
*PhysicalMediaType = 14 ; NdisPhysicalMedium802_3

[I219_SS.10.0.1.19H1.Services]
AddService = e1dexpress, 2, winblue.Service, winblue.EventLog

[I219_SS.10.0.1.19H1.HW]
Include            = pci.inf
Needs              = PciIoSpaceNotRequired.HW
AddReg             = MSI.reg

;-------------------------------------------------------------------------------

; Intel(R) Ethernet Connection (18) I219-LM

; Intel(R) Ethernet Connection (18) I219-V

; Intel(R) Ethernet Connection (20) I219-LM

; Intel(R) Ethernet Connection (20) I219-V

; Intel(R) Ethernet Connection (24) I219-LM

; Intel(R) Ethernet Connection (24) I219-V

; Intel(R) Ethernet Connection (25) I219-LM

; Intel(R) Ethernet Connection (25) I219-V

; Intel(R) Ethernet Connection (27) I219-LM

; Intel(R) Ethernet Connection (27) I219-V
;-------------------------------------------------------------------------------
[I219_SS_NOK1.10.0.1.19H1]
Characteristics    = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType            = 5    ; PCI
DelReg             = Advanced.DelReg
AddReg             = e1d.reg, TcpSeg.reg, JumboPacket.reg
AddReg             = Copper.reg, Copper1000.reg, Autoneg10100.reg
AddReg             = Powermgmt.reg, WakeOnSlot.reg
AddReg             = ModernStandbyWoLMagicPacket.reg
AddReg             = RTD3.reg
AddReg             = AcDcLink.reg
AddReg             = IntelANSVlanID.reg
AddReg             = NDISVlanId.reg
AddReg             = Sips.reg
AddReg             = Po.reg
AddReg             = SelectiveSuspend.reg
AddReg             = EEE.reg
AddReg             = ulp.reg
AddReg             = disableK1.reg
AddReg             = UninstallW2.reg
AddReg             = CoInKS.reg
AddReg             = PtpHardwareTimestamp.reg
AddReg             = SoftwareTimestamp.reg
CopyFiles          = winblue.CopyFiles, MessageDll.CopyFiles
*IfType            = 6    ; IF_TYPE_ETHERNET_CSMACD
*MediaType         = 0    ; NdisMedium802_3
*PhysicalMediaType = 14 ; NdisPhysicalMedium802_3

[I219_SS_NOK1.10.0.1.19H1.Services]
AddService = e1dexpress, 2, winblue.Service, winblue.EventLog

[I219_SS_NOK1.10.0.1.19H1.HW]
Include            = pci.inf
Needs              = PciIoSpaceNotRequired.HW
AddReg             = MSI.reg
    
        
    
    

;===============================================================================
;

;                Windows Server 2019 

;
;===============================================================================

;-------------------------------------------------------------------------------

; Intel(R) Ethernet Connection I217-LM

; Intel(R) Ethernet Connection I217-V

; Intel(R) Ethernet Connection (2) I218-LM

; Intel(R) Ethernet Connection (2) I218-V
;-------------------------------------------------------------------------------

[I217]
Characteristics    = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType            = 5    ; PCI
DelReg             = Advanced.DelReg
AddReg             = e1d.reg, TcpSeg.reg, JumboPacket.reg, SVOFFMode.reg
AddReg             = Copper.reg, Copper1000.reg, Autoneg10100.reg
AddReg             = AcDcLink.reg
AddReg             = Powermgmt.reg, WakeOnSlot.reg
AddReg             = Sips.reg
AddReg             = Po.reg
AddReg             = EEE.reg
AddReg             = enableK1.reg
AddReg             = UninstallW2.reg
AddReg             = CoInKS.reg
AddReg             = NDISVlanId.reg
CopyFiles          = winblue.CopyFiles, MessageDll.CopyFiles
*IfType            = 6    ; IF_TYPE_ETHERNET_CSMACD
*MediaType         = 0    ; NdisMedium802_3
*PhysicalMediaType = 14 ; NdisPhysicalMedium802_3

[I217.Services]
AddService = e1dexpress, 2, winblue.Service, winblue.EventLog

[I217.HW]
Include            = pci.inf
Needs              = PciIoSpaceNotRequired.HW
AddReg             = MSI.reg

;-------------------------------------------------------------------------------

; Intel(R) Ethernet Connection I218-LM

; Intel(R) Ethernet Connection (3) I218-LM

; Intel(R) Ethernet Connection I219-LM

; Intel(R) Ethernet Connection (2) I219-LM

; Intel(R) Ethernet Connection (3) I219-LM

; Intel(R) Ethernet Connection (4) I219-LM

; Intel(R) Ethernet Connection (5) I219-LM

; Intel(R) Ethernet Connection (6) I219-LM

; Intel(R) Ethernet Connection (7) I219-LM

; Intel(R) Ethernet Connection (8) I219-LM

; Intel(R) Ethernet Connection (9) I219-LM

; Intel(R) Ethernet Connection (10) I219-LM

; Intel(R) Ethernet Connection (11) I219-LM

; Intel(R) Ethernet Connection (12) I219-LM

; Intel(R) Ethernet Connection (13) I219-LM

; Intel(R) Ethernet Connection (14) I219-LM

; Intel(R) Ethernet Connection (15) I219-LM

; Intel(R) Ethernet Connection (16) I219-LM

; Intel(R) Ethernet Connection (17) I219-LM

; Intel(R) Ethernet Connection (19) I219-LM

; Intel(R) Ethernet Connection (22) I219-LM

; Intel(R) Ethernet Connection (23) I219-LM

; Intel(R) Ethernet Connection (26) I219-LM
;-------------------------------------------------------------------------------
[I219]
Characteristics    = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType            = 5    ; PCI
DelReg             = Advanced.DelReg
AddReg             = e1d.reg, TcpSeg.reg, JumboPacket.reg, SVOFFMode.reg
AddReg             = Copper.reg, Copper1000.reg, Autoneg10100.reg
AddReg             = AcDcLink.reg
AddReg             = Powermgmt.reg, WakeOnSlot.reg
AddReg             = Sips.reg
AddReg             = Po.reg
AddReg             = EEE.reg
AddReg             = ulp.reg
AddReg             = enableK1.reg
AddReg             = UninstallW2.reg
AddReg             = CoInKS.reg
AddReg             = NDISVlanId.reg
CopyFiles          = winblue.CopyFiles, MessageDll.CopyFiles
*IfType            = 6    ; IF_TYPE_ETHERNET_CSMACD
*MediaType         = 0    ; NdisMedium802_3
*PhysicalMediaType = 14 ; NdisPhysicalMedium802_3

[I219.Services]
AddService = e1dexpress, 2, winblue.Service, winblue.EventLog

[I219.HW]
Include            = pci.inf
Needs              = PciIoSpaceNotRequired.HW
AddReg             = MSI.reg

;-------------------------------------------------------------------------------

; Intel(R) Ethernet Connection (18) I219-LM

; Intel(R) Ethernet Connection (20) I219-LM

; Intel(R) Ethernet Connection (24) I219-LM

; Intel(R) Ethernet Connection (25) I219-LM

; Intel(R) Ethernet Connection (27) I219-LM
;-------------------------------------------------------------------------------
[I219_NOK1]
Characteristics    = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType            = 5    ; PCI
DelReg             = Advanced.DelReg
AddReg             = e1d.reg, TcpSeg.reg, JumboPacket.reg, SVOFFMode.reg
AddReg             = Copper.reg, Copper1000.reg, Autoneg10100.reg
AddReg             = AcDcLink.reg
AddReg             = Powermgmt.reg, WakeOnSlot.reg
AddReg             = Sips.reg
AddReg             = Po.reg
AddReg             = EEE.reg
AddReg             = ulp.reg
AddReg             = disableK1.reg
AddReg             = UninstallW2.reg
AddReg             = CoInKS.reg
AddReg             = NDISVlanId.reg
CopyFiles          = winblue.CopyFiles, MessageDll.CopyFiles
*IfType            = 6    ; IF_TYPE_ETHERNET_CSMACD
*MediaType         = 0    ; NdisMedium802_3
*PhysicalMediaType = 14 ; NdisPhysicalMedium802_3

[I219_NOK1.Services]
AddService = e1dexpress, 2, winblue.Service, winblue.EventLog

[I219_NOK1.HW]
Include            = pci.inf
Needs              = PciIoSpaceNotRequired.HW
AddReg             = MSI.reg
    
        
    
    

;===============================================================================
;

;                WINDOWS Server 2022 for 64-bit EXTENDED PLATFORMS

;
;===============================================================================

;-------------------------------------------------------------------------------

; Intel(R) Ethernet Connection I217-LM

; Intel(R) Ethernet Connection I217-V

; Intel(R) Ethernet Connection (2) I218-LM

; Intel(R) Ethernet Connection (2) I218-V
;-------------------------------------------------------------------------------
[I217.19H1]
Characteristics    = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType            = 5    ; PCI
DelReg             = Advanced.DelReg
AddReg             = e1d.reg, TcpSeg.reg, JumboPacket.reg, SVOFFMode.reg
AddReg             = Copper.reg, Copper1000.reg, Autoneg10100.reg
AddReg             = AcDcLink.reg
AddReg             = Powermgmt.reg, WakeOnSlot.reg
AddReg             = Sips.reg
AddReg             = Po.reg
AddReg             = EEE.reg
AddReg             = enableK1.reg
AddReg             = UninstallW2.reg
AddReg             = CoInKS.reg
AddReg             = NDISVlanId.reg
AddReg             = PtpHardwareTimestamp.reg
AddReg             = SoftwareTimestamp.reg
CopyFiles          = winblue.CopyFiles, MessageDll.CopyFiles
*IfType            = 6    ; IF_TYPE_ETHERNET_CSMACD
*MediaType         = 0    ; NdisMedium802_3
*PhysicalMediaType = 14 ; NdisPhysicalMedium802_3

[I217.19H1.Services]
AddService = e1dexpress, 2, winblue.Service, winblue.EventLog

[I217.19H1.HW]
Include            = pci.inf
Needs              = PciIoSpaceNotRequired.HW
AddReg             = MSI.reg

;-------------------------------------------------------------------------------

; Intel(R) Ethernet Connection I218-LM

; Intel(R) Ethernet Connection (3) I218-LM

; Intel(R) Ethernet Connection I219-LM

; Intel(R) Ethernet Connection (2) I219-LM

; Intel(R) Ethernet Connection (3) I219-LM

; Intel(R) Ethernet Connection (4) I219-LM

; Intel(R) Ethernet Connection (5) I219-LM

; Intel(R) Ethernet Connection (6) I219-LM

; Intel(R) Ethernet Connection (7) I219-LM

; Intel(R) Ethernet Connection (8) I219-LM

; Intel(R) Ethernet Connection (9) I219-LM

; Intel(R) Ethernet Connection (10) I219-LM

; Intel(R) Ethernet Connection (11) I219-LM

; Intel(R) Ethernet Connection (12) I219-LM

; Intel(R) Ethernet Connection (13) I219-LM

; Intel(R) Ethernet Connection (14) I219-LM

; Intel(R) Ethernet Connection (15) I219-LM

; Intel(R) Ethernet Connection (16) I219-LM

; Intel(R) Ethernet Connection (17) I219-LM

; Intel(R) Ethernet Connection (19) I219-LM

; Intel(R) Ethernet Connection (22) I219-LM

; Intel(R) Ethernet Connection (23) I219-LM

; Intel(R) Ethernet Connection (26) I219-LM
;-------------------------------------------------------------------------------
[I219.19H1]
Characteristics    = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType            = 5    ; PCI
DelReg             = Advanced.DelReg
AddReg             = e1d.reg, TcpSeg.reg, JumboPacket.reg, SVOFFMode.reg
AddReg             = Copper.reg, Copper1000.reg, Autoneg10100.reg
AddReg             = AcDcLink.reg
AddReg             = Powermgmt.reg, WakeOnSlot.reg
AddReg             = Sips.reg
AddReg             = Po.reg
AddReg             = EEE.reg
AddReg             = ulp.reg
AddReg             = enableK1.reg
AddReg             = UninstallW2.reg
AddReg             = CoInKS.reg
AddReg             = NDISVlanId.reg
AddReg             = PtpHardwareTimestamp.reg
AddReg             = SoftwareTimestamp.reg
CopyFiles          = winblue.CopyFiles, MessageDll.CopyFiles
*IfType            = 6    ; IF_TYPE_ETHERNET_CSMACD
*MediaType         = 0    ; NdisMedium802_3
*PhysicalMediaType = 14 ; NdisPhysicalMedium802_3

[I219.19H1.Services]
AddService = e1dexpress, 2, winblue.Service, winblue.EventLog

[I219.19H1.HW]
Include            = pci.inf
Needs              = PciIoSpaceNotRequired.HW
AddReg             = MSI.reg

;-------------------------------------------------------------------------------

; Intel(R) Ethernet Connection (18) I219-LM

; Intel(R) Ethernet Connection (20) I219-LM

; Intel(R) Ethernet Connection (24) I219-LM

; Intel(R) Ethernet Connection (25) I219-LM

; Intel(R) Ethernet Connection (27) I219-LM
;-------------------------------------------------------------------------------
[I219_NOK1.19H1]
Characteristics    = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType            = 5    ; PCI
DelReg             = Advanced.DelReg
AddReg             = e1d.reg, TcpSeg.reg, JumboPacket.reg, SVOFFMode.reg
AddReg             = Copper.reg, Copper1000.reg, Autoneg10100.reg
AddReg             = AcDcLink.reg
AddReg             = Powermgmt.reg, WakeOnSlot.reg
AddReg             = Sips.reg
AddReg             = Po.reg
AddReg             = EEE.reg
AddReg             = ulp.reg
AddReg             = disableK1.reg
AddReg             = UninstallW2.reg
AddReg             = CoInKS.reg
AddReg             = NDISVlanId.reg
AddReg             = PtpHardwareTimestamp.reg
AddReg             = SoftwareTimestamp.reg
CopyFiles          = winblue.CopyFiles, MessageDll.CopyFiles
*IfType            = 6    ; IF_TYPE_ETHERNET_CSMACD
*MediaType         = 0    ; NdisMedium802_3
*PhysicalMediaType = 14 ; NdisPhysicalMedium802_3

[I219_NOK1.19H1.Services]
AddService = e1dexpress, 2, winblue.Service, winblue.EventLog

[I219_NOK1.19H1.HW]
Include            = pci.inf
Needs              = PciIoSpaceNotRequired.HW
AddReg             = MSI.reg

;-------------------------------------------------------------------------------
; Registry Settings (decimal)
;
[e1d.reg]
HKR, Ndi\Interfaces,                                    UpperRange,             0, "ndis5"
HKR, Ndi\Interfaces,                                    LowerRange,             0, "ethernet"
HKR, Ndi,                                               Service,                0, "e1dexpress"

; *FlowControl
HKR, Ndi\Params\*FlowControl,                           ParamDesc,              0, %FlowControl%
HKR, Ndi\Params\*FlowControl,                           default,                0, "4"
HKR, Ndi\Params\*FlowControl\Enum,                      "0",                    0, %Disabled%
HKR, Ndi\Params\*FlowControl\Enum,                      "1",                    0, %FlowControl_TxOnly%
HKR, Ndi\Params\*FlowControl\Enum,                      "2",                    0, %FlowControl_RxOnly%
HKR, Ndi\Params\*FlowControl\Enum,                      "3",                    0, %FlowControl_Full%
HKR, Ndi\Params\*FlowControl\Enum,                      "4",                    0, %AutoNegotiation%
HKR, Ndi\Params\*FlowControl,                           type,                   0, "enum"

; *TransmitBuffers
HKR, Ndi\params\*TransmitBuffers,                       ParamDesc,              0, %TransmitBuffers%
HKR, Ndi\params\*TransmitBuffers,                       default,                0, "512"
HKR, Ndi\params\*TransmitBuffers,                       min,                    0, "80"
HKR, Ndi\params\*TransmitBuffers,                       max,                    0, "16384"
HKR, Ndi\params\*TransmitBuffers,                       step,                   0, "8"
HKR, Ndi\params\*TransmitBuffers,                       Base,                   0, "10"
HKR, Ndi\params\*TransmitBuffers,                       type,                   0, "int"

; *ReceiveBuffers
HKR, Ndi\params\*ReceiveBuffers,                        ParamDesc,              0, %ReceiveBuffers%
HKR, Ndi\params\*ReceiveBuffers,                        default,                0, "256"
HKR, Ndi\params\*ReceiveBuffers,                        min,                    0, "80"
HKR, Ndi\params\*ReceiveBuffers,                        max,                    0, "16384"
HKR, Ndi\params\*ReceiveBuffers,                        step,                   0, "8"
HKR, Ndi\params\*ReceiveBuffers,                        Base,                   0, "10"
HKR, Ndi\params\*ReceiveBuffers,                        type,                   0, "int"

; *TCPChecksumOffloadIPv4
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,                ParamDesc,              0, %TCPChksumOffv4%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,                default,                0, "3"
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\Enum,           "0",                    0, %Disabled%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\Enum,           "1",                    0, %ChksumOffTx%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\Enum,           "2",                    0, %ChksumOffRx%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\Enum,           "3",                    0, %ChksumOffTxRx%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,                type,                   0, "enum"

; *TCPChecksumOffloadIPv6
HKR, Ndi\Params\*TCPChecksumOffloadIPv6,                ParamDesc,              0, %TCPChksumOffv6%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6,                default,                0, "3"
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\Enum,           "0",                    0, %Disabled%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\Enum,           "1",                    0, %ChksumOffTx%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\Enum,           "2",                    0, %ChksumOffRx%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\Enum,           "3",                    0, %ChksumOffTxRx%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6,                type,                   0, "enum"

; *UDPChecksumOffloadIPv4
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,                ParamDesc,              0, %UDPChksumOffv4%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,                default,                0, "3"
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\Enum,           "0",                    0, %Disabled%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\Enum,           "1",                    0, %ChksumOffTx%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\Enum,           "2",                    0, %ChksumOffRx%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\Enum,           "3",                    0, %ChksumOffTxRx%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,                type,                   0, "enum"

; *UDPChecksumOffloadIPv6
HKR, Ndi\Params\*UDPChecksumOffloadIPv6,                ParamDesc,              0, %UDPChksumOffv6%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6,                default,                0, "3"
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\Enum,           "0",                    0, %Disabled%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\Enum,           "1",                    0, %ChksumOffTx%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\Enum,           "2",                    0, %ChksumOffRx%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\Enum,           "3",                    0, %ChksumOffTxRx%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6,                type,                   0, "enum"

; *IPChecksumOffloadIPv4
HKR, Ndi\Params\*IPChecksumOffloadIPv4,                 ParamDesc,              0, %IPChksumOffv4%
HKR, Ndi\Params\*IPChecksumOffloadIPv4,                 default,                0, "3"
HKR, Ndi\Params\*IPChecksumOffloadIPv4\Enum,            "0",                    0, %Disabled%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\Enum,            "1",                    0, %ChksumOffTx%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\Enum,            "2",                    0, %ChksumOffRx%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\Enum,            "3",                    0, %ChksumOffTxRx%
HKR, Ndi\Params\*IPChecksumOffloadIPv4,                 type,                   0, "enum"

; Network Address
HKR, Ndi\params\NetworkAddress,                         ParamDesc,              0, %LAA%
HKR, Ndi\params\NetworkAddress,                         Default,                0, ""
HKR, Ndi\params\NetworkAddress,                         type,                   0, "edit"
HKR, NDI\params\NetworkAddress,                         LimitText,              0, "12"
HKR, NDI\params\NetworkAddress,                         UpperCase,              0, "1"
HKR, NDI\params\NetworkAddress,                         optional,               0, "1"

;Log Link State Event
HKR,Ndi\Params\LogLinkStateEvent,                       ParamDesc,              0, %LogLinkState%
HKR,Ndi\Params\LogLinkStateEvent,                       Type,                   0, "enum"
HKR,Ndi\Params\LogLinkStateEvent,                       Default,                0, "51"
HKR,Ndi\Params\LogLinkStateEvent\Enum,                  "51",                   0, %Enabled%
HKR,Ndi\Params\LogLinkStateEvent\Enum,                  "16",                   0, %Disabled%
HKR,,                                                   LogLinkStateEvent,      0, "51"

; Wait for Link
HKR, Ndi\Params\WaitAutoNegComplete,                    ParamDesc,              0, %WaitAutoNegComplete%
HKR, Ndi\Params\WaitAutoNegComplete,                    default,                0, "2"
HKR, Ndi\Params\WaitAutoNegComplete\Enum,               "0",                    0, %Off%
HKR, Ndi\Params\WaitAutoNegComplete\Enum,               "1",                    0, %On%
HKR, Ndi\Params\WaitAutoNegComplete\Enum,               "2",                    0, %AutoDetect%
HKR, Ndi\Params\WaitAutoNegComplete,                    type,                   0, "enum"

;  Interrupt Throttle Rate
HKR, Ndi\Params\ITR,                                    ParamDesc,              0, %InterruptThrottleRate%
HKR, Ndi\Params\ITR,                                    default,                0, "65535"
HKR, Ndi\Params\ITR\Enum,                               "65535",                0, %Adaptive%
HKR, Ndi\Params\ITR\Enum,                               "3600",                 0, %Extreme%
HKR, Ndi\Params\ITR\Enum,                               "2000",                 0, %High%
HKR, Ndi\Params\ITR\Enum,                               "950",                  0, %Medium%
HKR, Ndi\Params\ITR\Enum,                               "400",                  0, %Low%
HKR, Ndi\Params\ITR\Enum,                               "200",                  0, %Minimal%
HKR, Ndi\Params\ITR\Enum,                               "0",                    0, %Off%
HKR, Ndi\Params\ITR,                                    type,                   0, "enum"
HKR,,                                                   ITR,                    0, "65535"

; *InterruptModeration
HKR, Ndi\Params\*InterruptModeration,                   ParamDesc,              0, %InterruptModeration%
HKR, Ndi\Params\*InterruptModeration,                   default,                0, "1"
HKR, Ndi\Params\*InterruptModeration\Enum,              "0",                    0, %Disabled%
HKR, Ndi\Params\*InterruptModeration\Enum,              "1",                    0, %Enabled%
HKR, Ndi\Params\*InterruptModeration,                   type,                   0, "enum"

; *PriorityVLANTag
HKR, Ndi\Params\*PriorityVLANTag,                       ParamDesc,              0, %PriorityVLANTag2%
HKR, Ndi\Params\*PriorityVLANTag,                       default,                0, "3"
HKR, Ndi\Params\*PriorityVLANTag\Enum,                  "0",                    0, %PriorityVlanDisabled2%
HKR, Ndi\Params\*PriorityVLANTag\Enum,                  "1",                    0, %PriorityEnabled2%
HKR, Ndi\Params\*PriorityVLANTag\Enum,                  "2",                    0, %VlanEnabled%
HKR, Ndi\Params\*PriorityVLANTag\Enum,                  "3",                    0, %PriorityVlanEnabled2%
HKR, Ndi\Params\*PriorityVLANTag,                       type,                   0, "enum"

; ReduceSpeedOnPowerDown
HKR,Ndi\Params\ReduceSpeedOnPowerDown,                  ParamDesc,              0, %ReduceSpeedOnPowerDown%
HKR,Ndi\Params\ReduceSpeedOnPowerDown,                  Type,                   0, "enum"
HKR,Ndi\Params\ReduceSpeedOnPowerDown,                  Default,                0, "1"
HKR,Ndi\Params\ReduceSpeedOnPowerDown\Enum,             "1",                    0, %Enabled%
HKR,Ndi\Params\ReduceSpeedOnPowerDown\Enum,             "0",                    0, %Disabled%

; EnablePME
HKR,Ndi\Params\EnablePME,                               ParamDesc,              0, %Enable_PME%
HKR,Ndi\Params\EnablePME,                               Type,                   0, "enum"
HKR,Ndi\Params\EnablePME,                               Default,                0, "1"
HKR,Ndi\Params\EnablePME\Enum,                          "1",                    0, %Enabled%
HKR,Ndi\Params\EnablePME\Enum,                          "0",                    0, %Disabled%

; Hardwired defaults
HKR,,                                                   PciScanMethod,          0, "3"
HKR,,                                                   TxIntDelay,             0, "28"
HKR,,                                                   MulticastFilterType,    0, "0"
HKR,,                                                   VlanFiltering,          0, "0"
HKR,,                                                   UniversalInstall,       0x00010001, 1

; temporary workaround for MSI. NDIS blocks registration
HKR,,                                                   EnableMSI,              0x00010001, "1"

; Advanced Power Consumption Features
HKR,,                                                   AutoPowerSaveModeEnabled, 0, "0"
HKR,,                                                   ProcessLSCinWorkItem,     0, "1"
HKR,,                                                   Enable9KJFTpt,            0, "1"

; RSS - Hash Only Mode
HKR,,                                                   ReceiveScalingMode,     2, "1"

[ulp.reg]
; ULP Mode
HKR,Ndi\Params\ULPMode,                                 ParamDesc,              0, %UltraLowPowerMode%
HKR,Ndi\Params\ULPMode,                                 Type,                   0, "enum"
HKR,Ndi\Params\ULPMode,                                 Default,                0, "1"
HKR,Ndi\Params\ULPMode\Enum,                            "1",                    0, %Enabled%
HKR,Ndi\Params\ULPMode\Enum,                            "0",                    0, %Disabled%

; Allow host driver to force exit ULP on ME systems
HKR,,                                                   ForceHostExitUlp,       0, "1"

[enableK1.reg]
; EnableK1
HKR,Ndi\Params\EnableK1,                                ParamDesc,              0, %EnableK1%
HKR,Ndi\Params\EnableK1,                                Type,                   0, "enum"
HKR,Ndi\Params\EnableK1,                                Default,                0, "1"
HKR,Ndi\Params\EnableK1\Enum,                           "1",                    0, %Enabled%
HKR,Ndi\Params\EnableK1\Enum,                           "0",                    0, %Disabled%

[disableK1.reg]
; Disable K1 by default for specific devices
HKR,Ndi\Params\EnableK1,                                ParamDesc,              0, %EnableK1%
HKR,Ndi\Params\EnableK1,                                Type,                   0, "enum"
HKR,Ndi\Params\EnableK1,                                Default,                0, "0"
HKR,Ndi\Params\EnableK1\Enum,                           "1",                    0, %Enabled%
HKR,Ndi\Params\EnableK1\Enum,                           "0",                    0, %Disabled%

[NDISVlanId.reg]
; VlanId
HKR, Ndi\params\VlanId,     ParamDesc,       0, %VlanID%
HKR, Ndi\params\VlanId,     default,         0, "0"
HKR, Ndi\params\VlanId,     type,            0, "DWORD"
HKR, Ndi\params\VlanId,     min,             0, "0"
HKR, Ndi\params\VlanId,     max,             0, "4094"
HKR, Ndi\params\VlanId,     step,            0, "1"
HKR, Ndi\params\VlanId,     base,            0, "10"

[IntelANSVlanID.reg]
; Intel ANS Vland ID
HKR,,                                           IntelANSVlanID,          0x00010000, ""

; *PtpHardwareTimestamp
[PtpHardwareTimestamp.reg]
HKR, Ndi\Params\*PtpHardwareTimestamp,                  ParamDesc,              0, %PtpHardwareTimestamp%
HKR, Ndi\Params\*PtpHardwareTimestamp,                  default,                0, "0"
HKR, Ndi\Params\*PtpHardwareTimestamp\Enum,             "0",                    0, %Disabled%
HKR, Ndi\Params\*PtpHardwareTimestamp\Enum,             "1",                    0, %Enabled%
HKR, Ndi\Params\*PtpHardwareTimestamp,                  type,                   0, "enum"

[SoftwareTimestamp.reg]
HKR, Ndi\params\*SoftwareTimestamp,                     ParamDesc,              0, %SoftwareTimestamp%
HKR, Ndi\params\*SoftwareTimestamp,                     default,                0, "0"
HKR, Ndi\params\*SoftwareTimestamp,                     type,                   0, "enum"
HKR, Ndi\params\*SoftwareTimestamp\enum,                "0",                    0, %Disabled%
HKR, Ndi\params\*SoftwareTimestamp\enum,                "1",                    0, %SoftwareTimestampRxAll%
HKR, Ndi\params\*SoftwareTimestamp\enum,                "2",                    0, %SoftwareTimestampTxAll%
HKR, Ndi\params\*SoftwareTimestamp\enum,                "3",                    0, %SoftwareTimestampRxAllTxAll%
HKR, Ndi\params\*SoftwareTimestamp\enum,                "4",                    0, %SoftwareTimestampTaggedTx%
HKR, Ndi\params\*SoftwareTimestamp\enum,                "5",                    0, %SoftwareTimestampRxAllTaggedTx%

[TcpSeg.reg]
; *LsoV2IPv4 / *LsoV2IPv6
HKR, Ndi\Params\*LsoV2IPv4,                             ParamDesc,              0, %LsoV2IPv4%
HKR, Ndi\Params\*LsoV2IPv4,                             default,                0, "1"
HKR, Ndi\Params\*LsoV2IPv4\Enum,                        "0",                    0, %Disabled%
HKR, Ndi\Params\*LsoV2IPv4\Enum,                        "1",                    0, %Enabled%
HKR, Ndi\Params\*LsoV2IPv4,                             type,                   0, "enum"
HKR, Ndi\Params\*LsoV2IPv6,                             ParamDesc,              0, %LsoV2IPv6%
HKR, Ndi\Params\*LsoV2IPv6,                             default,                0, "1"
HKR, Ndi\Params\*LsoV2IPv6\Enum,                        "0",                    0, %Disabled%
HKR, Ndi\Params\*LsoV2IPv6\Enum,                        "1",                    0, %Enabled%
HKR, Ndi\Params\*LsoV2IPv6,                             type,                   0, "enum"
HKR,,                                                   *LsoV1IPv4,             0, "0"

[Copper.reg]
HKR, Ndi\params\*SpeedDuplex,                           ParamDesc,              0, %SpeedDuplex%
HKR, Ndi\params\*SpeedDuplex,                           default,                0, "0"
HKR, Ndi\params\*SpeedDuplex,                           type,                   0, "enum"
HKR, Ndi\params\*SpeedDuplex\enum,                      "0",                    0, %AutoNegotiation%
HKR, Ndi\params\*SpeedDuplex\enum,                      "1",                    0, %10Mb_Half_Duplex%
HKR, Ndi\params\*SpeedDuplex\enum,                      "2",                    0, %10Mb_Full_Duplex%
HKR, Ndi\params\*SpeedDuplex\enum,                      "3",                    0, %100Mb_Half_Duplex%
HKR, Ndi\params\*SpeedDuplex\enum,                      "4",                    0, %100Mb_Full_Duplex%
HKR, PROSetNdi\NdiExt\Params\*SpeedDuplex,              ExposeLevel,            0, "3"

; Adaptive IFS
HKR, Ndi\Params\AdaptiveIFS,                            ParamDesc,              0, %AdaptiveIFS%
HKR, Ndi\Params\AdaptiveIFS,                            default,                0, "0"
HKR, Ndi\Params\AdaptiveIFS,                            type,                   0, "enum"
HKR, Ndi\Params\AdaptiveIFS\Enum,                       "0",                    0, %Disabled%
HKR, Ndi\Params\AdaptiveIFS\Enum,                       "1",                    0, %Enabled%

; Legacy Switch Compatibility Mode
HKR, Ndi\params\LinkNegotiationProcess,                 ParamDesc,              0, %LinkNegotiationProcess%
HKR, Ndi\params\LinkNegotiationProcess,                 default,                0, "1"
HKR, Ndi\params\LinkNegotiationProcess,                 type,                   0, "enum"
HKR, Ndi\params\LinkNegotiationProcess\enum,            "2",                    0, %Enabled%
HKR, Ndi\params\LinkNegotiationProcess\enum,            "1",                    0, %Disabled%
HKR, PROSetNdi\NdiExt\Params\LinkNegotiationProcess,    ExposeLevel,            0, "3"

[Copper1000.reg]
HKR, Ndi\params\*SpeedDuplex\enum,                      "6",                    0, %1000Mb_Full_Duplex%

; Gigabit Master Slave Mode
HKR,Ndi\Params\MasterSlave,                             ParamDesc,              0, %MasterSlaveMode%
HKR,Ndi\Params\MasterSlave,                             Type,                   0, "enum"
HKR,Ndi\Params\MasterSlave,                             Default,                0, "0"
HKR,Ndi\Params\MasterSlave\Enum,                        "0",                    0, %AutoDetect%
HKR,Ndi\Params\MasterSlave\Enum,                        "1",                    0, %GigabitMasterMode%
HKR,Ndi\Params\MasterSlave\Enum,                        "2",                    0, %GigabitSlaveMode%

; Selective advertisement or forced speed
[Autoneg10100.reg]
HKR,,                                                   LinkNegotiationProcess,     0, "1"

; EEE
[EEE.reg]
HKR, Ndi\Params\EEELinkAdvertisement,                   ParamDesc,              0, %EEELinkAdvertisement%
HKR, Ndi\Params\EEELinkAdvertisement,                   type,                   0, "enum"
HKR, Ndi\Params\EEELinkAdvertisement,                   default,                0, "1"
HKR, Ndi\Params\EEELinkAdvertisement\Enum,              "0",                    0, %Off%
HKR, Ndi\Params\EEELinkAdvertisement\Enum,              "1",                    0, %On%

;-------------------------------------------------------------------------------
; Packet specifics
;

; *JumboPacket
[JumboPacket.reg]
HKR, Ndi\Params\*JumboPacket,                           ParamDesc,              0, %JumboPacket%
HKR, Ndi\Params\*JumboPacket,                           default,                0, "1514"
HKR, Ndi\Params\*JumboPacket,                           min,                    0, "1514"
HKR, Ndi\Params\*JumboPacket,                           max,                    0, "9014"
HKR, Ndi\Params\*JumboPacket,                           step,                   0, "1"
HKR, Ndi\Params\*JumboPacket,                           base,                   0, "10"
HKR, Ndi\Params\*JumboPacket,                           type,                   0, "dword"

[Powermgmt.reg]
HKR, Ndi\Params\*WakeOnPattern,                         ParamDesc,              0, %WakeOnPattern%
HKR, Ndi\Params\*WakeOnPattern\Enum,                    "0",                    0, %Disabled%
HKR, Ndi\Params\*WakeOnPattern\Enum,                    "1",                    0, %Enabled%
HKR, Ndi\Params\*WakeOnPattern,                         type,                   0, "enum"
HKR, Ndi\Params\*WakeOnPattern,                         default,                0, "1"
HKR, Ndi\Params\*WakeOnMagicPacket,                     ParamDesc,              0, %WakeOnMagicPacket%
HKR, Ndi\Params\*WakeOnMagicPacket\Enum,                "0",                    0, %Disabled%
HKR, Ndi\Params\*WakeOnMagicPacket\Enum,                "1",                    0, %Enabled%
HKR, Ndi\Params\*WakeOnMagicPacket,                     type,                   0, "enum"
HKR, Ndi\Params\*WakeOnMagicPacket,                     default,                0, "1"
HKR, Ndi\Params\WakeOnLink,                             ParamDesc,              0, %WakeOnLinkSettings%
HKR, Ndi\Params\WakeOnLink\Enum,                        "0",                    0, %Disabled%
HKR, Ndi\Params\WakeOnLink\Enum,                        "2",                    0, %Forced%
HKR, Ndi\Params\WakeOnLink,                             type,                   0, "enum"
HKR, Ndi\Params\WakeOnLink,                             default,                0, "0"

[RTD3.reg]
HKR,,                                                  *DeviceSleepOnDisconnect,          0, "0"

[SelectiveSuspend.reg]
HKR, Ndi\Params\*SelectiveSuspend,                      ParamDesc,              0, %SelectiveSuspend%
HKR, Ndi\Params\*SelectiveSuspend,                      default,                0, "1"
HKR, Ndi\Params\*SelectiveSuspend\Enum,                 "0",                    0, %Disabled%
HKR, Ndi\Params\*SelectiveSuspend\Enum,                 "1",                    0, %Enabled%
HKR, Ndi\Params\*SelectiveSuspend,                      type,                   0, "enum"
HKR, Ndi\params\*SSIdleTimeout,                         ParamDesc,              0, %SSIdleTimeout%
HKR, Ndi\params\*SSIdleTimeout,                         default,                0, "20"
HKR, Ndi\params\*SSIdleTimeout,                         min,                    0, "1"
HKR, Ndi\params\*SSIdleTimeout,                         max,                    0, "60"
HKR, Ndi\params\*SSIdleTimeout,                         step,                   0, "1"
HKR, Ndi\params\*SSIdleTimeout,                         type,                   0, "int"

[ModernStandbyWoLMagicPacket.reg]
HKR, Ndi\Params\*ModernStandbyWoLMagicPacket,           ParamDesc,              0, %ModernStandbyWoLMagicPacket%
HKR, Ndi\Params\*ModernStandbyWoLMagicPacket,           default,                0, "1"
HKR, Ndi\Params\*ModernStandbyWoLMagicPacket\Enum,      "0",                    0, %Disabled%
HKR, Ndi\Params\*ModernStandbyWoLMagicPacket\Enum,      "1",                    0, %Enabled%
HKR, Ndi\Params\*ModernStandbyWoLMagicPacket,           type,                   0, "enum"

[AcDcLink.reg]
HKR, Ndi\Params\AutoPowerSaveModeEnabled,               ParamDesc,              0, %AcDcLinkStep%
HKR, Ndi\Params\AutoPowerSaveModeEnabled,               type,                   0, "enum"
HKR, Ndi\Params\AutoPowerSaveModeEnabled,               default,                0, "1"
HKR, Ndi\Params\AutoPowerSaveModeEnabled\Enum,          "0",                    0, %Disabled%
HKR, Ndi\Params\AutoPowerSaveModeEnabled\Enum,          "1",                    0, %Enabled%

; Sips
[Sips.reg]
HKR, Ndi\Params\SipsEnabled,                            ParamDesc,              0, %SipsEnabled%
HKR, Ndi\Params\SipsEnabled,                            type,                   0, "enum"
HKR, Ndi\Params\SipsEnabled,                            default,                0, "0"
HKR, Ndi\Params\SipsEnabled\Enum,                       "0",                    0, %Disabled%
HKR, Ndi\Params\SipsEnabled\Enum,                       "1",                    0, %Enabled%

; Protocol Offload
[Po.reg]
HKR, Ndi\Params\*PMARPOffload,                          ParamDesc,              0, %PMARPOffload%
HKR, Ndi\Params\*PMARPOffload,                          type,                   0, "enum"
HKR, Ndi\Params\*PMARPOffload,                          default,                0, "1"
HKR, Ndi\Params\*PMARPOffload\Enum,                     "0",                    0, %Disabled%
HKR, Ndi\Params\*PMARPOffload\Enum,                     "1",                    0, %Enabled%
HKR, Ndi\Params\*PMNSOffload,                           ParamDesc,              0, %PMNSOffload%
HKR, Ndi\Params\*PMNSOffload,                           type,                   0, "enum"
HKR, Ndi\Params\*PMNSOffload,                           default,                0, "1"
HKR, Ndi\Params\*PMNSOffload\Enum,                      "0",                    0, %Disabled%
HKR, Ndi\Params\*PMNSOffload\Enum,                      "1",                    0, %Enabled%

;-------------------------------------------------------------------------------
[WakeOnSlot.reg]
HKR,,                                                   WakeOnSlot,             0, 0

[SVOFFMode.reg]
HKR,,                                                   SVOFFMode,              0,  "1"

[MSI.reg]
HKR, "Interrupt Management", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 1
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x00010001, 1

;-------------------------------------------------------------------------------
; Uninstallation
[UninstallW2.reg]
HKR, Prounstl\SupportedDevices\8086, 153A, 0, "153A"
HKR, Prounstl\SupportedDevices\8086, 153B, 0, "153B"
HKR, Prounstl\SupportedDevices\8086, 155A, 0, "155A"
HKR, Prounstl\SupportedDevices\8086, 1559, 0, "1559"
HKR, Prounstl\SupportedDevices\8086, 15A0, 0, "15A0"
HKR, Prounstl\SupportedDevices\8086, 15A1, 0, "15A1"
HKR, Prounstl\SupportedDevices\8086, 15A2, 0, "15A2"
HKR, Prounstl\SupportedDevices\8086, 15A3, 0, "15A3"
HKR, Prounstl\SupportedDevices\8086, 156F, 0, "156F"
HKR, Prounstl\SupportedDevices\8086, 1570, 0, "1570"
HKR, Prounstl\SupportedDevices\8086, 15B7, 0, "15B7"
HKR, Prounstl\SupportedDevices\8086, 15B8, 0, "15B8"
HKR, Prounstl\SupportedDevices\8086, 15B9, 0, "15B9"
HKR, Prounstl\SupportedDevices\8086, 15D7, 0, "15D7"
HKR, Prounstl\SupportedDevices\8086, 15D8, 0, "15D8"
HKR, Prounstl\SupportedDevices\8086, 15E3, 0, "15E3"
HKR, Prounstl\SupportedDevices\8086, 15D6, 0, "15D6"
HKR, Prounstl\SupportedDevices\8086, 15BB, 0, "15BB"
HKR, Prounstl\SupportedDevices\8086, 15BC, 0, "15BC"
HKR, Prounstl\SupportedDevices\8086, 15BD, 0, "15BD"
HKR, Prounstl\SupportedDevices\8086, 15BE, 0, "15BE"
HKR, Prounstl\SupportedDevices\8086, 15DF, 0, "15DF"
HKR, Prounstl\SupportedDevices\8086, 15E0, 0, "15E0"
HKR, Prounstl\SupportedDevices\8086, 15E1, 0, "15E1"
HKR, Prounstl\SupportedDevices\8086, 15E2, 0, "15E2"
HKR, Prounstl\SupportedDevices\8086, 0D4E, 0, "0D4E"
HKR, Prounstl\SupportedDevices\8086, 0D4F, 0, "0D4F"
HKR, Prounstl\SupportedDevices\8086, 0D4C, 0, "0D4C"
HKR, Prounstl\SupportedDevices\8086, 0D4D, 0, "0D4D"
HKR, Prounstl\SupportedDevices\8086, 0D53, 0, "0D53"
HKR, Prounstl\SupportedDevices\8086, 0D55, 0, "0D55"
HKR, Prounstl\SupportedDevices\8086, 15F9, 0, "15F9"
HKR, Prounstl\SupportedDevices\8086, 15FA, 0, "15FA"
HKR, Prounstl\SupportedDevices\8086, 15FB, 0, "15FB"
HKR, Prounstl\SupportedDevices\8086, 15FC, 0, "15FC"
HKR, Prounstl\SupportedDevices\8086, 15F4, 0, "15F4"
HKR, Prounstl\SupportedDevices\8086, 1A1E, 0, "1A1E"
HKR, Prounstl\SupportedDevices\8086, 1A1F, 0, "1A1F"
HKR, Prounstl\SupportedDevices\8086, 1A1C, 0, "1A1C"
HKR, Prounstl\SupportedDevices\8086, 1A1D, 0, "1A1D"
HKR, Prounstl\SupportedDevices\8086, 0DC5, 0, "0DC5"
HKR, Prounstl\SupportedDevices\8086, 0DC6, 0, "0DC6"
HKR, Prounstl\SupportedDevices\8086, 0DC7, 0, "0DC7"
HKR, Prounstl\SupportedDevices\8086, 0DC8, 0, "0DC8"
HKR, Prounstl\SupportedDevices\8086, 550A, 0, "550A"
HKR, Prounstl\SupportedDevices\8086, 550B, 0, "550B"
HKR, Prounstl\SupportedDevices\8086, 550C, 0, "550C"
HKR, Prounstl\SupportedDevices\8086, 550D, 0, "550D"
HKR, Prounstl\SupportedDevices\8086, 57A0, 0, "57A0"
HKR, Prounstl\SupportedDevices\8086, 57A1, 0, "57A1"
HKR, Prounstl\SupportedDevices\8086, 550E, 0, "550E"
HKR, Prounstl\SupportedDevices\8086, 550F, 0, "550F"
HKR, Prounstl\SupportedDevices\8086, 57B3, 0, "57B3"
HKR, Prounstl\SupportedDevices\8086, 57B4, 0, "57B4"
HKR, Prounstl\SupportedDevices\8086, 57B5, 0, "57B5"
HKR, Prounstl\SupportedDevices\8086, 57B6, 0, "57B6"
HKR, Prounstl\SupportedDevices\8086, 57B7, 0, "57B7"
HKR, Prounstl\SupportedDevices\8086, 57B8, 0, "57B8"
HKR, Prounstl\Services, e1dexpress, 0, "e1d.sys"

;-------------------------------------------------------------------------------
; WinVista copy files
;

[winblue.CopyFiles]
e1d.sys,,,2

[winblue.Service]
DisplayName     = %e1dExpress.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %13%\e1d.sys
LoadOrderGroup  = NDIS
AddReg             = Service_AddReg
AddReg             = DmaRemapping.reg

[Service_AddReg]
HKR, Parameters, BootFlags, 0x00010001, 0x1

[DMARemapping.reg]
HKR, Parameters, DmaRemappingCompatible, 0x00010001, 2

;-------------------------------------------------------------------------------
; Common base for all drivers for Eventlog and TextModeFlags
;

[winblue.EventLog]
AddReg             = winblue.AddEventLog.reg

[winblue.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll;%13%\e1dmsg.dll"
HKR, , TypesSupported,   0x00010001, 7

[MessageDll.CopyFiles]
e1dmsg.dll

[CoInKS.reg]
HKR,,                                          CoInstallFlag,      0x00010001, 0x08203101

;-------------------------------------------------------------------------------
; DestinationDirs
;
[DestinationDirs]
DefaultDestDir                = 13
winblue.CopyFiles          = 13
MessageDll.CopyFiles          = 13

[SourceDisksNames]
;
; diskid = description[, [tagfile] [, <unused>,subdir]]
;
1 = %DISKNAME%,,,

[SourceDisksFiles]
;
; filename_on_source = diskID[, [subdir][, size]]
;
e1dmsg.dll   = 1,,
e1d.sys = 1,, ; on distribution disk 1

;-------------------------------------------------------------------------------
; Legacy
[Advanced.DelReg]
HKR, Ndi\Params
HKR, PROSetNdi\Params
HKR, PROSetNdi\NdiExt

;-----------------------------------------------------------------------------
; Localizable Strings

[Strings]
AutoDetect                      = "Auto Detect"
AutoNegotiation                 = "Auto Negotiation"
SpeedDuplex                     = "Speed & Duplex"
10Mb_Half_Duplex                = "10 Mbps Half Duplex"
10Mb_Full_Duplex                = "10 Mbps Full Duplex"
100Mb_Half_Duplex               = "100 Mbps Half Duplex"
100Mb_Full_Duplex               = "100 Mbps Full Duplex"
1000Mb_Full_Duplex              = "1.0 Gbps Full Duplex"
LinkNegotiationProcess          = "Legacy Switch Compatibility Mode"
IPChksumOffv4                   = "IPv4 Checksum Offload"
TCPChksumOffv4                  = "TCP Checksum Offload (IPv4)"
UDPChksumOffv4                  = "UDP Checksum Offload (IPv4)"
TCPChksumOffv6                  = "TCP Checksum Offload (IPv6)"
UDPChksumOffv6                  = "UDP Checksum Offload (IPv6)"
SipsEnabled                     = "System Idle Power Saver"
PMARPOffload                    = "Protocol ARP Offload"
PMNSOffload                     = "Protocol NS Offload"
LsoV2IPv4                       = "Large Send Offload V2 (IPv4)"
LsoV2IPv6                       = "Large Send Offload V2 (IPv6)"
ChksumOffTxRx                   = "Rx & Tx Enabled"
ChksumOffTx                     = "Tx Enabled"
ChksumOffRx                     = "Rx Enabled"
FlowControl                     = "Flow Control"
FlowControl_TxOnly              = "Tx Enabled"
FlowControl_RxOnly              = "Rx Enabled"
FlowControl_Full                = "Rx & Tx Enabled"
PriorityVlanDisabled2           = "Packet Priority & VLAN Disabled"
PriorityEnabled2                = "Packet Priority Enabled"
VlanEnabled                     = "VLAN Enabled"
PriorityVlanEnabled2            = "Packet Priority & VLAN Enabled"
TransmitBuffers                 = "Transmit Buffers"
ReceiveBuffers                  = "Receive Buffers"
PriorityVLANTag2                = "Packet Priority & VLAN"
On                              = "On"
Off                             = "Off"
Enabled                         = "Enabled"
Disabled                        = "Disabled"
LAA                             = "Locally Administered Address"
JumboPacket                     = "Jumbo Packet"
AdaptiveIFS                     = "Adaptive Inter-Frame Spacing"
AcDcLinkStep                    = "Link Speed Battery Saver"
WakeOnMagicPacket               = "Wake on Magic Packet"
Enable_PME                      = "Enable PME"
Forced                          = "Forced"
WakeOnLinkSettings              = "Wake on Link Settings"
WakeOnPattern                   = "Wake on Pattern Match"
LogLinkState                    = "Log Link State Event"
InterruptModeration             = "Interrupt Moderation"
InterruptThrottleRate           = "Interrupt Moderation Rate"
Adaptive                        = "Adaptive"
Extreme                         = "Extreme"
Minimal                         = "Minimal"
High                            = "High"
Medium                          = "Medium"
Low                             = "Low"
GigabitMasterMode               = "Force Master Mode"
GigabitSlaveMode                = "Force Slave Mode"
MasterSlaveMode                 = "Gigabit Master Slave Mode"
WaitAutoNegComplete             = "Wait for Link"
EEELinkAdvertisement            = "Energy Efficient Ethernet"
ReduceSpeedOnPowerDown          = "Reduce Speed On Power Down"
VlanID                          = "VLAN ID"
SelectiveSuspend                = "Selective Suspend"
SSIdleTimeout                   = "Selective Suspend Idle Timeout"
ModernStandbyWoLMagicPacket     = "Wake from S0ix on Magic Packet"
UltraLowPowerMode               = "Ultra Low Power Mode"
EnableK1                        = "PCI Express Link Power Saving"
PtpHardwareTimestamp            = "PTP Hardware Timestamp"
SoftwareTimestamp               = "Software Timestamp"
SoftwareTimestampRxAll          = "RxAll"
SoftwareTimestampTxAll          = "TxAll"
SoftwareTimestampRxAllTxAll     = "RxAll & TxAll"
SoftwareTimestampTaggedTx       = "TaggedTx"
SoftwareTimestampRxAllTaggedTx  = "RxAll & TaggedTx"
Intel                           = "Intel"
e1dExpress.Service.DispName     = "Intel(R) PRO/1000 PCI Express Network Connection Driver D"
DISKNAME                        = "Intel(R) PRO/1000 Driver Disk"

;; Brandnames.str
;------------------------------------------------------------------------------
E153ANC.DeviceDesc              = "Intel(R) Ethernet Connection I217-LM"
E153BNC.DeviceDesc              = "Intel(R) Ethernet Connection I217-V"
E155ANC.DeviceDesc              = "Intel(R) Ethernet Connection I218-LM"
E1559NC.DeviceDesc              = "Intel(R) Ethernet Connection I218-V"
E15A0NC.DeviceDesc              = "Intel(R) Ethernet Connection (2) I218-LM"
E15A1NC.DeviceDesc              = "Intel(R) Ethernet Connection (2) I218-V"
E15A2NC.DeviceDesc              = "Intel(R) Ethernet Connection (3) I218-LM"
E15A3NC.DeviceDesc              = "Intel(R) Ethernet Connection (3) I218-V"
E156FNC.DeviceDesc              = "Intel(R) Ethernet Connection I219-LM"
E1570NC.DeviceDesc              = "Intel(R) Ethernet Connection I219-V"
E15B7NC.DeviceDesc              = "Intel(R) Ethernet Connection (2) I219-LM"
E15B8NC.DeviceDesc              = "Intel(R) Ethernet Connection (2) I219-V"
E15B9NC.DeviceDesc              = "Intel(R) Ethernet Connection (3) I219-LM"
E15D7NC.DeviceDesc              = "Intel(R) Ethernet Connection (4) I219-LM"
E15D8NC.DeviceDesc              = "Intel(R) Ethernet Connection (4) I219-V"
E15E3NC.DeviceDesc              = "Intel(R) Ethernet Connection (5) I219-LM"
E15D6NC.DeviceDesc              = "Intel(R) Ethernet Connection (5) I219-V"
E15BDNC.DeviceDesc              = "Intel(R) Ethernet Connection (6) I219-LM"
E15BENC.DeviceDesc              = "Intel(R) Ethernet Connection (6) I219-V"
E15BBNC.DeviceDesc              = "Intel(R) Ethernet Connection (7) I219-LM"
E15BCNC.DeviceDesc              = "Intel(R) Ethernet Connection (7) I219-V"
E15DFNC.DeviceDesc              = "Intel(R) Ethernet Connection (8) I219-LM"
E15E0NC.DeviceDesc              = "Intel(R) Ethernet Connection (8) I219-V"
E15E1NC.DeviceDesc              = "Intel(R) Ethernet Connection (9) I219-LM"
E15E2NC.DeviceDesc              = "Intel(R) Ethernet Connection (9) I219-V"
E0D4ENC.DeviceDesc              = "Intel(R) Ethernet Connection (10) I219-LM"
E0D4FNC.DeviceDesc              = "Intel(R) Ethernet Connection (10) I219-V"
E0D4CNC.DeviceDesc              = "Intel(R) Ethernet Connection (11) I219-LM"
E0D4DNC.DeviceDesc              = "Intel(R) Ethernet Connection (11) I219-V"
E0D53NC.DeviceDesc              = "Intel(R) Ethernet Connection (12) I219-LM"
E0D55NC.DeviceDesc              = "Intel(R) Ethernet Connection (12) I219-V"
E15FBNC.DeviceDesc              = "Intel(R) Ethernet Connection (13) I219-LM"
E15FCNC.DeviceDesc              = "Intel(R) Ethernet Connection (13) I219-V"
E15F9NC.DeviceDesc              = "Intel(R) Ethernet Connection (14) I219-LM"
E15FANC.DeviceDesc              = "Intel(R) Ethernet Connection (14) I219-V"
E15F4NC.DeviceDesc              = "Intel(R) Ethernet Connection (15) I219-LM"
E1A1ENC.DeviceDesc              = "Intel(R) Ethernet Connection (16) I219-LM"
E1A1FNC.DeviceDesc              = "Intel(R) Ethernet Connection (16) I219-V"
E1A1CNC.DeviceDesc              = "Intel(R) Ethernet Connection (17) I219-LM"
E1A1DNC.DeviceDesc              = "Intel(R) Ethernet Connection (17) I219-V"
E0DC7NC.DeviceDesc              = "Intel(R) Ethernet Connection (22) I219-LM"
E0DC8NC.DeviceDesc              = "Intel(R) Ethernet Connection (22) I219-V"
E0DC5NC.DeviceDesc              = "Intel(R) Ethernet Connection (23) I219-LM"
E0DC6NC.DeviceDesc              = "Intel(R) Ethernet Connection (23) I219-V"
E550ANC.DeviceDesc              = "Intel(R) Ethernet Connection (18) I219-LM"
E550BNC.DeviceDesc              = "Intel(R) Ethernet Connection (18) I219-V"
E550CNC.DeviceDesc              = "Intel(R) Ethernet Connection (19) I219-LM"
E550DNC.DeviceDesc              = "Intel(R) Ethernet Connection (19) I219-V"
E57A0NC.DeviceDesc              = "Intel(R) Ethernet Connection (24) I219-LM"
E57A1NC.DeviceDesc              = "Intel(R) Ethernet Connection (24) I219-V"
E550ENC.DeviceDesc              = "Intel(R) Ethernet Connection (20) I219-LM"
E550FNC.DeviceDesc              = "Intel(R) Ethernet Connection (20) I219-V"
E57B3NC.DeviceDesc              = "Intel(R) Ethernet Connection (25) I219-LM"
E57B4NC.DeviceDesc              = "Intel(R) Ethernet Connection (25) I219-V"
E57B5NC.DeviceDesc              = "Intel(R) Ethernet Connection (26) I219-LM"
E57B6NC.DeviceDesc              = "Intel(R) Ethernet Connection (26) I219-V"
E57B7NC.DeviceDesc              = "Intel(R) Ethernet Connection (27) I219-LM"
E57B8NC.DeviceDesc              = "Intel(R) Ethernet Connection (27) I219-V"

;---------------------------------------------------------------------------------------------------
;---------------------------------------------------------------------------------------------------
;---------------------------------------------------------------------------------------------------
;---------------------------------------------------------------------------------------------------
;---------------------------------------------------------------------------------------------------

