; Copyright (c) 2009-2012  Intel Corporation  
; **********************************************************************************************  
; **********************************************************************************************  
; **    Filename:  iaAHCI.inf  
; **    Revision:  11/02/2012,3.6.0.1090 
; **    Abstract:  Windows* INF File for AHCI Intel(R) Rapid Storage Technology Enterprise Driver  
; **               Installs: RSTe AHCI Controller Miniport 
; **********************************************************************************************  
[Version]  
Signature="$Windows NT$"  
Provider=%INTEL%  
ClassGUID={4D36E97B-E325-11CE-BFC1-08002BE10318}  
Class=SCSIAdapter  
CatalogFile=iaAHCI.cat 
DriverVer=11/02/2012,3.6.0.1090
; 
[PackageInfo]  
Name=AHCI  
; 
[SourceDisksNames]  
1 = %DiskId1%,,,""  
[DestinationDirs]  
DefaultDestDir = 12  
; 
[ControlFlags]  
ExcludeFromSelect = *  
; 
[Manufacturer]  
%INTEL% = INTEL, NTx86.5.2, NTamd64    
; 
[iaStorA_Service_Inst]  
ServiceType    = %SERVICE_KERNEL_DRIVER%  
StartType      = %SERVICE_BOOT_START%  
ErrorControl   = %SERVICE_ERROR_NORMAL%  
ServiceBinary  = %12%\iaStorA.sys  
LoadOrderGroup = SCSI miniport  
AddReg         = pnpsafe_pci_addreg  
; 
[iaStorA_EventLog_Inst]  
AddReg = iaStorA_EventLog_AddReg  
; 
[iaStorA_EventLog_AddReg]  
HKR,,EventMessageFile,%REG_EXPAND_SZ%,"%%SystemRoot%%\System32\IoLogMsg.dll;%%SystemRoot%%\System32\drivers\iaStorA.sys" 
HKR,,TypesSupported,%REG_TYPE_DWORD%,7  
; 
;******************************************************************************  
;*  
;* 32-BIT X86 ARCHITECTURE  
;*  
;* This section specifies the 32-bit architecture specific INF file entries  
;* required to install a driver as a 32-bit compatible driver.  
;*  
;******************************************************************************  
[SourceDisksFiles.x86]  
iaStorA.sys = 1,,,  
; 
[INTEL.NTx86.5.2]  
;server devids 
%PCI\VEN_8086&DEV_1D02&CC_0106.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_1D02&CC_0106 
%PCI\VEN_8086&DEV_8C02&CC_0106.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_8C02&CC_0106 
; 
[iaStorA_inst.ntx86]  
CopyFiles=@iaStorA.sys 
; 
[iaStorA_inst.ntx86.HW] 
AddReg = msi_addreg 
AddReg = storport_addreg 
; 
[iaStorA_inst.ntx86.Services]  
AddService = iaStorA, %SPSVCINST_ASSOCSERVICE%, iaStorA_Service_Inst, iaStorA_EventLog_Inst  
; 
;********************************************************  
;*  
;* 64-BIT X86 ARCHITECTURE  
;*  
;* This section specifies the 64-bit architecture specific INF file entries  
;* required to install a driver as a 64-bit compatible driver.  
;*  
;******************************************************************************  
[SourceDisksFiles.amd64]   
iaStorA.sys = 1,,,   
; 
[INTEL.NTamd64] 
;server devids 
%PCI\VEN_8086&DEV_1D02&CC_0106.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_1D02&CC_0106 
%PCI\VEN_8086&DEV_8C02&CC_0106.DeviceDesc% = iaStorA_inst, PCI\VEN_8086&DEV_8C02&CC_0106 
; 
[iaStorA_inst.NTamd64]  
CopyFiles=@iaStorA.sys 
; 
[iaStorA_inst.NTamd64.HW] 
AddReg = msi_addreg 
AddReg = storport_addreg 
; 
[iaStorA_inst.ntamd64.Services]  
AddService = iaStorA, %SPSVCINST_ASSOCSERVICE%, iaStorA_Service_Inst, iaStorA_EventLog_Inst  
; 
[pnpsafe_pci_addreg] 
; Use raw values for BusType, not a DEFINE, ChkInf fails on hex alpha chars  
; BusType_ATA == 0x3, BusTypeATA, BusType_RAID == 0x8, BusType_SATA == 0xb 
HKR, Parameters\PnpInterface,  5,                           %REG_TYPE_DWORD%,  0x00000001  
HKR, Parameters,               BusType,                     %REG_TYPE_DWORD%,  0x0000000b 
; Tell Storport in Win7/Srv08R2(KB982018) that driver can report 4K sector size (not needed in Win8) 
HKR, Parameters\Device,        EnableQueryAccessAlignment,  %REG_TYPE_DWORD%,  0x00000001 
; 
[Strings]  
;  
; Localizable Strings  
;  
diskId1 = "RSTe AHCI Installation Disk"  
;server 
PCI\VEN_8086&DEV_1D02&CC_0106.DeviceDesc    = "Intel(R) C600 series chipset SATA AHCI Controller" 
PCI\VEN_8086&DEV_8C02&CC_0106.DeviceDesc    = "Intel(R) C220 series chipset SATA AHCI Controller" 
; 
INTEL = "Intel Corporation" 
; Non-Localizable Strings  
;  
SPSVCINST_ASSOCSERVICE = 0x00000002  
REG_MULTI_SZ           = 0x00010000  
REG_EXPAND_SZ          = 0x00020000  
REG_TYPE_DWORD         = 0x00010001  
SERVICE_KERNEL_DRIVER  = 1  
SERVICE_BOOT_START     = 0  
SERVICE_ERROR_NORMAL   = 1 
; 
; MSI enables.  
[msi_addreg]   
HKR, Interrupt Management, 0x00000010   
HKR, Interrupt Management\MessageSignaledInterruptProperties, 0x00000010   
HKR, Interrupt Management\MessageSignaledInterruptProperties, MSISupported,       %REG_TYPE_DWORD%,   1   
HKR, Interrupt Management\MessageSignaledInterruptProperties, MessageNumberLimit, %REG_TYPE_DWORD%,   1  
; 
[storport_addreg] 
;;; Enables/Disables Idle Power Management for StorPort 
HKR, "StorPort", "EnableIdlePowerManagement", %REG_TYPE_DWORD%, 0x00000000 
; 
