; Copyright 2024 ASR International (Europe) GmbH
; This is a Setup information file for monitors with ICM file.


[Version]
signature="$CHICAGO$"
Class=Monitor
ClassGuid={4D36E96E-E325-11CE-BFC1-08002BE10318}
Provider=%ASR%
Catalogfile=PG25FFT.cat
DriverVer=06/12/2024,1.0.0.0

[ControlFlags]
ExcludeFromSelect.nt=Monitor\ASRACA7
ExcludeFromSelect.nt=Monitor\ASRACA7
ExcludeFromSelect.nt=Monitor\ASRACA7


[DestinationDirs]
DefaultDestDir=11
ACA7_DP.CopyFiles=23
ACA7_H1.CopyFiles=23
ACA7_H2.CopyFiles=23

[SourceDisksNames]
1=%DiskName%,,,

[SourceDisksFiles]
PG25FFT.ICM=1

[Monitor_Service.Install]
DisplayName    = %Monitor.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\monitor.sys


[Manufacturer]
%ASR%=ASR,ntamd64

[ASR]
%ACA7_DP%=ACA7_DP.Install, Monitor\ASRACA7
%ACA7_H1%=ACA7_H1.Install, Monitor\ASRACA7
%ACA7_H2%=ACA7_H2.Install, Monitor\ASRACA7


[ASR.ntamd64]
%ACA7_DP%=ACA7_DP.Install, Monitor\ASRACA7
%ACA7_H1%=ACA7_H1.Install, Monitor\ASRACA7
%ACA7_H2%=ACA7_H2.Install, Monitor\ASRACA7

[ACA7_DP.Install]
DelReg=DEL_CURRENT_REG
AddReg=ACA7_DP.AddReg
Copyfiles=ACA7_DP.CopyFiles

[ACA7_DP.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install

[ACA7_H1.Install]
DelReg=DEL_CURRENT_REG
AddReg=ACA7_H1.AddReg
Copyfiles=ACA7_H1.CopyFiles

[ACA7_H1.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install

[ACA7_H2.Install]
DelReg=DEL_CURRENT_REG
AddReg=ACA7_H2.AddReg
Copyfiles=ACA7_H2.CopyFiles

[ACA7_H2.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install

[DEL_CURRENT_REG]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile


[ACA7_DP.AddReg]
HKR,"MODES\1920,1080",Mode1,,"215.0-215.0,48.0-180.0,+,+"
HKR,,MaxResolution,,"1920,1080"
HKR,,DPMS,,1
HKR,,ICMProfile,0,"PG25FFT.icm"

[ACA7_H1.AddReg]
HKR,"MODES\1920,1080",Mode1,,"30.0-215.0,48.0-180.0,+,+"
HKR,,MaxResolution,,"1920,1080"
HKR,,DPMS,,1
HKR,,ICMProfile,0,"PG25FFT.icm"

[ACA7_H2.AddReg]
HKR,"MODES\1920,1080",Mode1,,"30.0-215.0,48.0-180.0,+,+"
HKR,,MaxResolution,,"1920,1080"
HKR,,DPMS,,1
HKR,,ICMProfile,0,"PG25FFT.icm"

[ACA7_DP.CopyFiles]
PG25FFT.icm

[ACA7_H1.CopyFiles]
PG25FFT.icm

[ACA7_H2.CopyFiles]
PG25FFT.icm

[Strings]
SPSVCINST_ASSOCSERVICE = 0x07570002
Monitor.SVCDESC = "Microsoft Monitor Class Function Driver Service"

ASR="ASR International (Europe) GmbH"
DiskName="ASR Monitor Installation Disk"

ACA7_DP="ASR PG25FFT"
ACA7_H1="ASR PG25FFT"
ACA7_H2="ASR PG25FFT"
