; Copyright 2022 ASRock Corporation
; This is a Setup information file for monitors with ICM file .
; V001

[Version]
signature="$CHICAGO$"
Class=Monitor
ClassGuid={4D36E96E-E325-11CE-BFC1-08002BE10318}
Provider=%ASR%
Catalogfile=CL25FFB.cat
DriverVer=04/25/2025,1.0.0.0

[ControlFlags]
ExcludeFromSelect.nt=Monitor\ASRBCA4


[DestinationDirs]
DefaultDestDir=11
BCA4_A.CopyFiles=23
BCA4_H.CopyFiles=23


[SourceDisksNames]
1=%DiskName%,,,

[SourceDisksFiles]
CL25FFB.ICM=1

[Monitor_Service.Install]
DisplayName    = %Monitor.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\monitor.sys

[Manufacturer]
%ASR%=ASR,NTAMD64

[ASR]
%BCA4_A%=BCA4_A.Install, Monitor\ASRBCA4
%BCA4_H%=BCA4_H.Install, Monitor\ASRBCA4


[ASR.NTAMD64]
%BCA4_A%=BCA4_A.Install, Monitor\ASRBCA4
%BCA4_H%=BCA4_H.Install, Monitor\ASRBCA4



[BCA4_A.Install]
DelReg=DEL_CURRENT_REG
AddReg=BCA4_A.AddReg
Copyfiles=BCA4_A.CopyFiles

[BCA4_A.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install

[BCA4_H.Install]
DelReg=DEL_CURRENT_REG
AddReg=BCA4_H.AddReg
Copyfiles=BCA4_H.CopyFiles

[BCA4_H.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install


[DEL_CURRENT_REG]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile


[BCA4_A.AddReg]
HKR,"MODES\1920,1080",Mode1,,"30-85,48-75,+,+" 
HKR,,MaxResolution,,"1920,1080"
HKR,,DPMS,,1
HKR,,ICMProfile,0,"CL25FFB.icm"

[BCA4_H.AddReg]
HKR,"MODES\1920,1080",Mode1,,"30-160,48-144,+,+" 
HKR,,MaxResolution,,"1920,1080"
HKR,,DPMS,,1
HKR,,ICMProfile,0,"CL25FFB.icm"



[BCA4_A.CopyFiles]
CL25FFB.icm
[BCA4_H.CopyFiles]
CL25FFB.icm


[Strings]
SPSVCINST_ASSOCSERVICE = 0x00000002
Monitor.SVCDESC = "Microsoft Monitor Class Function Driver Service"

DiskName="ASRock CL25FFB Wizard"
ASR="ASRock"

BCA4_A="ASRock CL25FFB"
BCA4_H="ASRock CL25FFB"
