;=======================================================
; P34-9.INF Ver. 1.0 11/06/2019
;
; Monitor INF file for Fujitsu Display P34-9_UE QHD
;
; Copyright 2019 Fujitsu Technology Solutions GmbH
;=======================================================

[Version]
Signature   = "$Windows NT$"
Class       = Monitor
ClassGuid   = {4D36E96E-E325-11CE-BFC1-08002BE10318}
Provider    = %FTS-Mfg%
CatalogFile = P34-9_UE.cat
DriverVer   = 01/14/2020, 1.0.0.0

[SourceDisksNames]
1 = %DiskName%

[SourceDisksFiles]
P34-9_UE.icm = 1

[DestinationDirs]
DefaultDestDir   = 12
P34-9_UE.Copyfiles = 23

[ControlFlags]
ExcludeFromSelect = Monitor\FUS08E4
ExcludeFromSelect = Monitor\FUS08E5
ExcludeFromSelect = Monitor\FUS08E6
ExcludeFromSelect = Monitor\FUS08E7

[Manufacturer]
%FTS-Mfg% = FTS-Mfg, NTx86, NTAMD64

[FTS-Mfg]
%P34-9_UE.HDMI1%  = P34-9_UE.HDMI1.Install, Monitor\FUS08E4
%P34-9_UE.HDMI2%  = P34-9_UE.HDMI2.Install, Monitor\FUS08E5
%P34-9_UE.DP%     = P34-9_UE.DP.Install, Monitor\FUS08E6
%P34-9_UE.USB-C%  = P34-9_UE.USB-C.Install, Monitor\FUS08E7

[FTS-Mfg.NTx86]
%P34-9_UE.HDMI1%  = P34-9_UE.HDMI1.Install, Monitor\FUS08E4
%P34-9_UE.HDMI2%  = P34-9_UE.HDMI2.Install, Monitor\FUS08E5
%P34-9_UE.DP%     = P34-9_UE.DP.Install, Monitor\FUS08E6
%P34-9_UE.USB-C%  = P34-9_UE.USB-C.Install, Monitor\FUS08E7

[FTS-Mfg.NTAMD64]
%P34-9_UE.HDMI1%  = P34-9_UE.HDMI1.Install, Monitor\FUS08E4
%P34-9_UE.HDMI2%  = P34-9_UE.HDMI2.Install, Monitor\FUS08E5
%P34-9_UE.DP%     = P34-9_UE.DP.Install, Monitor\FUS08E6
%P34-9_UE.USB-C%  = P34-9_UE.USB-C.Install, Monitor\FUS08E7

[P34-9_UE.HDMI1.Install]
DelReg    = DEL_CURRENT_REG
AddReg    = P34-9_UE.HDMI1.AddReg, 3440x1440, DPMS
CopyFiles = P34-9_UE.CopyFiles

[P34-9_UE.HDMI2.Install]
DelReg    = DEL_CURRENT_REG
AddReg    = P34-9_UE.HDMI2.AddReg, 3440x1440, DPMS
CopyFiles = P34-9_UE.CopyFiles

[P34-9_UE.DP.Install]
DelReg    = DEL_CURRENT_REG
AddReg    = P34-9_UE.DP.AddReg, 3440x1440, DPMS
CopyFiles = P34-9_UE.CopyFiles

[P34-9_UE.USB-C.Install]
DelReg    = DEL_CURRENT_REG
AddReg    = P34-9_UE.USB-C.AddReg, 3440x1440, DPMS
CopyFiles = P34-9_UE.CopyFiles

[DEL_CURRENT_REG]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile

[P34-9_UE.HDMI1.AddReg]
HKR,"MODES\3440,1440",Mode1,,"30-160,28-102,+,-"
HKR,,ICMProfile,0,"P34-9_UE.icm"

[P34-9_UE.HDMI2.AddReg]
HKR,"MODES\3440,1440",Mode1,,"30-160,28-102,+,-"
HKR,,ICMProfile,0,"P34-9_UE.icm"

[P34-9_UE.DP.AddReg]
HKR,"MODES\3440,1440",Mode1,,"30-160,28-102,+,-"
HKR,,ICMProfile,0,"P34-9_UE.icm"

[P34-9_UE.USB-C.AddReg]
HKR,"MODES\3440,1440",Mode1,,"30-160,28-102,+,-"
HKR,,ICMProfile,0,"P34-9_UE.icm"

[3440x1440]
HKR,,MaxResolution,,"3440,1440"

[DPMS]
HKR,,DPMS,,1

[P34-9_UE.CopyFiles]
P34-9_UE.icm

[P34-9_UE.HDMI1.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install

[P34-9_UE.HDMI2.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install

[P34-9_UE.DP.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install

[P34-9_UE.USB-C.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install

[Monitor_Service.Install]
DisplayName    = %Monitor.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\monitor.sys

[Strings]
SPSVCINST_ASSOCSERVICE = 0x00000002
Monitor.SVCDESC = "Monitor Class Function Driver Service"
FTS-Mfg         = "Fujitsu Technology Solutions"
DiskName        = "Fujitsu Monitor Installation Disk"

P34-9_UE.HDMI1 = "Fujitsu P34-9_UE (HDMI1)"
P34-9_UE.HDMI2 = "Fujitsu P34-9_UE (HDMI2)"
P34-9_UE.DP    = "Fujitsu P34-9_UE (DP)"
P34-9_UE.USB-C = "Fujitsu P34-9_UE (USB-C)"
