;---- 
;---- Hints for translators:
;---- This file uses UNICODE format. To modify it, use Windows Notepad.
;---- In the 'File - Save as' dialog, make sure Encoding is set to Unicode.
;---- The syntax used herein is:
;----   KEY = String Value
;---- To translate the text, modify String Value. Leading and trailing spaces will be ignored.
;---- DO NOT modify KEY!
;---- DO NOT modify or remove special tokens in the form ${Identifier}. These are placeholders for numbers or other data.
;---- 

;---- 
;---- global strings
;---- 
APP_TITLE                                                          = FAS4 USB Audio Control Panel
NOTIFICATION_AREA_MENU_ENTRY_SHOW                                  = Show
NOTIFICATION_AREA_MENU_ENTRY_EXIT                                  = Exit

;---- 
;---- strings for the status page
;---- 
PAGE_STATUS_TITLE                                                  = Status
PAGE_STATUS_SECTION_DEVICE_TITLE                                   = USB Audio Device
PAGE_STATUS_SECTION_DEVICE_SELECTION_ENTRY_NO_DEVICE               = No devices connected.
PAGE_STATUS_SECTION_DEVICE_SELECTION_ENTRY_PLEASE_SELECT           = Please select a device.
PAGE_STATUS_SECTION_SAMPLE_RATE_TITLE                              = Current Sample Rate
PAGE_STATUS_SECTION_NO_VALID_SAMPLE_RATE                           = No valid sample rate
;---- Hint for translators: The token ${SampleRate} is a placeholder and must not be modified or removed.
PAGE_STATUS_SECTION_SAMPLE_RATE_UNIT                               = ${SampleRate} Hz

;---- 
;---- strings for the status page
;---- 
PAGE_OPTIONS_TITLE                                                 = Options
PAGE_OPTIONS_SECTION_STREAMING_MODE_TITLE                          = Streaming
PAGE_OPTIONS_SECTION_STREAMING_MODE_SELECTION_ENTRY_ON_WHEN_NEEDED = On when Needed
PAGE_OPTIONS_SECTION_STREAMING_MODE_SELECTION_ENTRY_ALWAYS_ON      = Always On

;---- 
;---- strings for the stream format page
;---- 
PAGE_STREAM_FORMATS_TITLE                                          = Format
;---- Hint for translators: The token ${NumberOfChannels} is a placeholder and must not be modified or removed.
PAGE_STREAM_FORMATS_DESCRIPTION_CHANNELS                           = ${NumberOfChannels} channel(s)
;---- Hint for translators: The token ${BitsPerSample} is a placeholder and must not be modified or removed.
PAGE_STREAM_FORMATS_DESCRIPTION_BITS                               = ${BitsPerSample} bits
PAGE_STREAM_FORMATS_SECTION_INPUT_TITLE                            = Input
PAGE_STREAM_FORMATS_SECTION_OUTPUT_TITLE                           = Output

;---- 
;---- strings for the sound device profiles page
;---- 
PAGE_SOUND_DEVICE_PROFILES_TITLE                                   = Profiles
PAGE_SOUND_DEVICE_PROFILES_SECTION_INPUT_TITLE                     = Input
PAGE_SOUND_DEVICE_PROFILES_SECTION_OUTPUT_TITLE                    = Output

;---- 
;---- strings for the sample rate page
;---- 
PAGE_SAMPLE_RATE_TITLE                                             = Sample Rate
;---- Hint for translators: The token ${SampleRate} is a placeholder and must not be modified or removed.
PAGE_SAMPLE_RATE_DESCRIPTION                                       = ${SampleRate} Hz
PAGE_SAMPLE_RATE_SECTION_TITLE                                     = Sample Rate

;---- 
;---- strings for the clock source page
;---- 
PAGE_CLOCK_SOURCE_TITLE                                            = Clock Source
PAGE_CLOCK_SOURCE_TABLE_TITLE                                      = Select Clock Source:
;---- Hint for translators: The token ${ClockSourceUnitId} is a placeholder and must not be modified or removed.
PAGE_CLOCK_SOURCE_TABLE_COLUMN_NAME_COMMON_NAME                    = Clock Source (ID ${ClockSourceUnitId})
PAGE_CLOCK_SOURCE_TABLE_COLUMN_IS_VALID_TEXT_IF_TRUE               = stable
PAGE_CLOCK_SOURCE_TABLE_COLUMN_IS_VALID_TEXT_IF_FALSE              = not valid
;---- Hint for translators: The token ${SampleRate} is a placeholder and must not be modified or removed.
PAGE_CLOCK_SOURCE_TABLE_COLUMN_SAMPLE_RATE_UNIT                    = ${SampleRate} Hz

;---- 
;---- strings for the ASIO device selection page
;---- 
PAGE_ASIO_DEVICE_TITLE                                             = ASIO Device
PAGE_ASIO_DEVICE_TABLE_TITLE                                       = Select ASIO Device:
PAGE_ASIO_DEVICE_CURRENT                                           = current
PAGE_ASIO_DEVICE_NOT_CURRENT                                       = 
PAGE_ASIO_DEVICE_IN_USE                                            = in use
PAGE_ASIO_DEVICE_UNUSED                                            = 
PAGE_ASIO_DEVICE_SECTION_INFO_TITLE                                = Device Info
PAGE_ASIO_DEVICE_SECTION_INFO_TEXT1                                = ${Product}
PAGE_ASIO_DEVICE_SECTION_INFO_TEXT2                                = Serial No: ${SerialNo}
PAGE_ASIO_DEVICE_SECTION_INFO_TEXT3                                = 
PAGE_ASIO_DEVICE_SECTION_INFO_TEXT4                                = 
PAGE_ASIO_DEVICE_SECTION_INFO_TEXT_NO_SERIAL_NO                    = 

;---- 
;---- strings for the buffer settings page
;---- 
PAGE_BUFFER_SETTINGS_TITLE                                         = Buffer Settings
PAGE_BUFFER_SETTINGS_SECTION_ASIO_BUFFER_TITLE                     = Preferred ASIO Buffer Size
PAGE_BUFFER_SETTINGS_SECTION_ASIO_BUFFER_SELECTION_UNIT            = samples
PAGE_BUFFER_SETTINGS_SECTION_SAFE_MODE                             = Safe Mode
PAGE_BUFFER_SETTINGS_SECTION_ASIO_STATUS_TITLE                     = ASIO Status
;---- Hint for translators: The token ${SampleRate} is a placeholder and must not be modified or removed.
PAGE_BUFFER_SETTINGS_SECTION_ASIO_STATUS_CURRENT_SAMPLE_RATE       = Current Sample Rate: ${SampleRate} Hz
PAGE_BUFFER_SETTINGS_SECTION_ASIO_INPUT_LATENCY                    = Input Latency: ${InLatencySamples} samples (${InLatencyMillisecs}.${InLatencyMillisecsFrac} ms)
PAGE_BUFFER_SETTINGS_SECTION_ASIO_OUTPUT_LATENCY                   = Output Latency: ${OutLatencySamples} samples (${OutLatencyMillisecs}.${OutLatencyMillisecsFrac} ms)
PAGE_BUFFER_SETTINGS_SECTION_ASIO_STATUS_STATE_ACTIVE_PCM          = ASIO in use (PCM mode)
PAGE_BUFFER_SETTINGS_SECTION_ASIO_STATUS_STATE_ACTIVE_DSD          = ASIO in use (DSD mode)
PAGE_BUFFER_SETTINGS_SECTION_ASIO_STATUS_STATE_NOT_ACTIVE          = ASIO not used
PAGE_BUFFER_SETTINGS__SECTION_NO_VALID_SAMPLE_RATE                 = No valid sample rate

;---- 
;---- strings for the volume page
;---- 
PAGE_VOLUME_TITLE                                                  = Volume
PAGE_VOLUME_SECTION_CHANNELS_TITLE                                 = Channels
PAGE_VOLUME_SECTION_CHANNELS_BUTTON_INPUT                          = Input ...
PAGE_VOLUME_SECTION_CHANNELS_BUTTON_OUTPUT                         = Output ...
PAGE_VOLUME_DIALOG_INPUT_VOLUME_TITLE                              = Input Volume
PAGE_VOLUME_DIALOG_OUTPUT_VOLUME_TITLE                             = Output Volume
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_MASTER                       = Master
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_MASTER                      = Master
;---- Any non-empty string defined below overwrites the string descriptor reported by the device
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_1                           = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_2                           = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_3                           = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_4                           = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_5                           = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_6                           = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_7                           = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_8                           = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_9                           = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_10                          = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_11                          = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_12                          = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_13                          = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_14                          = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_15                          = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_16                          = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_17                          = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_18                          = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_19                          = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_20                          = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_21                          = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_22                          = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_23                          = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_24                          = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_25                          = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_26                          = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_27                          = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_28                          = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_29                          = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_30                          = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_31                          = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_32                          = 
;---- Any non-empty string defined below overwrites the string descriptor reported by the device
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_1                            = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_2                            = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_3                            = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_4                            = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_5                            = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_6                            = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_7                            = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_8                            = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_9                            = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_10                           = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_11                           = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_12                           = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_13                           = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_14                           = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_15                           = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_16                           = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_17                           = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_18                           = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_19                           = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_20                           = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_21                           = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_22                           = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_23                           = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_24                           = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_25                           = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_26                           = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_27                           = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_28                           = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_29                           = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_30                           = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_31                           = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_32                           = 
;---- Any non-empty string defined below overwrites the string descriptor reported by the device
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_STEREO_1                    = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_STEREO_2                    = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_STEREO_3                    = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_STEREO_4                    = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_STEREO_5                    = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_STEREO_6                    = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_STEREO_7                    = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_STEREO_8                    = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_STEREO_9                    = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_STEREO_10                   = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_STEREO_11                   = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_STEREO_12                   = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_STEREO_13                   = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_STEREO_14                   = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_STEREO_15                   = 
PAGE_VOLUME_DIALOG_OUTPUT_CHANNEL_NAME_STEREO_16                   = 
;---- Any non-empty string defined below overwrites the string descriptor reported by the device
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_STEREO_1                     = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_STEREO_2                     = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_STEREO_3                     = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_STEREO_4                     = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_STEREO_5                     = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_STEREO_6                     = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_STEREO_7                     = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_STEREO_8                     = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_STEREO_9                     = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_STEREO_10                    = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_STEREO_11                    = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_STEREO_12                    = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_STEREO_13                    = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_STEREO_14                    = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_STEREO_15                    = 
PAGE_VOLUME_DIALOG_INPUT_CHANNEL_NAME_STEREO_16                    = 

;---- 
;---- strings for the client info page
;---- 
PAGE_CLIENT_INFO_TITLE                                             = Client Info
PAGE_CLIENT_INFO_TABLE_TITLE                                       = Current State
PAGE_CLIENT_INFO_TABLE_ROW_STREAMING_STATE_TITLE                   = Streaming State:
PAGE_CLIENT_INFO_TABLE_ROW_STREAMING_STATE_STATE_ACTIVE            = Active
PAGE_CLIENT_INFO_TABLE_ROW_STREAMING_STATE_STATE_STOPPED           = Stopped
PAGE_CLIENT_INFO_TABLE_ROW_ACTIVE_WDM_CLIENT_COUNT_TITLE           = Number of Active WDM Clients:
PAGE_CLIENT_INFO_TABLE_ROW_ACTIVE_ASIO_CLIENT_COUNT_TITLE          = Number of Active ASIO Clients:

;---- 
;---- strings for the info page
;---- 
PAGE_INFO_TITLE                                                    = Info
PAGE_INFO_TABLE_DEVICE_INFO_TITLE                                  = Device Info
PAGE_INFO_TABLE_DEVICE_INFO_ROW_MANUFACTURER_TITLE                 = Manufacturer:
PAGE_INFO_TABLE_DEVICE_INFO_ROW_PRODUCT_TITLE                      = Product:
PAGE_INFO_TABLE_DEVICE_INFO_ROW_VID_PID_TITLE                      = VID/PID:
PAGE_INFO_TABLE_DEVICE_INFO_ROW_REVISION_TITLE                     = Revision:
PAGE_INFO_TABLE_DEVICE_INFO_ROW_SERIAL_NO_TITLE                    = Serial No:

;---- 
;---- strings for the about page
;---- 
PAGE_ABOUT_TITLE                                                   = About
PAGE_ABOUT_TABLE_DRIVER_INFO_TITLE                                 = Driver Info
PAGE_ABOUT_TABLE_DRIVER_INFO_ROW_VERSION_VERSION_PREFIX            = Version
PAGE_ABOUT_TABLE_DRIVER_INFO_ROW_BUILDTYPE_TEXT_IF_DEBUG           = Debug Build
PAGE_ABOUT_TABLE_DRIVER_INFO_ROW_BUILDTYPE_TEXT_IF_RELEASE         = Release Build
;---- The copyright text is optional and set to empty by default. Example: Copyright (c) 2017 MyCompany
PAGE_ABOUT_TABLE_DRIVER_INFO_ROW_COPYRIGHT                         = 

;---- 
;---- strings for the error messages
;---- 
ERROR_MESSAGE_COMMON_ERROR                                         = An error has occurred. The internal error description is:
ERROR_MESSAGE_DRIVER_API_DLL_NOT_FOUND                             = The driver DLL required to access the device is missing.
ERROR_MESSAGE_DRIVER_API_DLL_NOT_COMPATIBLE                        = The driver DLL required to access the device is not compatible with this application version.
ERROR_MESSAGE_DRIVER_API_DLL_WITHOUT_INI                           = The configuration file for the driver DLL required to access the device is missing.
ERROR_MESSAGE_DRIVER_API_DLL_WITH_INVALID_INI                      = The configuration file for the driver DLL required to access the device is invalid.
ERROR_MESSAGE_SWITCH_STREAM_FORMAT_NOT_ALLOWED                     = Switching stream format is not allowed while the device is in use.
