;**************************************************************
;
; Copyright 2000 - 2006, Philips Semiconductors GmbH
;
;	  TerraTec Electronic GmbH - BDA Hybrid TV Capture Driver
;
;**************************************************************

[Version]
signature           = "$CHICAGO$" ;All Windows OS
Class               = MEDIA
ClassGUID           = {4d36e96c-e325-11ce-bfc1-08002be10318}
Provider            = %PROVIDER%
PNPLockDown         = 1 ;;; Lock driver against 3rd party application changes
DriverVer	    = 04/04/2007,6.0.1.3
CatalogFile	    = delta.cat

[Manufacturer]
%PROVIDER%  = SupportedBoards, NTx86, NTAMD64

;---> 32 BIT SUPPORT <---
[SupportedBoards.NTx86]
;******** Cinergy 400 TV ***
%CINERGY_400.DeviceDesc% = CINERGY_400.NTx86,PCI\VEN_1131&DEV_7134&SUBSYS_1142153B

;******** Cinergy 600 TV Radio (MK2) ***
%CINERGY_600_MK2.DeviceDesc% = CINERGY_600_MK2.NTx86,PCI\VEN_1131&DEV_7134&SUBSYS_1143153B

;******** Cinergy 200 TV ***
%CINERGY_200.DeviceDesc% = CINERGY_200.NTx86,PCI\VEN_1131&DEV_7130&SUBSYS_1152153B

;******** Cinergy 600 TV Radio (MK3) ***
%CINERGY_600_MK3.DeviceDesc% = CINERGY_600_MK3.NTx86,PCI\VEN_1131&DEV_7134&SUBSYS_1158153B

;******** Cinergy 250 PCI ***
%CINERGY_250.DeviceDesc% = CINERGY_250.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_1160153B


;---> 64 BIT SUPPORT <---
[SupportedBoards.NTAMD64]
;******** Cinergy 400 TV ***
%CINERGY_400.DeviceDesc% = CINERGY_400.NTAMD64,PCI\VEN_1131&DEV_7134&SUBSYS_1142153B

;******** Cinergy 600 TV Radio (MK2) ***
%CINERGY_600_MK2.DeviceDesc% = CINERGY_600_MK2.NTAMD64,PCI\VEN_1131&DEV_7134&SUBSYS_1143153B

;******** Cinergy 200 TV ***
%CINERGY_200.DeviceDesc% = CINERGY_200.NTAMD64,PCI\VEN_1131&DEV_7130&SUBSYS_1152153B

;******** Cinergy 600 TV Radio (MK3) ***
%CINERGY_600_MK3.DeviceDesc% = CINERGY_600_MK3.NTAMD64,PCI\VEN_1131&DEV_7134&SUBSYS_1158153B

;******** Cinergy 250 PCI ***
%CINERGY_250.DeviceDesc% = CINERGY_250.NTAMD64,PCI\VEN_1131&DEV_7133&SUBSYS_1160153B


[SourceDisksNames]
1 = %INSTALLATION_DISK%,,


[SourceDisksFiles]
Ph3xIB32.sys           = 1
Ph3xIB64.sys           = 1
Ph3xIB32MV.dll         = 1
Ph3xIB64MV.dll         = 1


[DestinationDirs]
Ph3xIB32.CopyDll.NTx86      = 11
Ph3xIB64.CopyDll.NTAMD64    = 11
Ph3xIB32.CopyDriver.NTx86   = 10,system32\drivers
Ph3xIB64.CopyDriver.NTAMD64 = 10,system32\drivers


[Ph3xIB32.CopyDll.NTx86]
Ph3xIB32MV.dll


[Ph3xIB64.CopyDll.NTAMD64]
Ph3xIB64MV.dll


[Ph3xIB32.CopyDriver.NTx86]
Ph3xIB32.sys


[Ph3xIB64.CopyDriver.NTAMD64]
Ph3xIB64.sys



;======================================
;
;       Initialization Entries
;
;======================================

;******** Cinergy 400 TV x32 ***
[CINERGY_400.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = Ph3xIB32.CopyDriver.NTx86, Ph3xIB32.CopyDll.NTx86
AddReg        = Ph3xIB32.AddReg.NTx86, CINERGY_400.AddReg
RegisterDlls  = Ph3xIB32.Register.NTx86
AddProperty   = Ph3xIB32.AddProp.NTx86

[CINERGY_400.NTx86.Services]
AddService    = %SERVICE_NAME_X32%, 0x00000002, Ph3xIB32.ServiceInstall.NTx86


;******** Cinergy 400 TV x64 ***
[CINERGY_400.NTAMD64]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = Ph3xIB64.CopyDriver.NTAMD64, Ph3xIB64.CopyDll.NTAMD64
AddReg        = Ph3xIB64.AddReg.NTAMD64, CINERGY_400.AddReg
RegisterDlls  = Ph3xIB64.Register.NTAMD64
AddProperty   = Ph3xIB64.AddProp.NTAMD64

[CINERGY_400.NTAMD64.Services]
AddService    = %SERVICE_NAME_X64%, 0x00000002, Ph3xIB64.ServiceInstall.NTAMD64


;******** Cinergy 600 TV Radio (MK2) x32 ***
[CINERGY_600_MK2.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = Ph3xIB32.CopyDriver.NTx86, Ph3xIB32.CopyDll.NTx86
AddReg        = Ph3xIB32.AddReg.NTx86, CINERGY_600_MK2.AddReg
RegisterDlls  = Ph3xIB32.Register.NTx86
AddProperty   = Ph3xIB32.AddProp.NTx86

[CINERGY_600_MK2.NTx86.Services]
AddService    = %SERVICE_NAME_X32%, 0x00000002, Ph3xIB32.ServiceInstall.NTx86


;******** Cinergy 600 TV Radio (MK2) x64 ***
[CINERGY_600_MK2.NTAMD64]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = Ph3xIB64.CopyDriver.NTAMD64, Ph3xIB64.CopyDll.NTAMD64
AddReg        = Ph3xIB64.AddReg.NTAMD64, CINERGY_600_MK2.AddReg
RegisterDlls  = Ph3xIB64.Register.NTAMD64
AddProperty   = Ph3xIB64.AddProp.NTAMD64

[CINERGY_600_MK2.NTAMD64.Services]
AddService    = %SERVICE_NAME_X64%, 0x00000002, Ph3xIB64.ServiceInstall.NTAMD64


;******** Cinergy 200 TV x32 ***
[CINERGY_200.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = Ph3xIB32.CopyDriver.NTx86, Ph3xIB32.CopyDll.NTx86
AddReg        = Ph3xIB32.AddReg.NTx86, CINERGY_200.AddReg
RegisterDlls  = Ph3xIB32.Register.NTx86
AddProperty   = Ph3xIB32.AddProp.NTx86

[CINERGY_200.NTx86.Services]
AddService    = %SERVICE_NAME_X32%, 0x00000002, Ph3xIB32.ServiceInstall.NTx86


;******** Cinergy 200 TV x64 ***
[CINERGY_200.NTAMD64]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = Ph3xIB64.CopyDriver.NTAMD64, Ph3xIB64.CopyDll.NTAMD64
AddReg        = Ph3xIB64.AddReg.NTAMD64, CINERGY_200.AddReg
RegisterDlls  = Ph3xIB64.Register.NTAMD64
AddProperty   = Ph3xIB64.AddProp.NTAMD64

[CINERGY_200.NTAMD64.Services]
AddService    = %SERVICE_NAME_X64%, 0x00000002, Ph3xIB64.ServiceInstall.NTAMD64


;******** Cinergy 600 TV Radio (MK3) x32 ***
[CINERGY_600_MK3.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = Ph3xIB32.CopyDriver.NTx86, Ph3xIB32.CopyDll.NTx86
AddReg        = Ph3xIB32.AddReg.NTx86, CINERGY_600_MK3.AddReg
RegisterDlls  = Ph3xIB32.Register.NTx86
AddProperty   = Ph3xIB32.AddProp.NTx86

[CINERGY_600_MK3.NTx86.Services]
AddService    = %SERVICE_NAME_X32%, 0x00000002, Ph3xIB32.ServiceInstall.NTx86


;******** Cinergy 600 TV Radio (MK3) x64 ***
[CINERGY_600_MK3.NTAMD64]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = Ph3xIB64.CopyDriver.NTAMD64, Ph3xIB64.CopyDll.NTAMD64
AddReg        = Ph3xIB64.AddReg.NTAMD64, CINERGY_600_MK3.AddReg
RegisterDlls  = Ph3xIB64.Register.NTAMD64
AddProperty   = Ph3xIB64.AddProp.NTAMD64

[CINERGY_600_MK3.NTAMD64.Services]
AddService    = %SERVICE_NAME_X64%, 0x00000002, Ph3xIB64.ServiceInstall.NTAMD64


;******** Cinergy 250 PCI x32 ***
[CINERGY_250.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = Ph3xIB32.CopyDriver.NTx86, Ph3xIB32.CopyDll.NTx86
AddReg        = Ph3xIB32.AddReg.NTx86, CINERGY_250.AddReg
RegisterDlls  = Ph3xIB32.Register.NTx86
AddProperty   = Ph3xIB32.AddProp.NTx86

[CINERGY_250.NTx86.Services]
AddService    = %SERVICE_NAME_X32%, 0x00000002, Ph3xIB32.ServiceInstall.NTx86


;******** Cinergy 250 PCI x64 ***
[CINERGY_250.NTAMD64]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = Ph3xIB64.CopyDriver.NTAMD64, Ph3xIB64.CopyDll.NTAMD64
AddReg        = Ph3xIB64.AddReg.NTAMD64, CINERGY_250.AddReg
RegisterDlls  = Ph3xIB64.Register.NTAMD64
AddProperty   = Ph3xIB64.AddProp.NTAMD64

[CINERGY_250.NTAMD64.Services]
AddService    = %SERVICE_NAME_X64%, 0x00000002, Ph3xIB64.ServiceInstall.NTAMD64


;******** GENERAL x32 ***
[Ph3xIB32.ServiceInstall.NTx86]
DisplayName   = %DISPLAY_NAME%
Description   = %SERVICE_DESCRIPTION%
ServiceType   = %SERVICE_KERNEL_DRIVER%
StartType     = %SERVICE_DEMAND_START%
ErrorControl  = %SERVICE_ERROR_IGNORE%
ServiceBinary = %12%\Ph3xIB32.sys


;******** GENERAL x64 ***
[Ph3xIB64.ServiceInstall.NTAMD64]
DisplayName   = %DISPLAY_NAME%
Description   = %SERVICE_DESCRIPTION%
ServiceType   = %SERVICE_KERNEL_DRIVER%
StartType     = %SERVICE_DEMAND_START%
ErrorControl  = %SERVICE_ERROR_IGNORE%
ServiceBinary = %12%\Ph3xIB64.sys



;======================================
;
;           Property Entries
;
;======================================
[Ph3xIB32.AddProp.NTx86]
GenericDriverInstalled,,,,1

[Ph3xIB64.AddProp.NTAMD64]
GenericDriverInstalled,,,,1


;======================================
;
;           Registry Entries
;
;======================================
; [StartName=driver-object-name]
; [AddReg=add-registry-section[, add-registry-section] ...]
; [DelReg=del-registry-section[, del-registry-section] ...]
; [BitReg=bit-registry-section[,bit-registry-section] ...]
; [LoadOrderGroup=load-order-group-name]
; [Dependencies=depend-on-item-name[,depend-on-item-name]...]

;
;******** General DLL Registry Entries ***
;

[Ph3xIB32.Register.NTx86]
11,,Ph3xIB32MV.dll,1 ;FLG_REGSVR_DLLREGISTER


[Ph3xIB64.Register.NTAMD64]
11,,Ph3xIB64MV.dll,1 ;FLG_REGSVR_DLLREGISTER


;
;******** General Driver Registry Entries ***
;

[Ph3xIB32.AddReg.NTx86]

HKR,,DevLoader,,*NTKERN
HKR,,NTMPDriver,,Ph3xIB32.sys

; --- Registry Entries For Audio Capture ---
HKR,,Driver,,Ph3xIB32.sys
HKR,,AssociatedFilters,,"wdmaud,swmidi,redbook"

HKR,Drivers,SubClasses,,"wave,mixer"
HKR,Drivers\wave\wdmaud.drv,Driver,,wdmaud.drv
HKR,Drivers\mixer\wdmaud.drv,Driver,,wdmaud.drv
HKR,Drivers\wave\wdmaud.drv,Description,,"Philips Audio Capture Device"
HKR,Drivers\mixer\wdmaud.drv,Description,,"Philips Audio Capture Device"

; add audio input and output pinnames
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_AUDIO_IN_PIN%,"Name",,"Analog Audioinput"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_AUDIO_OUT_PIN%,"Name",,"Audio"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_VIDEO_ITU_PIN%,"Name",,"Analog ITU Video"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_AUDIO_I2S_PIN%,"Name",,"I2S Audio"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_AUDIO_CAP_PIN%,"Name",,"~Audio"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_VIDEO_CAP_PIN%,"Name",,"~Capture"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_VIDEO_PRE_PIN%,"Name",,"~Preview"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_MPEG_AES_PIN%,"Name",,"MPEG Audio ES"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_MPEG_VES_PIN%,"Name",,"MPEG Video ES"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_MPEG_PS_PIN%,"Name",, "MPEG2 Program"


[Ph3xIB64.AddReg.NTAMD64]

HKR,,DevLoader,,*NTKERN
HKR,,NTMPDriver,,Ph3xIB64.sys

; --- Registry Entries For Audio Capture ---
HKR,,Driver,,Ph3xIB64.sys
HKR,,AssociatedFilters,,"wdmaud,swmidi,redbook"

HKR,Drivers,SubClasses,,"wave,mixer"
HKR,Drivers\wave\wdmaud.drv,Driver,,wdmaud.drv
HKR,Drivers\mixer\wdmaud.drv,Driver,,wdmaud.drv
HKR,Drivers\wave\wdmaud.drv,Description,,"Philips Audio Capture Device"
HKR,Drivers\mixer\wdmaud.drv,Description,,"Philips Audio Capture Device"

; add audio input and output pinnames
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_AUDIO_IN_PIN%,"Name",,"Analog Audioinput"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_AUDIO_OUT_PIN%,"Name",,"Audio"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_VIDEO_ITU_PIN%,"Name",,"Analog ITU Video"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_AUDIO_I2S_PIN%,"Name",,"I2S Audio"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_AUDIO_CAP_PIN%,"Name",,"~Audio"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_VIDEO_CAP_PIN%,"Name",,"~Capture"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_VIDEO_PRE_PIN%,"Name",,"~Preview"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_MPEG_AES_PIN%,"Name",,"MPEG Audio ES"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_MPEG_VES_PIN%,"Name",,"MPEG Video ES"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_MPEG_PS_PIN%,"Name",, "MPEG2 Program"


;
;******** Board - Specific Registry Entries ***
;

;---- Cinergy 400 TV ----
[CINERGY_400.AddReg]

; Prefix will be displayed in front of the device name on every filter
HKR, "Parameters","Prefix",,%CINERGY_400_CUSTOM_TUNERNAME%

; SmallXBar=0: XBar inputs => Tuner, Composite1, S-Video1, Composite2, S-Video2
; SmallXBar=1: XBar inputs => Tuner, Composite1, S-Video1
HKR, "Parameters", "SmallXBar",0x00010001,1

HKR, "I2C Devices", "Force Registry Settings",0x00010001,0x01
HKR, "VideoDecoder", "Tuner Channel",0x00010001,0x01
HKR, "VideoDecoder", "CVBS Channel",0x00010001,0x04
HKR, "VideoDecoder", "SVHS Channel",0x00010001,0x06
HKR, "VideoDecoder", "FM Radio Channel",0x00010001,0xFF

HKR, "AudioDecoder", "Tuner Channel",0x00010001,0x01
HKR, "AudioDecoder", "CVBS Channel",0x00010001,0x02
HKR, "AudioDecoder", "SVHS Channel",0x00010001,0x02
HKR, "AudioDecoder", "FM Radio Channel",0x00010001,0x03
HKR, "AudioDecoder", "XTAL",0x00010001,0x1

HKR, "I2C Devices", "Number of I2C Devices",0x00010001,0x01
HKR, "I2C Devices", "Device 0, Data1",0x00010001,0x03  ; Tuner ID
HKR, "I2C Devices", "Device 0, Data2",0x00010001,0xC0  ; Tuner slave addr.
;HKR, "I2C Devices", "Device 0, Data3",0x00010001,0xFF  ; Tuner IF PLL slave addr.
;HKR, "I2C Devices", "Device 0, Data4",0x00010001,0xFF  ; Demod
;HKR, "I2C Devices", "Device 0, Data5",0x00010001,0xFF  ; # of Add. Data


;---- Cinergy 600 TV Radio (MK2) ----
[CINERGY_600_MK2.AddReg]

; Prefix will be displayed in front of the device name on every filter
HKR, "Parameters","Prefix",,%CINERGY_600_MK2_CUSTOM_TUNERNAME%

; SmallXBar=0: XBar inputs => Tuner, Composite1, S-Video1, Composite2, S-Video2
; SmallXBar=1: XBar inputs => Tuner, Composite1, S-Video1
HKR, "Parameters", "SmallXBar",0x00010001,1

HKR, "I2C Devices", "Force Registry Settings",0x00010001,0x01
HKR, "VideoDecoder", "Tuner Channel",0x00010001,0x01
HKR, "VideoDecoder", "CVBS Channel",0x00010001,0x04
HKR, "VideoDecoder", "SVHS Channel",0x00010001,0x06
HKR, "VideoDecoder", "FM Radio Channel",0x00010001,0xFF

HKR, "AudioDecoder", "Tuner Channel",0x00010001,0x01
HKR, "AudioDecoder", "CVBS Channel",0x00010001,0x02
HKR, "AudioDecoder", "SVHS Channel",0x00010001,0x02
HKR, "AudioDecoder", "FM Radio Channel",0x00010001,0x03
HKR, "AudioDecoder", "XTAL",0x00010001,0x1

HKR, "I2C Devices", "Number of I2C Devices",0x00010001,0x01
HKR, "I2C Devices", "Device 0, Data1",0x00010001,0x09  ; Tuner ID
HKR, "I2C Devices", "Device 0, Data2",0x00010001,0xC0  ; Tuner slave addr.
;HKR, "I2C Devices", "Device 0, Data3",0x00010001,0xFF  ; Tuner IF PLL slave addr.
;HKR, "I2C Devices", "Device 0, Data4",0x00010001,0xFF  ; Demod
;HKR, "I2C Devices", "Device 0, Data5",0x00010001,0xFF  ; # of Add. Data


;---- Cinergy 200 TV ----
[CINERGY_200.AddReg]

; Prefix will be displayed in front of the device name on every filter
HKR, "Parameters","Prefix",,%CINERGY_200_CUSTOM_TUNERNAME%

; SmallXBar=0: XBar inputs => Tuner, Composite1, S-Video1, Composite2, S-Video2
; SmallXBar=1: XBar inputs => Tuner, Composite1, S-Video1
HKR, "Parameters", "SmallXBar",0x00010001,1

HKR, "I2C Devices", "Force Registry Settings",0x00010001,0x01
HKR, "VideoDecoder", "Tuner Channel",0x00010001,0x01
HKR, "VideoDecoder", "CVBS Channel",0x00010001,0x04
HKR, "VideoDecoder", "SVHS Channel",0x00010001,0x06
HKR, "VideoDecoder", "FM Radio Channel",0x00010001,0xFF

HKR, "AudioDecoder", "Tuner Channel",0x00010001,0x03
HKR, "AudioDecoder", "CVBS Channel",0x00010001,0x02
HKR, "AudioDecoder", "SVHS Channel",0x00010001,0x02
HKR, "AudioDecoder", "FM Radio Channel",0x00010001,0x03
HKR, "AudioDecoder", "XTAL",0x00010001,0x1

HKR, "I2C Devices", "Number of I2C Devices",0x00010001,0x01
HKR, "I2C Devices", "Device 0, Data1",0x00010001,0x03  ; Tuner ID
HKR, "I2C Devices", "Device 0, Data2",0x00010001,0xC0  ; Tuner slave addr.
;HKR, "I2C Devices", "Device 0, Data3",0x00010001,0xFF  ; Tuner IF PLL slave addr.
;HKR, "I2C Devices", "Device 0, Data4",0x00010001,0xFF  ; Demod
;HKR, "I2C Devices", "Device 0, Data5",0x00010001,0xFF  ; # of Add. Data


;---- Cinergy 600 TV Radio (MK3) ----
[CINERGY_600_MK3.AddReg]

; Prefix will be displayed in front of the device name on every filter
HKR, "Parameters","Prefix",,%CINERGY_600_MK3_CUSTOM_TUNERNAME%

; SmallXBar=0: XBar inputs => Tuner, Composite1, S-Video1, Composite2, S-Video2
; SmallXBar=1: XBar inputs => Tuner, Composite1, S-Video1
HKR, "Parameters", "SmallXBar",0x00010001,1

HKR, "I2C Devices", "Force Registry Settings",0x00010001,0x01
HKR, "VideoDecoder", "Tuner Channel",0x00010001,0x01
HKR, "VideoDecoder", "CVBS Channel",0x00010001,0x04
HKR, "VideoDecoder", "SVHS Channel",0x00010001,0x06
HKR, "VideoDecoder", "FM Radio Channel",0x00010001,0xFF

HKR, "AudioDecoder", "Tuner Channel",0x00010001,0x01
HKR, "AudioDecoder", "CVBS Channel",0x00010001,0x02
HKR, "AudioDecoder", "SVHS Channel",0x00010001,0x02
HKR, "AudioDecoder", "FM Radio Channel",0x00010001,0x03
HKR, "AudioDecoder", "XTAL",0x00010001,0x1

HKR, "I2C Devices", "Number of I2C Devices",0x00010001,0x01
HKR, "I2C Devices", "Device 0, Data1",0x00010001,0x05  ; Tuner ID
HKR, "I2C Devices", "Device 0, Data2",0x00010001,0xC0  ; Tuner slave addr.
HKR, "I2C Devices", "Device 0, Data3",0x00010001,0x86  ; Tuner IF PLL slave addr.
;HKR, "I2C Devices", "Device 0, Data4",0x00010001,0xFF  ; Demod slave addr.
;HKR, "I2C Devices", "Device 0, Data5",0x00010001,0xFF  ; # of Add. Data


;---- Cinergy 250 PCI ----
[CINERGY_250.AddReg]

; Prefix will be displayed in front of the device name on every filter
HKR, "Parameters","Prefix",,%CINERGY_250_CUSTOM_TUNERNAME%

; SmallXBar=0: XBar inputs => Tuner, Composite1, S-Video1, Composite2, S-Video2
; SmallXBar=1: XBar inputs => Tuner, Composite1, S-Video1
HKR, "Parameters", "SmallXBar",0x00010001,1

HKR, "I2C Devices", "Force Registry Settings",0x00010001,0x01
HKR, "VideoDecoder", "Tuner Channel",0x00010001,0x01
HKR, "VideoDecoder", "CVBS Channel",0x00010001,0x03
HKR, "VideoDecoder", "SVHS Channel",0x00010001,0x08
HKR, "VideoDecoder", "FM Radio Channel",0x00010001,0x01

HKR, "AudioDecoder", "Tuner Channel",0x00010001,0x01
HKR, "AudioDecoder", "CVBS Channel",0x00010001,0x03
HKR, "AudioDecoder", "SVHS Channel",0x00010001,0x03
HKR, "AudioDecoder", "FM Radio Channel",0x00010001,0x01
HKR, "AudioDecoder", "XTAL",0x00010001,0x0

HKR, "I2C Devices", "Number of I2C Devices",0x00010001,0x01
HKR, "I2C Devices", "Device 0, Data1",0x00010001,0x22  ; Tuner ID
HKR, "I2C Devices", "Device 0, Data2",0x00010001,0xC2  ; Tuner slave addr.
HKR, "I2C Devices", "Device 0, Data3",0x00010001,0x96  ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data4",0x00010001,0x00  ; Demod slave addr.
HKR, "I2C Devices", "Device 0, Data5",0x00010001,0x01  ; # of Add. Data
HKR, "I2C Devices", "Device 0, Data6",0x00010001,0x30  ; Data Byte 1


;======================================
;
;           Strings Defines
;
;======================================

[Strings]
;-------------------------------
; Capture Filter Pin Name GUIDs
;-------------------------------
AVSTREAM_ANLG_AUDIO_IN_PIN   = "{7BB284B9-714D-493d-A101-B1B028E782BD}"
AVSTREAM_ANLG_AUDIO_OUT_PIN  = "{5582E657-E596-42b5-9DB3-541B27A2355F}"
AVSTREAM_ANLG_VIDEO_ITU_PIN  = "{82631A2E-403C-4581-A4B0-EC173D004410}"
AVSTREAM_ANLG_AUDIO_I2S_PIN  = "{C2E46358-F032-4d88-B802-06B59D162730}"
AVSTREAM_ANLG_VIDEO_CAP_PIN  = "{16FFBD0A-F770-4692-A2FF-DD394DFE9564}"
AVSTREAM_ANLG_VIDEO_PRE_PIN  = "{A19F6121-9CF7-4081-8053-256668FCBE1F}"
AVSTREAM_ANLG_AUDIO_CAP_PIN  = "{BA9E27B1-CF44-490e-8EAB-5F662E5FFE74}"
AVSTREAM_MPEG_AES_PIN        = "{9DEC84B9-BCEF-4aac-997E-43EDD0A2D6C7}"
AVSTREAM_MPEG_VES_PIN        = "{181CF87E-7741-47ba-8629-22347E03C64C}"
AVSTREAM_MPEG_PS_PIN         = "{DDA87B83-65DB-4aec-82D0-79FBE67D2BB6}"


;--------------------
; System Defines
;--------------------
SERVICE_BOOT_START       = 0x0 
SERVICE_SYSTEM_START     = 0x1 
SERVICE_AUTO_START       = 0x2 
SERVICE_DEMAND_START     = 0x3 
SERVICE_DISABLED         = 0x4 

SERVICE_KERNEL_DRIVER    = 0x1 
SERVICE_ERROR_IGNORE     = 0x0 
SERVICE_ERROR_NORMAL     = 0x1 
SERVICE_ERROR_SEVERE     = 0x2
SERVICE_ERROR_CRITICAL   = 0x3 
FLG_REGSVR_DLLREGISTER   = 0x00000001


;--------------------
; Customer Strings
;--------------------

DRIVER_NAME_X32               = "Ph3xIB32.sys"
DRIVER_NAME_X64               = "Ph3xIB64.sys"
MACROVISION_NAME_X32          = "Ph3xIB32MV.dll"
MACROVISION_NAME_X64          = "Ph3xIB64MV.dll"

SERVICE_NAME_X32              = "Ph3xIB32"
SERVICE_NAME_X64              = "Ph3xIB64"
SERVICE_DESCRIPTION           = "Philips 713x Inbox BDA Capture Driver"
DISPLAY_NAME                  = "Philips 713x Inbox PCI TV Card"

PROVIDER                      = "TerraTec Electronic GmbH"
INSTALLATION_DISK             = "Vista Installation Disk"


;*** Specific Names ***
;-----------------
CINERGY_400_CUSTOM_TUNERNAME      = "Cinergy 400 TV"
CINERGY_400.DeviceDesc            = "Cinergy 400 TV Capture (MK2)"

CINERGY_600_MK2_CUSTOM_TUNERNAME  = "Cinergy 600 TV"
CINERGY_600_MK2.DeviceDesc        = "Cinergy 600 TV Capture (MK2)"

CINERGY_200_CUSTOM_TUNERNAME      = "Cinergy 200 TV"
CINERGY_200.DeviceDesc            = "Cinergy 200 TV Capture"

CINERGY_600_MK3_CUSTOM_TUNERNAME  = "Cinergy 600 TV"
CINERGY_600_MK3.DeviceDesc        = "Cinergy 600 TV Capture (MK3)"

CINERGY_250_CUSTOM_TUNERNAME      = "Cinergy 250 PCI"
CINERGY_250.DeviceDesc            = "Cinergy 250 PCI Capture"
