; Windows USB CDC ACM Setup File
;
; Copyright (c) 2012 Intel Corporation 
;
; For use only on Windows operating systems.

[Version]
Signature="$Windows NT$"
Class=Ports
ClassGuid={4D36E978-E325-11CE-BFC1-08002BE10318}
Provider=%ProviderName%
DriverVer=04/11/2012,5.1.2600.0
CatalogFile.NTx86  = gserialx86.cat
CatalogFile.NTAMD64 = gserialamd64.cat

[Manufacturer]
%ProviderName%=DeviceList, NTamd64

[DestinationDirs]
DefaultDestDir=12

;------------------------------------------------------------------------------
;  Windows 2000/XP/Vista-32bit Sections
;------------------------------------------------------------------------------
[DriverInstall.NT]
include=mdmcpq.inf
CopyFiles=FakeModemCopyFileSection
AddReg=DriverInstall.NT.AddReg

[DriverInstall.NT.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,usbser.sys
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropP ageProvider"

[DriverInstall.NT.Services]
AddService=usbser, 0x00000002, DriverServiceInst

;------------------------------------------------------------------------------
;  Vista-64bit Sections
;------------------------------------------------------------------------------
[DriverInstall.NTamd64]
include=mdmcpq.inf
CopyFiles=FakeModemCopyFileSection
AddReg=DriverInstall.NTamd64.AddReg

[DriverInstall.NTamd64.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,usbser.sys
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropP ageProvider"

[DriverInstall.NTamd64.Services]
AddService=usbser, 0x00000002, DriverServiceInst

;------------------------------------------------------------------------------
[DriverServiceInst]
DisplayName=%SERVICE%
ServiceType = 1 ; SERVICE_KERNEL_DRIVER
StartType = 3 ; SERVICE_DEMAND_START
ErrorControl = 1 ; SERVICE_ERROR_NORMAL
ServiceBinary= %12%\usbser.sys
LoadOrderGroup = Base

;------------------------------------------------------------------------------
;  Vendor and Product ID Definitions
;------------------------------------------------------------------------------
; When developing your USB device, the VID and PID used in the PC side
; application program and the firmware on the microcontroller must match.
; Modify the below line to use your VID and PID.  Use the format as shown
; below.
; Note: One INF file can be used for multiple devices with different
;       VID and PIDs.  For each supported device, append
;       ",USB\VID_xxxx&PID_yyyy" to the end of the line.
;------------------------------------------------------------------------------
[SourceDisksNames]
1=%DISK%,,,

[SourceDisksFiles]

[DeviceList]
;%DESCRIPTION%=DriverInstall, USB\VID_0525&PID_A4A7, USB\VID_1D6B&PID_0104&MI_02
%MFLDCDC%=DriverInstall,USB\VID_8087&PID_09f2&MI_02
%MFLDCDC%=DriverInstall,USB\VID_8087&PID_09f1&MI_02
%MFLDCDC%=DriverInstall,USB\VID_8087&PID_09f6&MI_02

%MFLDCDC%=DriverInstall,USB\VID_8087&PID_09f8&MI_02

[DeviceList.NTamd64]
;%DESCRIPTION%=DriverInstall, USB\VID_0525&PID_A4A7, USB\VID_1D6B&PID_0104&MI_02
%MFLDCDC%=DriverInstall,USB\VID_8087&PID_09f2&MI_02
%MFLDCDC%=DriverInstall,USB\VID_8087&PID_09f1&MI_02
%MFLDCDC%=DriverInstall,USB\VID_8087&PID_09f6&MI_02

%MFLDCDC%=DriverInstall,USB\VID_8087&PID_09f8&MI_02

;------------------------------------------------------------------------------
;  String Definitions
;------------------------------------------------------------------------------
;Modify these strings to customize your device
;------------------------------------------------------------------------------
[Strings]
ProviderName       	= "Intel Corporation"
DRIVERFILENAME 		= "usbser"
;DESCRIPTION       	= "Gadget Serial"
MFLDCDC 			= "Intel Android Virtual Com Port"
SERVICE             = "USB RS-232 Emulation Driver"
DISK             	= "USB RS-232 Emulation Driver Disk"
