; MS-Windows driver that can install usbccgp.sys
;(generic driver for composite devices)
; For use with composite devices that have more than 1 configuration
; Based on linux.inf

[Version]
Signature = "$WINDOWS NT$"
Class = USB
ClassGUID = {36fc9e60-c465-11cf-8056-444553540000}
Provider = %Linux%
DriverVer = 11/05/2013,2.0.0.0
CatalogFile.NTx86   = telit_composite_x86.cat
CatalogFile.NTAMD64 = telit_composite_x64.cat

[Manufacturer]
%Linux%	 = CCGPLoader,NTx86,NTamd64,NTia64

; Decoration for x86 architecture
[CCGPLoader.NTx86]
%LinuxCompositeDevice% = Composite.Device,USB\VID_1bc7&PID_2300

; Decoration for x64 architecture
[CCGPLoader.NTamd64]
%LinuxCompositeDevice% = Composite.Device,USB\VID_1bc7&PID_2300

; Decoration for ia64 architecture
[CCGPLoader.NTia64]
%LinuxCompositeDevice% = Composite.Device,USB\VID_1bc7&PID_2300

[ControlFlags]
ExcludeFromSelect=*

; Common Class Generic Parent for root ID
[Composite.Device.NTx86]
Include=usb.inf
Needs=Composite.Dev.NT

[Composite.Device.NTx86.Services]
Include=usb.inf
Needs=Composite.Dev.NT.Services

[Composite.Device.NTamd64]
Include=usb.inf
Needs=Composite.Dev.NT

[Composite.Device.NTamd64.Services]
Include=usb.inf
Needs=Composite.Dev.NT.Services

[Composite.Device.NTia64]
Include=usb.inf
Needs=Composite.Dev.NT

[Composite.Device.NTia64.Services]
Include=usb.inf
Needs=Composite.Dev.NT.Services

[SourceDisksNames]
1=%SourceDisk%,,1

[Strings]
ServiceDisplayName = "USB Composite Device Driver"
Linux = "Telit"
LinuxCompositeDevice = "USB Composite Device"
SourceDisk = "Composite Gadget Driver Install Disk"
