;
; omron husbd setup INF file ver 1.1 for X86 ver1.5
;
;   For Inverters
;
; Copyright (c) Hitachi Industrial Equipment Systems Co.,Ltd. 2010-2018
;
;
[Version]
Signature="$CHICAGO$"
Class=HUSBD
ClassGUID={69910468-8802-11d3-ABC7-A756B2FDFB29}
Provider=%OMRON%
DriverVer=07/09/2018,1.1.2.0
CatalogFile.NTx86   = HUSBD86.cat
;CatalogFile.NTAMD64 = HUSBD64.cat

[ClassInstall]
Addreg=USBClassReg

[ClassInstall32]
Addreg=USBClassReg

[USBClassReg]
HKR,,,,%HUSBDClassName%
HKR,,Icon,,-20

[Manufacturer]
;%MfgName%=omron,NTx86,NTamd64
%MfgName%=omron,NTx86

[omron.NTx86]
;新しいデバイスを追加する場合はこの下に追加するデバイスの
;Vendor ID,Product IDを調べ例にならって記述する。複数行記述可。
;これに対応して[Strings]セクションも変更すること
;VID(VendorID), PID(ProductID)
;
;例
;   %USB\VID_0627&PID_0002.DeviceDesc%=HUSBD.Dev, USB\VID_0627&PID_0002
;            ~~~~     ~~~~                                ~~~~     ~~~~
%USB\VID_04A4&PID_008D.DeviceDesc%=HUSBD.Dev, USB\VID_04A4&PID_008D
%USB\VID_04A4&PID_00CF.DeviceDesc%=HUSBD.Dev, USB\VID_04A4&PID_00CF


;[omron.NTamd64]
;;新しいデバイスを追加する場合はこの下に追加するデバイスの
;;Vendor ID,Product IDを調べ例にならって記述する。複数行記述可。
;;これに対応して[Strings]セクションも変更すること
;;
;;例
;;   %USB\VID_0627&PID_0002.DeviceDesc%=HUSBD.Dev, USB\VID_0627&PID_0002
;;            ~~~~     ~~~~                                ~~~~     ~~~~
;%USB\VID_04A4&PID_008D.DeviceDesc%=HUSBD.Dev, USB\VID_04A4&PID_008D
;%USB\VID_04A4&PID_00CF.DeviceDesc%=HUSBD.Dev, USB\VID_04A4&PID_00CF

[DestinationDirs]
DefaultDestDir = 12

[HUSBD.Dev.NT]
CopyFiles=HUSBD.Files.Ext

[HUSBD.Dev.NT.Services]
Addservice = HUSBD, 0x00000002, HUSBD.AddService

[HUSBD.AddService]
DisplayName    = %HUSBD.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\HUSBD.sys
AddReg         = HUSBD.AddReg
LoadOrderGroup = Base

[HUSBD.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,HUSBD.sys

[HUSBD.Files.Ext]
HUSBD.sys

[SourceDisksNames]
1 = ,HUSBD.tag,,\i386
;2 = ,HUSBD.tag,,\amd64

[SourceDisksFiles.x86]
HUSBD.sys = 1

;[SourceDisksFiles.amd64]
;HUSBD.sys = 2

;---------------------------------------------------------------;

[Strings]
OMRON="Omron Corporation"
MfgName="Omron Corporation"
HUSBD.SvcDesc="Universal USB Driver"
HUSBDClassName="HUSBD USB Device"
;DiskId1 = "Omron USB Driver Installation Disk #1"

;
;デバイスを追加したら、ここにそのデバイスの名前を記述すること
;
USB\VID_04A4&PID_008D.DeviceDesc="OMRON Inverter USB Driver"
USB\VID_04A4&PID_00CF.DeviceDesc="OMRON Inverter USB Driver"
