; Generated by DriverWizard v6.20 - http://www.jungo.com.   *
; Installation file (.inf) for "USB Multilink 2.0" device
; Copyright (c) 2012 P&E Microcomputer Systems, Inc.
;
; You can create a customized version of this file
; by modifying the specified sections.
;
; Refer to Windows DDK documentation for more information on INF files
;

; Version Information
; -------------------
[Version]
Signature="$CHICAGO$"  ; Represents all Windows OSs
Provider=%jun%
; You may modify the driver version:
CatalogFile=pemicro12.cat
DriverVer=11/30/2017, 12.7.0

; Select an appropriate class for the device.
; There are several options:
; - Use the Jungo class.
; - Define your own class by generating a private GUID and a class description.
; - Use a system-defined class. This is required for a device that belongs to 
;   a device class that is supported by system-provided drivers, i.e. HID or USB Audio.
;   For example, to replace a default USB mouse driver you have to specify the 
;   description and GUID of HID class:
;       Class=HIDClass
;       ClassGuid={745a17a0-74d3-11d0-b6fe-00a0c90f57da}
;
; We use a Jungo class, you may modify here and use a different class:
Class=Jungo
ClassGuid={c671678c-82c1-43f3-d700-0049433e9a4b}

; Driver Information
; ------------------
[Manufacturer]
; You may modify the manufacturer name by changing the Mfg variable in the [Strings]
; section in this INF file.
%Mfg%=DeviceList

[DeviceList]
; The Vendor ID is 1357, and the Product ID is 0503
; The next line includes the device name that is specified in the Device Manager
; and the hardware ID used as the registry key. 
; You may modify the device name and the hardware ID.
"USB Multilink 2.0"=Install, USB\VID_1357&PID_0503
"Cyclone/TraceLink"=Install, USB\VID_1357&PID_0001
"PEMicro OpenSDA Debug Driver"=Install, USB\VID_1357&PID_0089&Mi_02
"PEMicro USB Multilink (i0)"=Install, USB\VID_1357&PID_0504&Mi_00
"PEMicro USB Serial Port (i1)"=Install, USB\VID_1357&PID_0504&Mi_01
"PEMicro USB Serial Port (i1)"=Install, USB\VID_15A2&PID_0042&Mi_01
"PEMicro USB Serial Port (i1)"=Install, USB\VID_15A2&PID_0058&Mi_01

; Installation Section
; --------------------
[Install]  ; Installation script for Windows 98/Me
CopyFiles=WINDRIVER.Files.Sys, WINDRIVER.Files.Dll
AddReg=UpDateRegistry

[Install.NT]  ; Installation script for Windows 2000/XP/Server 2003
CopyFiles=WINDRIVER.Files.Sys, WINDRIVER.Files.Dll
AddReg=UpDateRegistry

[WINDRIVER.Files.Sys]
; To copy windrvr6.sys upon installation remove the ';' from the start of the following line
windrvr6.sys 

[WINDRIVER.Files.Dll]
peusb32bin32os.dll
peusbmgr2.dll

[ClassInstall]  ; Register a new class in Windows 98/Me
AddReg=UpDateRegistry

[ClassInstall32]  ; Register a new class in Windows 2000/XP/Server 2003
AddReg=UpDateRegistry

[UpDateRegistry]
HKR,,,,Jungo
HKR,,Icon,,-5
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,, windrvr6.sys

[ControlFlags]
ExcludeFromSelect = *  ; Remove all devices listed in this INF file from certain user 
;    interface displays, from which a user is expected to select a particular device 
;    for installation.

[PreCopySection]
HKR,,NoSetupUI,,1

; Defining WinDriver6 Service
; ---------------------------
[Install.NT.Services]
Addservice=WinDriver6, 0x00000002, Service_Info

[Service_Info]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\windrvr6.sys

; Source File Information
; -----------------------
[SourceDisksFiles]
windrvr6.sys=1  ; This indicates that the windrvr6.sys file is located on
    ; disk number 1 of "P&E Microcomputer Systems, Inc. Installation disks" set.
peusb32bin32os.dll=1,\redist,
peusbmgr2.dll=1,\redist,

[SourceDisksNames]
1="P&E Microcomputer Systems, Inc. Installation Disk",,  ; This indicates that disk number 1
    ; has the label "P&E Microcomputer Systems, Inc. Installation Disk". The installer will
    ; search for windrvr6.sys in this disk.

[DestinationDirs]
WINDRIVER.Files.Sys=10, System32\Drivers  ; The location to which the windrvr6.sys
    ; file will be copied (10 translates to the correct Windows directory
    ; on the target machine).
WINDRIVER.Files.Dll=10, System32
;---------------------------------------------------------------;

[Strings]
jun="Jungo LTD."
Mfg="P&E Microcomputer Systems, Inc."

