;
; SYM_HI.INF - version LH.3 - LSI Logic
;
; This is the INF file for Windows (in-box) for the SYM_HI based
; PCI SCSI Cards (895A, 896)
;
; Copyright (c) LSI Logic Incorporated

[version]
signature="$Windows NT$"
Class=SCSIAdapter
ClassGUID={4D36E97B-E325-11CE-BFC1-08002BE10318}
Provider=%LSI%
DriverVer=11/08/2005,4.16.06

;
; Source file information
;

[SourceDisksNames]
3426=windows cd

[SourceDisksFiles]
sym_hi.sys = 3426

[DestinationDirs]
DefaultDestDir = 12 ; DIRID_DRIVERS

[Manufacturer]
%LSI%=LSI,NTx86,NTia64,NTamd64

[LSI]

[LSI.NTx86]
%DevDesc2% = SYM_HI_Inst, PCI\VEN_1000&DEV_000B
%DevDesc3% = SYM_HI_Inst, PCI\VEN_1000&DEV_0012

[LSI.NTia64]
%DevDesc2% = SYM_HI_Inst, PCI\VEN_1000&DEV_000B
%DevDesc3% = SYM_HI_Inst, PCI\VEN_1000&DEV_0012

[LSI.NTamd64]
%DevDesc2% = SYM_HI_Inst, PCI\VEN_1000&DEV_000B
%DevDesc3% = SYM_HI_Inst, PCI\VEN_1000&DEV_0012

[Control Flags]
ExcludeFromSelect = PCI\VEN_1000&DEV_000B
ExcludeFromSelect = PCI\VEN_1000&DEV_0012

[SYM_HI_Inst]
CopyFiles = SYM_HI_CopyFiles
AddReg = SYM_HI_AddReg

[SYM_HI_Inst.HW]
DelReg = LegacyScsiportValues

[SYM_HI_Inst.Services]
AddService = Sym_hi, %SPSVCINST_ASSOCSERVICE%, SYM_HI_Service_Inst, Miniport_EventLog_Inst

[SYM_HI_Service_Inst]
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_BOOT_START%
ErrorControl   = %SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\sym_hi.sys
LoadOrderGroup = SCSI Miniport
AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type_scsi

[SYM_HI_CopyFiles]
sym_hi.sys,,,1

[SYM_HI_AddReg]
HKLM,SYSTEM\CurrentControlSet\Services\Sym_hi\Parameters\Device,MaximumSGList,0x00010001,0x41
HKLM,SYSTEM\CurrentControlSet\Services\Sym_hi\Parameters\Device,NumberOfRequests,0x00010001,0x80

[LegacyScsiportValues]
HKR,Scsiport,BusNumber
HKR,Scsiport,LegacyInterfaceType
HKR,Scsiport,SlotNumber

[pnpsafe_pci_addreg]
HKR, "Parameters\PnpInterface", "5", 0x00010001, 0x00000001

[bus_type_scsi]
HKR, "Parameters", "BusType", 0x00010001, 0x00000001

[Miniport_EventLog_Inst]
AddReg = Miniport_EventLog_AddReg

[Miniport_EventLog_AddReg]
HKR,,EventMessageFile,%REG_EXPAND_SZ%,"%%SystemRoot%%\System32\IoLogMsg.dll"
HKR,,TypesSupported,%REG_DWORD%,7

[Strings]
; localizable
LSI = "LSI Logic"
DevDesc2 = "LSI Logic 22910, 21002 PCI SCSI Adapter; 53C896 Device"
DevDesc3 = "LSI Logic 8953U PCI SCSI Adapter; 53C895A Device"

;*******************************************
;Handy macro substitutions (non-localizable)
SPSVCINST_ASSOCSERVICE = 0x00000002
SERVICE_KERNEL_DRIVER  = 1
SERVICE_BOOT_START     = 0
SERVICE_ERROR_NORMAL   = 1
REG_EXPAND_SZ          = 0x00020000
REG_DWORD              = 0x00010001
