; ar170.inf - Windows XP installation file for the
;             Mylex AcceleRAID 170 Disk Array
;             Controller device.
;
; Version   - 1.1
; Date      - 09/11/2001
;
; Copyright (c) 2001, Mylex Corporation

[Version]
Signature="$Windows NT$"
Class=SCSIAdapter
ClassGUID={4D36E97B-E325-11CE-BFC1-08002BE10318}
Provider=%MYLEX%
CatalogFile=ar170.cat
DriverVer=10/25/2001, 6.03.10.0

[SourceDisksNames]
1 = %Disk1.Desc%,,,\

[SourceDisksFiles]
dac2w2k.sys = 1,,

[DestinationDirs]
DefaultDestDir = 12 ; DIRID_DRIVERS

[ControlFlags]
ExcludeFromSelect=*

[Manufacturer]
%MYLEX% = MYLEX.Mfg

[MYLEX.Mfg]
%MYLEX.DeviceDesc% = MYLEX, PCI\VEN_1069&DEV_0050&SUBSYS_00521069

[MYLEX]
AddReg = MYLEX.AddReg
CopyFiles = MYLEX.Miniport
DriverVer=10/25/2001, 6.03.10.0

[MYLEX.AddReg]

[MYLEX.Miniport]
%MYLEX.DriverName%

[MYLEX.Services]
AddService = %MYLEX.ServiceDesc%, 0x00000002, MYLEX_Service_Inst, MYLEX_EventLog_Inst

[MYLEX_Service_Inst]
ServiceType    = 0x1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0x0                  ; SERVICE_BOOT_START
ErrorControl   = 0x1                  ; SERVICE_ERROR_NORMAL
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\%MYLEX.DriverName%
AddReg         = MYLEX_Miniport_AddReg
AddReg         = pnpsafe_pci_addreg

[MYLEX_EventLog_Inst]
AddReg = MYLEX_EventLog_Inst.AddReg

[MYLEX_EventLog_Inst.AddReg]
HKR,,EventMessageFile,0x00020000,"%SystemRoot%\System32\IoLogMsg.dll"
HKR,,TypesSupported,0x00010001,7

[MYLEX_Miniport_AddReg]
HKR, "Parameters\Device0", "MaximumSGList", 0x00010001, 0x00000080
HKR, "Parameters\Device1", "MaximumSGList", 0x00010001, 0x00000080
HKR, "Parameters\Device2", "MaximumSGList", 0x00010001, 0x00000080
HKR, "Parameters\Device3", "MaximumSGList", 0x00010001, 0x00000080
HKR, "Parameters\Device4", "MaximumSGList", 0x00010001, 0x00000080
HKR, "Parameters\Device5", "MaximumSGList", 0x00010001, 0x00000080
HKR, "Parameters\Device6", "MaximumSGList", 0x00010001, 0x00000080
HKR, "Parameters\Device7", "MaximumSGList", 0x00010001, 0x00000080
HKR, "Parameters\Device0", "NumberOfRequests", 0x00010001, 0x00000100
HKR, "Parameters\Device1", "NumberOfRequests", 0x00010001, 0x00000100
HKR, "Parameters\Device2", "NumberOfRequests", 0x00010001, 0x00000100
HKR, "Parameters\Device3", "NumberOfRequests", 0x00010001, 0x00000100
HKR, "Parameters\Device4", "NumberOfRequests", 0x00010001, 0x00000100
HKR, "Parameters\Device5", "NumberOfRequests", 0x00010001, 0x00000100
HKR, "Parameters\Device6", "NumberOfRequests", 0x00010001, 0x00000100
HKR, "Parameters\Device7", "NumberOfRequests", 0x00010001, 0x00000100

[pnpsafe_pci_addreg]
HKR, "Parameters\PnpInterface", "5", 0x00010001, 0x00000001

[Strings]

;  *******Localizable Strings*******
MYLEX = "Mylex"
Disk1.Desc = "Mylex Software Kit 4.03 (Windows XP)"

MYLEX.DeviceDesc = "Mylex AcceleRAID 170 Disk Array Controller"
MYLEX.DriverName = "dac2w2k.sys"
MYLEX.ServiceDesc = "dac2w2k"
