; Copyright 2019 Lenovo International (Europe) GmbH
; This is a Setup information file for monitors with ICM file .
; V001

[Version]
signature="$CHICAGO$"
Class=Monitor
ClassGuid={4D36E96E-E325-11CE-BFC1-08002BE10318}
Provider=%LEN%
Catalogfile=lenl27q-30.cat
DriverVer=08/31/2019,1.0.0.0

[ControlFlags]
ExcludeFromSelect.nt=Monitor\LEN65FC


[DestinationDirs]
DefaultDestDir=11
65FC_H.CopyFiles=23
65FC_DP.CopyFiles=23

[SourceDisksNames]
1=%DiskName%,,,

[SourceDisksFiles]
lenl27q-30.ICM=1

[Monitor_Service.Install]
DisplayName    = %Monitor.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\monitor.sys

[Manufacturer]
%LEN%=LEN,NTAMD64

[LEN]
%65FC_H%=65FC_H.Install, Monitor\LEN65FC
%65FC_DP%=65FC_DP.Install, Monitor\LEN65FC

[LEN.NTAMD64]
%65FC_H%=65FC_H.Install, Monitor\LEN65FC
%65FC_DP%=65FC_DP.Install, Monitor\LEN65FC


[65FC_H.Install]
DelReg=DEL_CURRENT_REG
AddReg=65FC_H.AddReg
Copyfiles=65FC_H.CopyFiles

[65FC_H.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install

[65FC_DP.Install]
DelReg=DEL_CURRENT_REG
AddReg=65FC_DP.AddReg
Copyfiles=65FC_DP.CopyFiles

[65FC_DP.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install
[DEL_CURRENT_REG]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile


[65FC_H.AddReg]
HKR,"MODES\2560,1440",Mode1,,"30.0-114.0,48.0-75.0,+,+"
HKR,,MaxResolution,,"2560,1440"
HKR,,DPMS,,1
HKR,,ICMProfile,0,"lenl27q-30.icm"
[65FC_DP.AddReg]
HKR,"MODES\2560,1440",Mode1,,"114.0-114.0,48.0-75.0,+,+"
HKR,,MaxResolution,,"2560,1440"
HKR,,DPMS,,1
HKR,,ICMProfile,0,"lenl27q-30.icm"

[65FC_H.CopyFiles]
lenl27q-30.icm
[65FC_DP.CopyFiles]
lenl27q-30.icm

[Strings]
SPSVCINST_ASSOCSERVICE = 0x00000002
Monitor.SVCDESC = "Microsoft Monitor Class Function Driver Service"

DiskName="LEN Monitor Installation Disk"
LEN="LEN International (Europe) GmbH"

65FC_H="LEN L27q-30"
65FC_DP="LEN L27q-30"