;**************************************************************************
;
; sorndis.inf   -- Sony Android RNDIS Interface Driver
;
;**************************************************************************

[Version]
Signature           = "$Windows NT$"
Class               = Net
ClassGUID           = {4D36E972-E325-11CE-BFC1-08002BE10318}
Provider            = %ProviderName%
DriverVer           = 07/02/2015,0.0.0000.00001
CatalogFile.NTx86   = sorndis86.cat

[Manufacturer]
%ProviderName%         = RndisDevices,NTx86

; Decoration for x86 architecture
[RndisDevices.NTx86]
%RndisDevice%    = RNDIS.NT.5.1, USB\VID_0FCE&PID_71AA&MI_00
%RndisDevice%    = RNDIS.NT.5.1, USB\VID_0FCE&PID_81AA&MI_00
%RndisDevice%    = RNDIS.NT.5.1, USB\VID_0FCE&PID_71AB&MI_00
%RndisDevice%    = RNDIS.NT.5.1, USB\VID_0FCE&PID_81AB&MI_00
%RndisDevice%    = RNDIS.NT.5.1, USB\VID_0FCE&PID_71AD&MI_00
%RndisDevice%    = RNDIS.NT.5.1, USB\VID_0FCE&PID_81AD&MI_00
%RndisDevice%    = RNDIS.NT.5.1, USB\VID_0FCE&PID_71B5&MI_00
%RndisDevice%    = RNDIS.NT.5.1, USB\VID_0FCE&PID_81B5&MI_00
%RndisDevice%    = RNDIS.NT.5.1, USB\VID_0FCE&PID_71B8&MI_00
%RndisDevice%    = RNDIS.NT.5.1, USB\VID_0FCE&PID_81B8&MI_00
%RndisDevice%    = RNDIS.NT.5.1, USB\VID_0FCE&PID_71BC&MI_00
%RndisDevice%    = RNDIS.NT.5.1, USB\VID_0FCE&PID_81BC&MI_00
%RndisDevice%    = RNDIS.NT.5.1, USB\VID_0FCE&PID_71C5&MI_00
%RndisDevice%    = RNDIS.NT.5.1, USB\VID_0FCE&PID_81C5&MI_00
%RndisDevice%    = RNDIS.NT.5.1, USB\VID_0FCE&PID_71CB&MI_00
%RndisDevice%    = RNDIS.NT.5.1, USB\VID_0FCE&PID_81CB&MI_00
%RndisDevice%    = RNDIS.NT.5.1, USB\VID_0FCE&PID_71D2&MI_00
%RndisDevice%    = RNDIS.NT.5.1, USB\VID_0FCE&PID_81D2&MI_00
%RndisDevice%    = RNDIS.NT.5.1, USB\VID_0FCE&PID_71C4&MI_00
%RndisDevice%    = RNDIS.NT.5.1, USB\VID_0FCE&PID_81C4&MI_00
%RndisDevice%    = RNDIS.NT.5.1, USB\VID_0FCE&PID_71D6&MI_00
%RndisDevice%    = RNDIS.NT.5.1, USB\VID_0FCE&PID_81D6&MI_00
%RndisDevice%    = RNDIS.NT.5.1, USB\VID_0FCE&PID_71D7&MI_00
%RndisDevice%    = RNDIS.NT.5.1, USB\VID_0FCE&PID_81D7&MI_00



;@@@ This is the common setting for setup
[ControlFlags]
ExcludeFromSelect=*

; DDInstall section
; References the in-build Netrndis.inf
[RNDIS.NT.5.1]
Characteristics = 0x84   ; NCF_PHYSICAL + NCF_HAS_UI
BusType         = 15
; NEVER REMOVE THE FOLLOWING REFERENCE FOR NETRNDIS.INF
include         = netrndis.inf
needs           = Usb_Rndis.ndi

; DDInstal.Services section
[RNDIS.NT.5.1.Services]
include     = netrndis.inf
needs       = Usb_Rndis.ndi.Services

; No sys copyfiles - the sys files are already in-build
; (part of the operating system).

; Modify these strings for your device as needed.
[Strings]
ProviderName                = "Sony"
RndisDevice                 = "Sony Android Remote NDIS based Device"