;                     
; Windows CE USB Host Setup File
; Copyright (c) Microsoft Corporation
;
; WCEUSBSH.INF  -- This is the inf installation script for the stand-alone
;                  release of serial-over-USB host driver for WCE USB Function devices.
;

[Version]
Signature="$CHICAGO$"
Class=WCEUSBS
ClassGuid={25dbce51-6c8f-4a72-8a6d-b54c2b4fc835}
Provider=%FIH%
DriverVer=10/06/2004, 4.0.4232.0
CatalogFile.NT=wceusbsh.cat

[ControlFlags]
ExcludeFromSelect = *

[DestinationDirs]
DefaultDestDir = 12
NTCopyFiles = 12
Win9xWDMFiles = 10,system32\drivers ; %windir%\SYSTEM32\DRIVERS


[SourceDisksNames.x86]
1 = %MediaDescription%


[SourceDisksFiles.x86]
wceusbsh.sys = 1



[NTCopyFiles]
wceusbsh.sys

[Win9xWDMFiles]
;wceusbsh.sys



;
; Class Install section
;
[ClassInstall]
Addreg=Interface_ClassReg

[ClassInstall32]
Addreg=Interface_ClassReg32

[Interface_ClassReg]
HKR,,,,%Interface.ClassName%
;HKR,,NoInstallClass,,1
HKR,,SilentInstall,,1
HKR,,Icon,,-20

[Interface_ClassReg32]
HKR,,,,%Interface.ClassName%
;HKR,,NoInstallClass,,1
HKR,,SilentInstall,,1
HKR,,Icon,,-20


;
;
;  <VENDOR SECTION>
;
;  1 of 3.
;  Add your manufacturer name here (and a string definition under [strings] below)
;
;  e.g.
;  %ACME%=ACME
;

[Manufacturer]
%FIH% = FIH



;
;  <VENDOR SECTION>
;
;  2 of 3.
;  Add your manufacturer section and device entry here.
;  Use the hardware PnP ID of your device.
;
;  e.g.
;  [ACME]
;  %USB\VID_xxxx&PID_yyyy.DeviceDesc% = Host_Inst, USB\VID_xxxx&PID_yyyy
;

[FIH]
%USB\Vid_0489&Pid_00CE.DeviceDesc% = Host_Inst, USB\Vid_0489&Pid_00CE
%USB\Vid_0489&Pid_FFFF.DeviceDesc% = Host_Inst, USB\Vid_0489&Pid_FFFF
%USB\Vid_0489&Pid_7001.DeviceDesc% = Host_Inst, USB\Vid_0489&Pid_7001
%USB\Vid_0489&Pid_7002.DeviceDesc% = Host_Inst, USB\Vid_0489&Pid_7002
%USB\Vid_0489&Pid_7003.DeviceDesc% = Host_Inst, USB\Vid_0489&Pid_7003
%USB\Vid_0489&Pid_7004.DeviceDesc% = Host_Inst, USB\Vid_0489&Pid_7004
%USB\Vid_0489&Pid_7005.DeviceDesc% = Host_Inst, USB\Vid_0489&Pid_7005
%USB\Vid_0489&Pid_7006.DeviceDesc% = Host_Inst, USB\Vid_0489&Pid_7006
%USB\Vid_0489&Pid_7007.DeviceDesc% = Host_Inst, USB\Vid_0489&Pid_7007
%USB\Vid_0489&Pid_7008.DeviceDesc% = Host_Inst, USB\Vid_0489&Pid_7008
%USB\Vid_0489&Pid_7009.DeviceDesc% = Host_Inst, USB\Vid_0489&Pid_7009
%USB\Vid_0489&Pid_700A.DeviceDesc% = Host_Inst, USB\Vid_0489&Pid_700A


;
; Win 9x DDInstall section
;
[Host_Inst]
Copyfiles = Win9xWDMFiles
AddReg = Host_Win9x_AddReg
DriverVer=10/06/2004, 4.0.4232.0

[Host_Win9x_AddReg]
HKR,,DevLoader,0,*NTKERN
HKR,,NTMPDriver,,"wceusbsh.sys"


;
; Windows 2000 and XP DDInstall section
;
[Host_Inst.NT]
CopyFiles=NTCopyFiles
DriverVer=10/06/2004, 4.0.4232.0

[Host_Inst.NT.Services]
AddService = wceusbsh,0x00000002,Host_Service_Inst, Host_EventLog_Inst

[Host_Service_Inst]
DisplayName   = %Host_Inst.SVCDESC%
ServiceType   = 1  ; SERVICE_KERNEL_DRIVER
StartType     = 3  ; SERVICE_DEMAND_START
ErrorControl  = 0  ; SERVICE_ERROR_IGNORE
ServiceBinary = %12%\wceusbsh.sys
LoadOrderGroup = Extended base

[Host_EventLog_Inst]
AddReg = Host_EventLog_AddReg

[Host_EventLog_AddReg]
HKR,,EventMessageFile,0x00020000,"%%SystemRoot%%\System32\IoLogMsg.dll;%%SystemRoot%%\System32\drivers\wceusbsh.sys"
HKR,,TypesSupported,0x00010001,7



[Strings]
;----------------------
REG_DWORD = 0x00010001
MICROSOFT = "Microsoft"

Host_Inst.SVCDESC   = "Windows CE USB Serial Host Driver"
Interface.ClassName = "Windows CE USB Devices"


MediaDescription	= "Windows CE ActiveSync Media"

;
;  <VENDOR SECTION>
;
; 3 of 3.
; Define your strings here
;
;  e.g.
;  ACME = "ACME"
;  USB\VID_xxxx&PID_yyyy.DeviceDesc = "ACME USB Sync"
;

FIH = "FIH"
USB\Vid_0489&Pid_00CE.DeviceDesc = "PP5420 USB Serial Device"
USB\Vid_0489&Pid_FFFF.DeviceDesc = "PP5420 Mass Storage Device"
USB\Vid_0489&Pid_7001.DeviceDesc = "PP5420 USB Sync"
USB\Vid_0489&Pid_7002.DeviceDesc = "PP3400 USB Sync"
USB\Vid_0489&Pid_7003.DeviceDesc = "SP1400 USB Sync"
USB\Vid_0489&Pid_7004.DeviceDesc = "PP5421 USB Sync"
USB\Vid_0489&Pid_7005.DeviceDesc = "FIH USB Sync"
USB\Vid_0489&Pid_7006.DeviceDesc = "FIH USB Sync"
USB\Vid_0489&Pid_7007.DeviceDesc = "FIH USB Sync"
USB\Vid_0489&Pid_7008.DeviceDesc = "FIH USB Sync"
USB\Vid_0489&Pid_7009.DeviceDesc = "FIH USB Sync"
USB\Vid_0489&Pid_700A.DeviceDesc = "FIH USB Sync"

