
; Windows USB CDC ACM Setup File
; Copyright (c) 2000 Microsoft Corporation
; Copyright (C) 2012 Microflex, LLC

[Version] 
Signature="$Windows NT$" 
Class=Ports
ClassGuid={4D36E978-E325-11CE-BFC1-08002BE10318} 
Provider=%MFGNAME% 
LayoutFile=layout.inf
CatalogFile=Mflex485.cat
DriverVer=03/11/2010,5.1.2600.2

[Manufacturer] 
%MFGNAME%=DeviceList, NTamd64

[DestinationDirs] 
DefaultDestDir=12 


;------------------------------------------------------------------------------
;  Windows 2000/XP/Server2003/Vista/Server2008/7 - 32bit Sections
;------------------------------------------------------------------------------

[DriverInstall.nt] 
include=mdmcpq.inf
CopyFiles=DriverCopyFiles.nt
AddReg=DriverInstall.nt.AddReg 

[DriverCopyFiles.nt]
usbser.sys,,,0x20

[DriverInstall.nt.AddReg] 
HKR,,DevLoader,,*ntkern 
HKR,,NTMPDriver,,%DRIVERFILENAME%.sys 
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider" 

[DriverInstall.nt.Services] 
AddService=usbser, 0x00000002, DriverService.nt

[DriverService.nt] 
DisplayName=%SERVICE% 
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\%DRIVERFILENAME%.sys 

;------------------------------------------------------------------------------
;  Windows XP/Server2003/Vista/Server2008/7 - 64bit Sections
;------------------------------------------------------------------------------

[DriverInstall.NTamd64] 
include=mdmcpq.inf
CopyFiles=DriverCopyFiles.NTamd64
AddReg=DriverInstall.NTamd64.AddReg 

[DriverCopyFiles.NTamd64]
%DRIVERFILENAME%.sys,,,0x20

[DriverInstall.NTamd64.AddReg] 
HKR,,DevLoader,,*ntkern 
HKR,,NTMPDriver,,%DRIVERFILENAME%.sys 
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider" 

[DriverInstall.NTamd64.Services] 
AddService=usbser, 0x00000002, DriverService.NTamd64

[DriverService.NTamd64] 
DisplayName=%SERVICE% 
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\%DRIVERFILENAME%.sys 


[SourceDisksFiles]
[SourceDisksNames]
[DeviceList]
%DESCRIPTION%=DriverInstall, USB\VID_04D8&PID_FEAC 

[DeviceList.NTamd64] 
%DESCRIPTION%=DriverInstall, USB\VID_04D8&PID_FEAC 


;------------------------------------------------------------------------------
;  String Definitions
;------------------------------------------------------------------------------
;Modify these strings to customize your device
;------------------------------------------------------------------------------
[Strings]
MFGFILENAME="Mflex485"
DRIVERFILENAME ="usbser"
MFGNAME="Microflex,LLC "
INSTDISK="Microflex, LLC RS-485 Converter Installation Disc"
DESCRIPTION="USB RS485 Serial Converter"
SERVICE="USB RS-232 Emulation Driver"


