;   Prolific PL254X VCP Series

;   acm4pl.INF (for WinXP )

;   Copyright (c) 2018, Prolific Technology Inc.



[version]
signature="$CHICAGO$"
Class=Ports
ClassGuid={4D36E978-E325-11CE-BFC1-08002BE10318}
Provider=%PRO%
DriverVer=06/21/2024,7.0.4.1
CatalogFile=acm4pl.cat


; ================= Device Install section =====================

[ControlFlags]
ExcludeFromSelect=*

[Manufacturer]
%PRO%=PRO,NT,NTAMD64

[SourceDisksFiles]
acm4pl.sys=1
acm4pl64.sys=1
WdfCoInstaller19acm4pl.dll=2
WdfCoInstaller19acm4pl.dll=3

[SourceDisksNames]
1=%DISK_NAME%,
2= %InstallDisk%,,,\x86
3= %InstallDisk%,,,\amd64

[DestinationDirs]
DefaultDestDir  = 12
CoInstaller_CopyFiles86 = 11
CoInstaller_CopyFiles64 = 11


[PRO.NT]
%DeviceDescA% = ComPort, USB\VID_067B&PID_2543&REV_4302&MI_00
%DeviceDescB% = ComPort, USB\VID_067B&PID_2543&REV_4302&MI_02
%DeviceDesc0% = ComPort, USB\VID_067B&PID_2563&MI_00
%DeviceDesc1% = ComPort, USB\VID_067B&PID_2565&MI_00
%DeviceDesc2% = ComPort, USB\VID_067B&PID_2565&MI_02
%DeviceDesc3% = ComPort, USB\VID_067B&PID_2565&MI_04
%DeviceDesc4% = ComPort, USB\VID_067B&PID_2565&MI_06
%DeviceDesc5% = ComPort, USB\VID_067B&PID_2543&REV_4304&MI_00
%DeviceDesc6% = ComPort, USB\VID_067B&PID_2543&REV_4304&MI_02
%DeviceDesc7% = ComPort, USB\VID_067B&PID_2543&REV_4304&MI_04
%DeviceDesc8% = ComPort, USB\VID_067B&PID_2543&REV_4304&MI_06

[PRO.NTAMD64]
%DeviceDescA% = ComPort, USB\VID_067B&PID_2543&REV_4302&MI_00
%DeviceDescB% = ComPort, USB\VID_067B&PID_2543&REV_4302&MI_02
%DeviceDesc2% = ComPort, USB\VID_067B&PID_2565&MI_02
%DeviceDesc3% = ComPort, USB\VID_067B&PID_2565&MI_04
%DeviceDesc4% = ComPort, USB\VID_067B&PID_2565&MI_06
%DeviceDesc5% = ComPort, USB\VID_067B&PID_2543&REV_4304&MI_00
%DeviceDesc6% = ComPort, USB\VID_067B&PID_2543&REV_4304&MI_02
%DeviceDesc7% = ComPort, USB\VID_067B&PID_2543&REV_4304&MI_04
%DeviceDesc8% = ComPort, USB\VID_067B&PID_2543&REV_4304&MI_06

[ComPort.AddReg]
HKR,,PortSubClass,1,01

[ComPort.NT]
CopyFiles=ComPort.NT.Copy
AddReg=ComPort.NT.AddReg

[ComPort.NT.HW]
AddReg=ComPort.HW.AddReg

[ComPort.NT.Services]
AddService = acm4plx86, 0x00000002, Serial_Service_Inst.NT
AddService = Serenum,,Serenum_Service_Inst

[ComPort.NT.Copy]
acm4pl.sys

[ComPort.NT.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,acm4pl.sys
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"

[ComPort.HW.AddReg]
HKR,,"UpperFilters",0x00010000,"serenum"
HKR,,"PL2303C1",0x00010001,10
HKR,,"PL2303C2",0x00010001,0
HKR,,"PL2303C3",0x00010001,4096

[ComPort.NTAMD64]
CopyFiles=ComPort.NTAMD64.Copy
AddReg=ComPort.NTAMD64.AddReg

[ComPort.NTAMD64.HW]
AddReg=ComPort.HW.AddReg

[ComPort.NTAMD64.Services]
AddService = acm4pl, 0x00000002, Serial_Service_Inst.NTAMD64
AddService = Serenum,,Serenum_Service_Inst

[ComPort.NTAMD64.Copy]
acm4pl64.sys

[ComPort.NTAMD64.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,acm4pl64.sys
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"


[Serial_Service_Inst.NT]
DisplayName    = %Serial.SVCDESC%                            
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\acm4pl.sys                            
LoadOrderGroup = Base

[Serial_Service_Inst.NTAMD64]
DisplayName    = %Serial.SVCDESC%                            
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\acm4pl64.sys                            
LoadOrderGroup = Base

[Serenum_Service_Inst]
DisplayName    = %Serenum.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\serenum.sys
LoadOrderGroup = PNP Filter

;-------------- WDF Coinstaller installation
[SourceDisksFiles.x86]
WdfCoInstaller19acm4pl.dll=2

[SourceDisksFiles.amd64]
WdfCoInstaller19acm4pl.dll=3

[ComPort.NT.CoInstallers]
CopyFiles=CoInstaller_CopyFiles86
AddReg=CoInstaller_AddReg

[CoInstaller_CopyFiles86]
WdfCoInstaller19acm4pl.dll

[ComPort.NT.Wdf]
KmdfService = acm4plx86, acm4pl_wdfsect

[ComPort.NTAMD64.CoInstallers]
CopyFiles=CoInstaller_CopyFiles64
AddReg=CoInstaller_AddReg

[CoInstaller_CopyFiles64]
WdfCoInstaller19acm4pl.dll

[CoInstaller_AddReg]
HKR,,CoInstallers32,0x00010000, "WdfCoInstaller19acm4pl.dll,WdfCoInstaller"

[ComPort.NTAMD64.Wdf]
KmdfService = acm4pl, acm4pl_wdfsect


[acm4pl_wdfsect]
KmdfLibraryVersion = 1.9

[Strings]
PRO = "Prolific"
DeviceDescA = "PL2523 USB2.0 HS Serial Port_0"
DeviceDescB = "PL2523 USB2.0 HS Serial Port_1"
DeviceDesc0 = "PL2563 USB2.0 HS Serial Port_0"
DeviceDesc1 = "PL2565 USB2.0 HS Serial Port_0"
DeviceDesc2 = "PL2565 USB2.0 HS Serial Port_1"
DeviceDesc3 = "PL2565 USB2.0 HS Serial Port_2"
DeviceDesc4 = "PL2565 USB2.0 HS Serial Port_3"
DeviceDesc5 = "PL2543 USB2.0 HS Serial Port_0"
DeviceDesc6 = "PL2543 USB2.0 HS Serial Port_1"
DeviceDesc7 = "PL2543 USB2.0 HS Serial Port_2"
DeviceDesc8 = "PL2543 USB2.0 HS Serial Port_3"
Serial.SVCDESC  = "PL256X USB2.0 HS Serial Port WDF driver"
Serenum.SVCDESC = "Serenum Filter Driver"
DISK_NAME = "USB-Serial Cable Diskette"
InstallDisk="Installation disk or directory"