; FR_USB-Serial_port_(IF_with_cdc-eth).inf
; Copyright (c) 2016 Pete Batard <pete@akeo.ie> (GNU LGPL)
; Based on the USB CDC .inf sample file provided by James Stephanick
; at https://community.freescale.com/message/493287#493287
; With acknowledgement to Sensics, Inc. <http://sensics.com/osvr>,
; for providing an original (yet no longer used) inf file.

[Strings]
DeviceName = "FR USB-Serial port (IF with cdc-eth)"
VendorName = "Fiscal Labs"
SourceName = "FR USB-Serial port (IF with cdc-eth) Install Disk"
DeviceID   = "VID_0FB9&PID_2608&MI_02"
DeviceGUID = "{856C0683-4960-4F7E-9F08-7F48827D8EF9}"
Service    = "USB COM Port"

[Version]
Signature   = "$Windows NT$"
Class       = Ports
ClassGuid   = {4D36E978-E325-11CE-BFC1-08002BE10318}
Provider    = "SHTRIH-M JSC"
CatalogFile = FR_USB-Serial_port_(IF_with_cdc-eth).cat
DriverVer   = 11/14/2022, 1.0.0.0

[Manufacturer]
%VendorName% = DeviceList,NTx86,NTamd64,NTarm

[DeviceList.NTx86]
%DeviceName% = UsbSer_Install, USB\%DeviceID%

[DeviceList.NTamd64]
%DeviceName% = UsbSer_Install, USB\%DeviceID%

[DeviceList.NTarm]
%DeviceName% = UsbSer_Install, USB\%DeviceID%

[UsbSer_Install]
; See https://support.microsoft.com/en-us/kb/837637
include     = mdmcpq.inf
CopyFiles   = FakeModemCopyFileSection ; defined in mdmcpq.inf
AddReg      = UsbSer_Install.AddReg
AddProperty = UsbSer_AddProperty

[UsbSer_Install.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,usbser.sys
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"

[UsbSer_Install.Services]
AddService = usbser,0x00000002,UsbSer_Service

[UsbSer_Service]
DisplayName   = %Service%
ServiceType   = 1
StartType     = 3
ErrorControl  = 1
ServiceBinary = %12%\usbser.sys

[UsbSer_AddProperty]
GenericDriverInstalled,,,,1

[DestinationDirs]
DefaultDestDir = 12

[SourceDisksNames]
1 = %SourceName%

[SourceDisksFiles]
